;/*++
;
;Copyright (c) 2006-2009 AuthenTec. Inc,  All rights reserved.
;
;Module Name:
;
;    ATSwpWDF.INF
;
;Abstract:
;    Driver INF file for installing Authentec Swipe
;    sensor drivers on x86 and x64 platforms.
;
;    NOTE: Currently not supporting IA64 platforms.

;--*/

[Version]
Signature="$WINDOWS NT$"
Class=Biometric
ClassGUID={53D29EF7-377C-4D14-864B-EB3A85769359}
provider=%Authentec%
DriverVer=05/19/2010,9.0.8.21
CatalogFile.NTx86   = ATSwpWDF.cat
CatalogFile.NTamd64 = ATSwpWDFAMD64.cat


; ================= Class section =====================

[ClassInstall32.NT]
Addreg=BiometricClassReg

[BiometricClassReg]
HKR,,,,%ClassName%
HKR,,NoInstallClass,,1
HKR,,Icon,,-30


; ================= Device Install section =====================

;
; Manufacturer section
;  This consists of [Manufacturer][Models] with the
;	supported OS platform decorations
;
;
[Manufacturer]
%MfgName%=AuthentecModels,NTx86,NTamd64

;-----------------------------------------------------------------
; Models for XP or later, x86 based machines
;
[AuthentecModels.NTx86]
%AES1610%=ATSwpWDF_Inst, USB\VID_08FF&PID_1600
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1660
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_169F
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_169E
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168F
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168E
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168D
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168C
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168B
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168A
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1689
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1688
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1687
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1686
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1685
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1684
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1683
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1682
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1681
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1680
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2500
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2501
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2502
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2503
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2504
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2505
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2506
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2507
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2508
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2509
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250A
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250B
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250C
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250D
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250E
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250F
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_2580
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_2588
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_2589
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258A
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258B
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258C
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258D
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258E
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258F
%AES2550%=ATSwpWDF_Inst, USB\VID_08FF&PID_2550
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2660
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_269F
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_269E
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268F
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268E
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268D
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268C
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268B
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268A
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2689
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2688
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2687
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2686
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2685
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2684
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2683
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2682
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2681
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2680
%AES2810%=ATSwpWDF_Inst, USB\VID_08FF&PID_2810

;-----------------------------------------------------------------
; Models for AMD64 (or Intel EM64T) based machines
;
[AuthentecModels.NTamd64]
%AES1610%=ATSwpWDF_Inst, USB\VID_08FF&PID_1600
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1660
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_169F
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_169E
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168F
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168E
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168D
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168C
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168B
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_168A
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1689
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1688
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1687
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1686
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1685
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1684
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1683
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1682
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1681
%AES1660%=ATSwpWDF_Inst, USB\VID_08FF&PID_1680
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2500
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2501
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2502
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2503
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2504
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2505
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2506
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2507
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2508
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_2509
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250A
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250B
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250C
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250D
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250E
%AES2501%=ATSwpWDF_Inst, USB\VID_08FF&PID_250F
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_2580
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_2588
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_2589
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258A
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258B
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258C
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258D
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258E
%AES2501A%=ATSwpWDF_Inst, USB\VID_08FF&PID_258F
%AES2550%=ATSwpWDF_Inst, USB\VID_08FF&PID_2550
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2660
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_269F
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_269E
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268F
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268E
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268D
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268C
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268B
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_268A
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2689
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2688
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2687
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2686
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2685
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2684
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2683
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2682
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2681
%AES2660%=ATSwpWDF_Inst, USB\VID_08FF&PID_2680
%AES2810%=ATSwpWDF_Inst, USB\VID_08FF&PID_2810


; ================= File Copy section =====================

[ATSwpWDF_Inst]
CopyFiles=ATSwpWDF_Inst_CopyFiles
FeatureScore=80

[ATSwpWDF_Inst.HW]
AddReg=ATSwpWDF_Inst_HW.AddReg

[DestinationDirs]
DefaultDestDir = 12

[SourceDisksNames.x86]
1=%Disk1Name%,,,\i386

[SourceDisksNames.amd64]
1=%Disk1Name%,,,\amd64

[SourceDisksFiles]
ATSwpWDF.sys = 1

[ATSwpWDF_Inst_CopyFiles]
ATSwpWDF.sys

; ================= Service Installation section =====================

[ATSwpWDF_Inst.Services]
Addservice = ATSwpWDF, 0x00000002, ATSwpWDF_Inst.AddService

[ATSwpWDF_Inst.AddService]
DisplayName    = %ATSwpWDF.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\ATSwpWDF.sys
AddReg         = ATSwpWDF_Inst.AddReg
LoadOrderGroup = Base

[ATSwpWDF_Inst.AddReg]
HKR, Parameters\Wdf, VerboseOn,       0x00010001, 0
HKR, Parameters\Wdf, VerifierOn,      0x00010001, 0
HKR, Parameters\Wdf, DbgBreakOnError, 0x00010001, 0
HKR,,"DriverVersion",0,%DriverVersionInfo%

; == Clear the Exclusive flag because the service opens multiple handles to the driver ==

[ATSwpWDF_Inst_HW.AddReg]
HKR,,"Exclusive",0x10001,0

; ================= WDF Coinstaller Installation section =====================

[ATSwpWDF_Inst.CoInstallers]
CopyFiles = ATSwpWDF_CoInstaller_CopyFiles
AddReg = ATSwpWDF_CoInstallers_AddReg

[DestinationDirs]
ATSwpWDF_CoInstaller_CopyFiles = 11

[ATSwpWDF_CoInstaller_CopyFiles]
WdfCoinstaller01009.dll

[SourceDisksNames.x86]
1=%Disk1Name%,,,\i386

[SourceDisksNames.amd64]
1=%Disk1Name%,,,\amd64

[SourceDisksFiles]
WdfCoinstaller01009.dll=1 ; make sure the number matches with SourceDisksNames

[ATSwpWDF_CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"

[ATSwpWDF_Inst.Wdf]
KmdfService = ATSwpWDF, ATSwpWDF_wdfsect

[ATSwpWDF_wdfsect]
KmdfLibraryVersion = 1.9

; ================= Strings section =====================

[Strings]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Biometric Devices"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Spanish (Spain)
[Strings.040A]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Dispositivos biométricos"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Spanish (Mexico)
[Strings.080A]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Dispositivos biométricos"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; French
[Strings.040C]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Appareils biométriques"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Portugese (Brazil)
[Strings.0416]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Dispositivos biométricos"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; German
[Strings.0407]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Biometrie-Geräte"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Italian
[Strings.0410]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Dispositivi biometrici"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Japanese
[Strings.0411]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "生体認証デバイス"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Simplified Chinese
[Strings.0804]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "生物识别设备"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Traditional Chinese
[Strings.0404]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = " 生物測定裝置"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Traditional Korean
[Strings.0404]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "바이오메트릭 장치"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Finnish
[Strings.081D]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Biometriset laitteet"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Swedish
[Strings.041D]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "biometrisk utrustning"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Danish
[Strings.0406]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Biometriske enheder"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Norwegian
[Strings.0414]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Biometriske enheter"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"

; Dutch
[Strings.0413]
AuthenTec="AuthenTec Inc."
MfgName="AuthenTec"
AES1610="AuthenTec Inc. AES1610"
AES1660="AuthenTec Inc. AES1660"
AES2501="AuthenTec Inc. AES2501"
AES2501A="AuthenTec Inc. AES2501A"
AES2550="AuthenTec Inc. AES2550"
AES2660="AuthenTec Inc. AES2660"
AES2810="AuthenTec Inc. AES2810"
ATSwpWDF.SvcDesc="AuthenTec TruePrint USB Driver"
ClassName = "Biometrische apparatuur"
Disk_Description="ATSwpWDF USB Installation Disk"
Disk1Name="Fingerprint Device CD-ROM"
DriverVersionInfo="9.0.8.21"
