version: 0x242E(HCI_REVISION), 0x9512(LMP_SUBVERSION)
Update  8723B cut patch code

Version: 0x242E(HCI_REVISION), 0x63D6(LMP_SUBVERSION)
1. Update 8723B CUT patch code

version: 0x242E(HCI_REVISION), 0x4626(LMP_SUBVERSION)
1. First released version for 8723B cut


Version: 0x4239(HCI_REVISION), 0x38DE(LMP_SUBVERSION)
1. erase the trash data in fifo to avoid ring noise after receive hci reset command

Version: 0x4239(HCI_REVISION), 0xD38C(LMP_SUBVERSION)
1. fixed an issue with ring noise of HFP/HSP application
   *  send mute code in SCO/eSCO channel when controller does not receive any hci isochronous data packets from upstream

Version: 0x423B(HCI_REVISION), 0xBD88(LMP_SUBVERSION)
1. enhance acl downlink throughput in USB 2.0

Version: 0x423C(HCI_REVISION), 0x0DAA (LMP_SUBVERSION)
1. correct the gpio settings
2. fixed an issue with afh channel map generator deadlock

Version: 0x423D(HCI_REVISION), 0x1BFB(LMP_SUBVERSION)
1. fixed an issue with missing radio off indication in cpu boot time

Version: 0x424B(HCI_REVISION), 0x4E4C(LMP_SUBVERSION)
1. fixed some IOT issues with some bt devices
2. reset duplicated filter after disable le scan

Version: 0x201E(HCI_REVISION), 0xD3DD(LMP_SUBVERSION)
1. fixed some IOT issues with some bt devices
2. improve the performance of multi-links and co-existence

Version: 0x201E(HCI_REVISION), 0xD701(LMP_SUBVERSION)
1. fixed an issue with power control after download patch code when reboot the system

Version: 0x201E(HCI_REVISION), 0xFC81(LMP_SUBVERSION)
----------------------------------------------------------------------
1. Improve the processing time and flow in feature exchange procedure

Details :
When local device and remote device initate feature exchange simultaneous in noisy environment,
local device has probability to finish one feature exchange procedure too late or reject the 
response pdu from remote device at wrong state. 
When the feature exchange is triggered from the driver via hci read remote features command,
it can cause the driver timeout. This patch can fix the issue and speed up orignal procedure.

Related Operations/Tests :
local device and remote device initate feature exchange simultaneous

Affected Devices :
----------------------------------------------------------------------

Version: 0x241F(HCI_REVISION), 0x99ED(LMP_SUBVERSION)
----------------------------------------------------------------------
1.  Improve the processing time and flow for Win8 WHCK test

Details :
For dual mode test, we adjust some processing time and flow to provide 
more bandwidth for LE. For BR/EDR test, fixed an issue with SSP debug mode.

Related Operations/Tests :
Win8 WHCK test

Affected Devices :
----------------------------------------------------------------------
2. Improve the bandwidth utilization to avoid audio skips when using A2DP 
   headset with HID mouse simultaneously

Details :
When user uses some basic rate A2DP headsets and HID devices simultaneously,
the bandwidth cost is too high to operate the application smoothly in original settings.
We improve the bandwidth utilization in this version.

Related Operations/Tests :
use basic rate A2DP headset and HID mouse simultaneously

Affected Devices :
----------------------------------------------------------------------
3. Fixed an issue with headset reconnect in Win8 Bluetooth MS stack

Details :
During HW Radio Off/On or S3/S4 to S0, some headsets maybe can not be reconnected
or audio player can not be played automatically because Win8 Bluetooth Stack
does not receive excepted event packet. We fix an issue about this.

Related Operations/Tests :
connect the headset and play music then HW Radio Off/On or S3/S4 to S0 

Affected Devices :
----------------------------------------------------------------------

Version: 0x241F(HCI_REVISION), 0xBDDA(LMP_SUBVERSION)
----------------------------------------------------------------------
1. Fixed an issue with A2DP reconnect after resume from S3 in 
   Win8 Bluetooth MS stack

Details :
During S3 to S0, some headsets maybe can not be reconnected or audio player 
can not be played automatically because Win8 Bluetooth Stack can not finish
some procedures before enter S3. We fix an issue about this.

Related Operations/Tests :
connect the headset and play music from S3 to S0

Affected Devices :
----------------------------------------------------------------------
2. Improve Win8 WHCK dual mode test in noisy environment

Details :
Some criterion of Win8 WHCK test cases can not pass easily in noisy environment.
We adjust some procedure and guarantee bandwidth for dual mode to help pass test 
cases more easily.

Related Operations/Tests :
Win8 WHCK test

Affected Devices :
----------------------------------------------------------------------

RtkBtFilter_1227.2012_1.2.2.5_Without_BtDevMgr

Version: 0x2420(HCI_REVISION), 0x617F(LMP_SUBVERSION)

root cause:
    In a noisy environment, sometimes LE initiator is hard to find the LE advertiser when there is a BR/EDR link sending/receiving ACL data.

final solution:
    We increase the scanning rate of LE initiator when there is a BR/EDR link sending/receiving ACL data.

----------------------------------------------------------------------
