;
;  Purpose:   Netcard setup information file for Windows 98SE/ME/2000/XP/Server2003 x86 Edition
;
;  Author:    Anders Ma
;
;  Date:      May, 2012
;
;  Copyright: Copyright (C) VIA Technologies, Inc.
;

[Version]
CatalogFile = getndis.cat
Signature   = "$Chicago$"
Compatible  = 1
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Prov%
DriverVer   = 05/10/2012, 1.76.0.1

[Manufacturer]
%Manuf%     = MANUF

[MANUF]
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_01101106
%VT3119.DeviceDesc% = VT3119MgF.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_0808A0A0
%GEN119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119

;(1)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_011016F3
;(4)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_043C1462
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_047C1462
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_04701462
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_70761462
;(1)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_90271695
;(1)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_E0001458
;(4)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_20011919
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_20031919
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_20041919
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_20061919
;(1)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_000218EE
;(1)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_85001584
;(1)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_FC10270F
;(1)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_01101019
;(4)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_A00A14FF
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_A00E14FF
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_A01614FF
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_A02314FF
;(3)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_00291B0A
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_00331B0A
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_002F1B0A
;(1)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_02221025
;(3)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_0E1B105B
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_0CF9105B
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_0CD8105B
;(1)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_0702A0A0
;(2)
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_31701297
%VT3119.DeviceDesc% = VT3119.ndi, PCI\VEN_1106&DEV_3119&SUBSYS_51701297
;-------------------------------------------------------------------------------
; ndi for 3119 force wakeup mode to magic
;-------------------------------------------------------------------------------
[VT3119MgF.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = GET.delreg, GET.SW.delreg
AddReg          = VT3119.reg, GET.reg, GET.reg.NT, Tagging.reg, VLAN.reg, Jumbo.reg, WakeupMgF.reg, GET.SW.NT
CopyFiles       = GET.CopyFiles.NTx86, GET.SW.CopyFiles.NTx86

[VT3119MgF.ndi.NTx86.Services]
AddService      = GETND5BV, 2, GET.Service, GET.EventLog

;-------------------------------------------------------------------------------
; ndi for 3119
;-------------------------------------------------------------------------------
[VT3119.ndi]
DelReg          = GET.delreg, GET.SW.delreg
AddReg          = VT3119.reg, GET.reg, GET.reg.win, Tagging.reg, VLAN.reg, Jumbo.reg, GET.SW.win
CopyFiles       = GET.ndi.CopyFiles, GET.SW.CopyFiles

[VT3119.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = GET.delreg, GET.SW.delreg
AddReg          = VT3119.reg, GET.reg, GET.reg.NT, Tagging.reg, VLAN.reg, Jumbo.reg, Wakeup.reg, GET.SW.NT
CopyFiles       = GET.CopyFiles.NTx86, GET.SW.CopyFiles.NTx86

[VT3119.ndi.NTx86.Services]
AddService      = GETND5BV, 2, GET.Service, GET.EventLog

;-------------------------------------------------------------------------------
; VT3119 specific
;
[VT3119.reg]
HKR, Ndi, DeviceID,    0, "PCI\VEN_1106&DEV_3119"
HKR, ,    AdapterType, 0, "5"
HKR, ,    MediaType,   0, "1"

;-------------------------------------------------------------------------------
; Common driver parameters
;
[GET.reg]
; UI for Connection Type
HKR, ,                               ConnectionType, 0, "0"
HKR, Ndi\params\ConnectionType,      ParamDesc,      0, %ConnectionType%
HKR, Ndi\params\ConnectionType,      default,        0, "0"
HKR, Ndi\params\ConnectionType,      type,           0, "enum"
HKR, Ndi\params\ConnectionType\enum, 0,              0, %autoN%
HKR, Ndi\params\ConnectionType\enum, 1,              0, %100HD%
HKR, Ndi\params\ConnectionType\enum, 2,              0, %100FD%
HKR, Ndi\params\ConnectionType\enum, 3,              0, %10HD%
HKR, Ndi\params\ConnectionType\enum, 4,              0, %10FD%
HKR, Ndi\params\ConnectionType\enum, 5,              0, %1000FD%
HKR, Ndi\params\ConnectionType,      flag,           1, "20","00","00","00"

; UI for Flow control capability advertisement
HKR, ,                         FlowCtrl,  0, "0"
HKR, Ndi\params\FlowCtrl,      ParamDesc, 0, %FlowCtl%
HKR, Ndi\params\FlowCtrl,      default,   0, "0"
HKR, Ndi\params\FlowCtrl,      type,      0, "enum"
HKR, Ndi\params\FlowCtrl\enum, 0,         0, %HwDefault%
HKR, Ndi\params\FlowCtrl\enum, 1,         0, %EnableTx%
HKR, Ndi\params\FlowCtrl\enum, 2,         0, %EnableRx%
HKR, Ndi\params\FlowCtrl\enum, 3,         0, %EnableTxRx%
HKR, Ndi\params\FlowCtrl\enum, 4,         0, %Disabled%
HKR, Ndi\params\FlowCtrl,      flag,      1, "20","00","00","00"

; Activity Property show Packets or Bytes
HKR, ,                                 ActivityProperty, 0, "0"
HKR, Ndi\params\ActivityProperty,      ParamDesc,        0, %ActivityProperty%
HKR, Ndi\params\ActivityProperty,      default,          0, "0"
HKR, Ndi\params\ActivityProperty,      type,             0, "enum"
HKR, Ndi\params\ActivityProperty\enum, 0,                0, %ShowPackets%
HKR, Ndi\params\ActivityProperty\enum, 1,                0, %ShowBytes%
HKR, Ndi\params\ActivityProperty,      flag,             1, "20","00","00","00"

; Validate Rx SNAP/802.3 packet length
HKR, , ValidatePacketLen,    0, "0"

; Nway Forced Mode
HKR, , NwayForce,            0, "1"

; Power Management Capability
HKR, , PMC,                  0, "0"

HKR, , ReceiveBurstIndicate, 0, "64"
HKR, , ReceiveThreshold,     0, "0"
HKR, , BurstLength,          0, "7"
HKR, , MapRegisters,         0, "128"
HKR, , TxSupThr,             0, "31"
HKR, , RxSupThr,             0, "31"
HKR, , SyncTIC,              0, "1"
HKR, , MRDPL,                0, "1"

;-------------------------------------------------------------------------------
; Win95/Win98/WinME only
;
[GET.reg.win]
HKR, Ndi,            NdiInstaller, 0, "wndi.dll, NdiProc"
HKR, Ndi\Install,    ndis3,        0, "GET.ndis5"

HKR, NDIS,           MajorNdisVersion, 1, 03
HKR, NDIS,           MinorNdisVersion, 1, 0A
HKR, NDIS,           LogDriverName,    0, "GETND5AV"

HKR, ,               DevLoader,  0, "*ndis"
HKR, ,               DeviceVxDs, 0, "getnd5av.sys"

HKR, NDIS\NDIS2,     DriverName, 0, "GETND2$"
HKR, NDIS\NDIS2,     FileName,   0, "getnd2.dos"

HKR, Ndi\Interfaces, DefLower,   0, "ethernet"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, DefUpper,   0, "ndis3,ndis2"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"

; Network Address, No UI
HKR, ,                         NetworkAddress, 0, ""

; UI for Wake On LAN Event
HKR, ,                         WOLEvent,  0, "0"
HKR, Ndi\params\WOLEvent,      ParamDesc, 0, %WOLEvent%
HKR, Ndi\params\WOLEvent,      default,   0, "0"
HKR, Ndi\params\WOLEvent,      type,      0, "enum"
HKR, Ndi\params\WOLEvent\enum, 0,         0, %OSDefault%
HKR, Ndi\params\WOLEvent\enum, 1,         0, %OSAndUnicast%
HKR, Ndi\params\WOLEvent,      flag,      1, "20","00","00","00"

; UI for TxBuffer Number
HKR, ,                           TransmitBuffers, 0, "128"
HKR, Ndi\params\TransmitBuffers, ParamDesc,       0, %TXBuffer%
HKR, Ndi\params\TransmitBuffers, default,         0, "128"
HKR, Ndi\params\TransmitBuffers, type,            0, "int"
HKR, Ndi\params\TransmitBuffers, Min,             0, "64"
HKR, Ndi\params\TransmitBuffers, Max,             0, "256"
HKR, Ndi\params\TransmitBuffers, Step,            0, "1"
HKR, Ndi\params\TransmitBuffers, Base,            0, "10"
HKR, Ndi\params\TransmitBuffers, flag,            1, "20","00","00","00"

; UI for RxBuffer Number
HKR, ,                          ReceiveBuffers, 0, "160"
HKR, Ndi\params\ReceiveBuffers, ParamDesc,      0, %RXBuffer%
HKR, Ndi\params\ReceiveBuffers, default,        0, "160"
HKR, Ndi\params\ReceiveBuffers, type,           0, "int"
HKR, Ndi\params\ReceiveBuffers, Min,            0, "64"
HKR, Ndi\params\ReceiveBuffers, Max,            0, "256"
HKR, Ndi\params\ReceiveBuffers, Step,           0, "4"
HKR, Ndi\params\ReceiveBuffers, Base,           0, "10"
HKR, Ndi\params\ReceiveBuffers, flag,           1, "20","00","00","00"

;-------------------------------------------------------------------------------
; 16-bit UnInstaller
[GET.SW.win]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Velocity_VIA, DisplayName, 0, %VT3119.DeviceDesc%
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Velocity_VIA, UninstallString, 0, "Rundll.exe vuins16.dll,vuins16Ex $Velocity $VIA"
HKLM, Software\VN_VUIns\Velocity\VIA\DeviceIdList, 3119, 0, "0"

;-------------------------------------------------------------------------------
; Windows 2000/XP/Server2003 only
;
[GET.reg.NT]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "GETND5BV"

; This parameter only for Win2000
HKR, ,               2kScatterGather, 0, "1"

; UI for TxBuffer Number
HKR, ,                           TransmitBuffers, 0, "256"
HKR, Ndi\params\TransmitBuffers, ParamDesc,       0, %TXBuffer%
HKR, Ndi\params\TransmitBuffers, default,         0, "256"
HKR, Ndi\params\TransmitBuffers, type,            0, "int"
HKR, Ndi\params\TransmitBuffers, Min,             0, "64"
HKR, Ndi\params\TransmitBuffers, Max,             0, "384"
HKR, Ndi\params\TransmitBuffers, Step,            0, "1"
HKR, Ndi\params\TransmitBuffers, Base,            0, "10"

; UI for RxBuffer Number
HKR, ,                          ReceiveBuffers, 0, "160"
HKR, Ndi\params\ReceiveBuffers, ParamDesc,      0, %RXBuffer%
HKR, Ndi\params\ReceiveBuffers, default,        0, "160"
HKR, Ndi\params\ReceiveBuffers, type,           0, "int"
HKR, Ndi\params\ReceiveBuffers, Min,            0, "64"
HKR, Ndi\params\ReceiveBuffers, Max,            0, "256"
HKR, Ndi\params\ReceiveBuffers, Step,           0, "4"
HKR, Ndi\params\ReceiveBuffers, Base,           0, "10"

; UI for user defined Network Address
HKR, ,                          NetworkAddress, 0, ""
HKR, Ndi\params\NetworkAddress, ParamDesc,      0, %NetAddress%
HKR, Ndi\params\NetworkAddress, Default,        0, ""
HKR, Ndi\params\NetworkAddress, type,           0, "edit"
HKR, NDI\params\NetworkAddress, LimitText,      0, "12"
HKR, NDI\params\NetworkAddress, UpperCase,      0, "1"
HKR, NDI\params\NetworkAddress, optional,       0, "1"
HKR, NDI\params\NetworkAddress, Base,           0, "16"

; UI for Adaptive Interrupt Capability -> Optimized for performance by Interrupt
HKR, ,                   AI,        0, "1"
HKR, Ndi\params\AI,      ParamDesc, 0, %AI%
HKR, Ndi\params\AI,      default,   0, "1"
HKR, Ndi\params\AI,      type,      0, "enum"
HKR, Ndi\params\AI\enum, 0,         0, %Disabled%
HKR, Ndi\params\AI\enum, 1,         0, %Enabled%

HKR, ,                   TqeTmr,    0, "89"
HKR, ,                   RqeTmr,    0, "20"
HKR, ,                   TxCntWak,  0, "8"

; UI for Rx Checksum Offload Ability
HKR, ,                           RxCksmOfld, 0, "1"
HKR, Ndi\params\RxCksmOfld,      ParamDesc,  0, %RxCksmOfld%
HKR, Ndi\params\RxCksmOfld,      default,    0, "1"
HKR, Ndi\params\RxCksmOfld,      type,       0, "enum"
HKR, Ndi\params\RxCksmOfld\enum, 0,          0, %Disabled%
HKR, Ndi\params\RxCksmOfld\enum, 1,          0, %Enabled%

; UI for Tx Task Offload Ability
HKR, ,                           TxTaskOfld, 0, "2"
HKR, Ndi\params\TxTaskOfld,      ParamDesc,  0, %TxTaskOfld%
HKR, Ndi\params\TxTaskOfld,      default,    0, "2"
HKR, Ndi\params\TxTaskOfld,      type,       0, "enum"
HKR, Ndi\params\TxTaskOfld\enum, 0,          0, %Disabled%
HKR, Ndi\params\TxTaskOfld\enum, 1,          0, %TxTaskOfldCksm%
HKR, Ndi\params\TxTaskOfld\enum, 2,          0, %TxTaskOfldTcpLS%

; TCPLS Max Segment count
HKR, ,                           TCPLSSeg,   0, "8"

;-------------------------------------------------------------------------------
; 32-bit UnInstaller
[GET.SW.NT]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Velocity_VIA, DisplayName, 0, %VT3119.DeviceDesc%
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Velocity_VIA, UninstallString, 0, "Rundll32.exe vuins32.dll,vuins32Ex $Velocity $VIA"
HKLM, Software\VN_VUIns\Velocity\VIA\DeviceIdList, 3119, 0, "0"

;-------------------------------------------------------------------------------
;
[Tagging.reg]
; number of Tx queue allocation
HKR, ,                          TxQueueNum, 0, "4"
; UI for 802.1p/Q Packet Tagging
HKR, ,                          8021pqtag, 0, "0"
HKR, Ndi\Params\8021pqtag,      ParamDesc, 0, %8021pq%
HKR, Ndi\Params\8021pqtag,      Default,   0, "0"
HKR, Ndi\Params\8021pqtag,      type,      0, "enum"
HKR, Ndi\Params\8021pqtag\enum, "0",       0, %Disabled%
HKR, Ndi\Params\8021pqtag\enum, "1",       0, %Enabled%
HKR, Ndi\params\8021pqtag,      flag,      1, "20","00","00","00"

;-------------------------------------------------------------------------------
;
[VLAN.reg]
; UI for static single VLAN ID setting
HKR, ,                  VLANID,    0, "0"
HKR, Ndi\params\VLANID, ParamDesc, 0, %VLANID%
HKR, Ndi\params\VLANID, default,   0, "0"
HKR, Ndi\params\VLANID, type,      0, "int"
HKR, Ndi\params\VLANID, Min,       0, "0"
HKR, Ndi\params\VLANID, Max,       0, "4094"
HKR, Ndi\params\VLANID, Step,      0, "1"
HKR, Ndi\params\VLANID, Base,      0, "10"
HKR, Ndi\params\VLANID, flag,      1, "20","00","00","00"

;-------------------------------------------------------------------------------
;
[Jumbo.reg]
HKR, ,                      Jumbo,     0, "0"
HKR, Ndi\params\Jumbo,      ParamDesc, 0, %Jumbo%
HKR, Ndi\params\Jumbo,      default,   0, "0"
HKR, Ndi\params\Jumbo,      type,      0, "enum"
HKR, Ndi\params\Jumbo\enum, 0,         0, %Disabled%
HKR, Ndi\params\Jumbo\enum, 1,         0, %Enabled%
HKR, Ndi\params\Jumbo,      flag,      1, "20","00","00","00"

;-------------------------------------------------------------------------------
;
[Wakeup.reg]
HKR, ,                       Wakeup,    0, "0"
HKR, Ndi\params\Wakeup,      ParamDesc, 0, %Wakeup%
HKR, Ndi\params\Wakeup,      default,   0, "0"
HKR, Ndi\params\Wakeup,      type,      0, "enum"
HKR, Ndi\params\Wakeup\enum, 0,         0, %OSControl%
HKR, Ndi\params\Wakeup\enum, 1,         0, %Magic%
HKR, Ndi\params\Wakeup\enum, 2,         0, %Pattern%
HKR, Ndi\params\Wakeup\enum, 3,         0, %All%
HKR, Ndi\params\Wakeup,      flag,      1, "20","00","00","00"

; WOL Speed Forced 10M
HKR, ,                                         WOLSpeedForced10M,        0, "1"
HKR, Ndi\Params\WOLSpeedForced10M,             ParamDesc,                0, %WOL10M%
HKR, Ndi\Params\WOLSpeedForced10M,             Default,                  0, "1"
HKR, Ndi\Params\WOLSpeedForced10M,             type,                     0, "enum"
HKR, Ndi\Params\WOLSpeedForced10M\enum,        "0",                      0, %Disabled%
HKR, Ndi\Params\WOLSpeedForced10M\enum,        "1",                      0, %10MbpsFirst%
HKR, Ndi\Params\WOLSpeedForced10M\enum,        "2",                      0, %100MbpsFirst%

;-------------------------------------------------------------------------------
;force wakeup mode to magic
[WakeupMgF.reg]
HKR, ,                       Wakeup,    0, "1"
HKR, Ndi\params\Wakeup,      ParamDesc, 0, %Wakeup%
HKR, Ndi\params\Wakeup,      default,   0, "1"
HKR, Ndi\params\Wakeup,      type,      0, "enum"
HKR, Ndi\params\Wakeup\enum, 1,         0, %Magic%
HKR, Ndi\params\Wakeup,      flag,      1, "20","00","00","00"

;-------------------------------------------------------------------------------
; Installation for NT (Windows 2000/XP/Server2003)
;
[GET.CopyFiles.NTx86]
getnd5bv.sys,,,2

[GET.SW.CopyFiles.NTx86]
vuins32.dll,,,2

[GET.Service]
DisplayName    = %GET.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\getnd5bv.sys
LoadOrderGroup = NDIS

[GET.EventLog]
AddReg = GET.AddEventLog.reg

[GET.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;-------------------------------------------------------------------------------
; Installation for Windows 95/98/ME
;
[GET.ndis5]
CopyFiles=GET.ndis5.CopyFiles

[GET.ndis4]
CopyFiles=GET.ndis4.CopyFiles

[GET.ndis3]
CopyFiles=GET.ndis3.CopyFiles

[GET.ndis2]
CopyFiles=GET.ndis2.CopyFiles

;-------------------------------------------------------------------------------
; CopyFiles sections for Windows 95/98/ME
;
[GET.ndi.CopyFiles]
wndi.dll,,,2

[GET.ndis5.CopyFiles]
getnd5av.sys,,,2

[GET.ndis4.CopyFiles]
getnd4.sys,,,2

[GET.ndis3.CopyFiles]
getnd3.sys,,,2

[GET.ndis2.CopyFiles]
getnd2.dos

[GET.SW.CopyFiles]
vuins16.dll,,,2

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir               = 11
GET.CopyFiles.NTx86          = 12
GET.ndis2.CopyFiles          = 10
GET.SW.CopyFiles.NTx86       = 11
GET.SW.CopyFiles             = 11

[SourceDisksFiles]
getnd5av.sys = 1
getnd5bv.sys = 1
getnd4.sys   = 1
getnd3.sys   = 1
wndi.dll     = 1
getnd2.dos   = 1
vuins32.dll  = 1
vuins16.dll  = 1

[SourceDisksNames]
1 = %DiskName%,,,

;-------------------------------------------------------------------------------
; Uninstall/DelFiles/DelReg
;
[GET.delreg]
HKR, Ndi\Params
[GET.SW.delreg]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VUInstVelocity
HKLM, Software\VNT\VUInst\Velocity
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Velocity_VNT
HKLM, Software\VN_VUIns\Velocity\VNT
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VUInstVelocity
HKLM, Software\VIA\VUInst\Velocity
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Velocity_VIA
HKLM, Software\VN_VUIns\Velocity\VIA

;-------------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
Prov                    = "VIA"
DiskName            = "VIA Gigabit Ethernet Adapter driver disk"
ConnectionType   = "Connection Type"
autoN                  = "Auto-Negotiation"
100HD                 = "100BaseTx Half Duplex"
100FD               = "100BaseTx Full Duplex"
10HD                = "10BaseT Half Duplex"
10FD                = "10BaseT Full Duplex"
1000FD             = "1000BaseT Full Duplex"           
Disabled            = "Disabled"
Enabled             = "Enabled"
WOLEvent            = "Wake On LAN Event"
OSDefault           = "OS Default Event"
OSAndUnicast        = "OS Default & Unicast"
TXBuffer            = "Transmit Buffers"
RXBuffer            = "Receive Buffers"
NetAddress          = "Network Address"
FlowCtl             = "Flow Control"
HwDefault           = "Hardware Default (Auto)"
EnableTx            = "Enable Tx"
EnableRx            = "Enable Rx"
EnableTxRx          = "Enable Tx/Rx"
8021pq              = "802.1p/Q Tagging"
VLANID              = "VLAN ID"
RxCksmOfld          = "Rx Checksum Offload"
TxTaskOfld          = "Tx Task Offload"
TxTaskOfldCksm      = "Checksum Offload"
TxTaskOfldTcpLS     = "Checksum and TCP Large Send Offload"
Jumbo               = "Jumbo Frames Support"
AI                  = "High Performance Interrupt"
Wakeup              = "Wake up Type"
OSControl           = "OS Controlled"
Magic               = "Magic Packet"
Pattern             = "Pattern Match"
All                 = "ALL"
WOL10M              = "WOL Speed"
100MbpsFirst        = "100 Mbps First"
10MbpsFirst         = "10 Mbps First"
ActivityProperty    = "Activity Property"
ShowPackets         = "Show Packets"
ShowBytes           = "Show Bytes"

Manuf                = "VIA Technologies, Inc."
VT3119.DeviceDesc    = "VIA Velocity Family Gigabit Ethernet Adapter"
GEN119.DeviceDesc    = "VIA Velocity-Compatible Ethernet Adapter"
GET.Service.DispName = "VIA Velocity Family Gigabit Ethernet Adapter Driver"
