; /****************************************************************************
; * Copyright 2009 Qualcomm Atheros,Inc., all rights reserved.                *
; * INF file for Atheros reference designs                                    *
; *   Added support for ar946x chip  11/11/2011                               *
; ****************************************************************************/

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
LoutFiles   = layout.inf
CatalogFile = akw8x86.cat
DriverVer   = 04/01/2013,10.0.1.242

[Manufacturer]
%ATHEROS%     = Atheros, NTX86.6.2

[ControlFlags]
ExcludeFromSelect = *
;
; OS Win8 6.2 Manufacturer section
;
[Atheros.NTX86.6.2]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
;legacy HW Entries
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946x.ndi,   PCI\VEN_168C&DEV_0034&SUBSYS_20031A56  ;Killer 2x2 1202
%ATHR.DeviceDesc.osprey%   = ATHR_DEV_OS61_OSPREY.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_20011A56  ;killer 3x3 1103
%BFOOT.DeviceDesc.3096%    = ATHR_DEV_OS61_OSPREY.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_20001A56  ;Killer 2x2 1102
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,   PCI\VEN_168C&DEV_0036&SUBSYS_3027168C  ;Non-Killer
;
;
; OS 6.2 Manufacturer section
;
[BFOOT_DEV_OS61_002A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = killer_os61.reg, atheros11n.reg, ledcontrol2.reg, btcoex.reg, l2devices.reg 
DelReg          = atheros.DelReg
CopyFiles       = killer.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[BFOOT_DEV_OS61_002A.ndi.NTX86.Services]
AddService = akw8x86, 2, killer.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[BFOOT_DEV_OS61_002A.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_OSPREY.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = killer_os61.reg, atheros11n.reg, led_func0_10.reg, smpsDynamic.reg, htAdhoc.reg, l2devices.reg
DelReg          = atheros.DelReg
CopyFiles       = killer.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_OSPREY.ndi.NTX86.Services]
AddService = akw8x86, 2, killer.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_OSPREY.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

;
;  Jupiter support secton
;
[ATHR_DEV_OS61_946x.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = killer_os61.reg, atheros11n.reg, smpsDynamic.reg, led_func0_4.reg, htAdhoc.reg, l2devices.reg, jupiter2ant.reg
DelReg          = atheros.DelReg
CopyFiles       = killer.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_946x.ndi.NTX86.Services]
AddService = akw8x86, 2, killer.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_946x.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_956x.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = killer_os61.reg, atheros11n.reg, smpsDynamic.reg, led_func0_4.reg, htAdhoc.reg, l2devices.reg, jupiter2ant.reg
DelReg          = atheros.DelReg
CopyFiles       = killer.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_956x.ndi.NTX86.Services]
AddService = akw8x86, 2, killer.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_956x.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;;End of Others Section

[killer_os61.reg]
HKR, Ndi,                           Service,    0, "akw8x86"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet,vwifi"

[atheros11n.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "512"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "512"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\NetworkAddress,     ParamDesc,  0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,     default,    0,  ""
HKR, Ndi\params\NetworkAddress,     LimitText,  0,  "12"
HKR, Ndi\params\NetworkAddress,     UpperCase,  0,  "1"
HKR, Ndi\params\NetworkAddress,     optional,   0,  "1"
HKR, Ndi\params\NetworkAddress,     type,       0,  "edit"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

;/* Enable these if VLAN or 802.1p is to be enabled */
;HKR, Ndi\Params\*PriorityVLANTag,  ParamDesc,  , %PriorityVLAN%
;HKR, Ndi\Params\*PriorityVLANTag,  default,    , "3"
;HKR, Ndi\Params\*PriorityVLANTag,  type,       , "enum"
;HKR, Ndi\Params\*PriorityVLANTag\enum, 0,      , %PriorityVLANDisabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 1,      , %PriorityEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 2,      , %VLANEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 3,      , %PriorityVLANEnabled%

[atheros.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,halPcieClockReq
HKR,Ndi\params,MapRegisters,0x2000
HKR,,MapRegisters
HKR,Ndi\params,radioEnable,0x2000
HKR,Ndi\params,sleepMode,0x2000
HKR,,sleepMode
HKR,,gpioFunc0ActHi
HKR,,gpioFunc1ActHi
HKR,,gpioLedCustom
HKR,,gpioPinFunc0
HKR,,gpioPinFunc1
HKR,,transmitRateMax
HKR, Ndi\params\*TransmitBuffers
HKR,,*TransmitBuffers
HKR,,rxChainMask
HKR,,txChainMaskLegacy
HKR,,rxChainMaskLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR, Ndi\params\smpsDynamic
HKR,,d3forcel1disable.reg
HKR,,d3forcel1disablekite.reg
HKR,,d3forcel1disablekite1.reg
HKR,,wmeEnabled
HKR,,halPcieWaen
HKR,,halPcieDetach
HKR,,ampEnable
HKR,Ndi\IHVExtensions

[expresscardaspmoff.reg]
HKR, ,                                  pciDetectEnable,                0x00002,  "2"
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[rfKillDelayDetect.reg]
HKR, ,                                  rfKillDelayDetect,              0x00002,  "1"

[d3hot.reg] 
HKR, ,                                  halPciePowerReset,              0x00002,  "0"
HKR, ,                                  halPcieRestore,                 0x00002,  "1"

[enableswretry] 
HKR, ,                                  numSwRetries,                   0x00002,  "4"

[interruptpolling.reg]
HKR, ,                                  isrPollInterval,                0x00002,  "100"

[pcibusconfig.reg]
HKR, ,                                  BusConfig,                      0x00002,  "0"
HKR, ,                                  serializeRegMode,               0x00002,  "2"

[serializing.reg]
HKR, ,                                  serializeRegMode,               0x00002,  "1"

[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1647"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "1647",                         0,        %Auto%
HKR, Ndi\params\NetBand\enum,           "1603",                         0,        %5GOnly%
HKR, Ndi\params\NetBand\enum,           "44",                           0,        %2GOnly%

[roamthreshA.reg]
HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

[ignore11d.reg]
HKR,NDI\params\ignore11dBeacon,         ParamDesc,,                               %11DModeSwitch%
HKR,NDI\params\ignore11dBeacon,         type,,                                    "enum"
HKR,NDI\params\ignore11dBeacon,         Default,,                                 "1"
HKR,NDI\params\ignore11dBeacon\enum,    0,,                                       %Enable%
HKR,NDI\params\ignore11dBeacon\enum,    1,,                                       %Disable%

;[radioswitch.reg]
;HKR, Ndi\params\radioEnable,            ParamDesc,                      0,        %radioEnable%
;HKR, Ndi\params\radioEnable,            Base,                           0,        "10"
;HKR, Ndi\params\radioEnable,            default,                        0,        "1"
;HKR, Ndi\params\radioEnable,            type,                           0,        "enum"
;HKR, Ndi\params\radioEnable\enum,       "1",                            0,        %radioEnableOn%
;HKR, Ndi\params\radioEnable\enum,       "0",                            0,        %radioEnableOff%

[overridetxok.reg]
HKR, ,                                  OverrideTxOk,                   0x00002,  "1"

[adhocchannelselect.reg]
HKR, Ndi\params\defaultIbssChannel,     ParamDesc,                      0,        %adhocchannel%
HKR, Ndi\params\defaultIbssChannel,     default,                        0,        "10"
HKR, Ndi\params\defaultIbssChannel,     min,                            0,        "1"
HKR, Ndi\params\defaultIbssChannel,     max,                            0,        "11"
HKR, Ndi\params\defaultIbssChannel,     step,                           0,        "1"
HKR, Ndi\params\defaultIbssChannel,     base,                           0,        "10"
HKR, Ndi\params\defaultIbssChannel,     type,                           0,        "int"

[5416.bgnxb.reg]
HKR, ,                                  NetBand,                        0x00002,  "26636"
HKR, ,                                  wmodeselect,                    0x00002,  "26636"

[5416.bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130671"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "130671",                       0,  %Auto%
HKR, Ndi\params\NetBand\enum,           "104003",                       0,  %5GOnly%
HKR, Ndi\params\NetBand\enum,           "26668",                        0,  %2GOnly%

[wirelessmodeselectkite.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "26636"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "26636",                        0,  %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "12",                           0,  %WirelessMode11bgOnly%

[5416.antennacontrols.reg] 
HKR, ,                                  rxChainMask,                    0x00002,  "7"
;HKR, ,                                  txChainMaskLegacy,              0x00002,  "5"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "7"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

[pushbutton.reg]
HKR, ,                                  wpsButtonGpio,                  0x00002,  "9"

[jupiter2ant.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "3"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "3"

[smpsDynamic.reg]
HKR, Ndi\params\smpsDynamic,            ParamDesc,  0,  %smpsDynamic%
HKR, Ndi\params\smpsDynamic,            Base,       0,  "10"
HKR, Ndi\params\smpsDynamic,            default,    0,  "0"
HKR, Ndi\params\smpsDynamic,            type,       0,  "enum"
HKR, Ndi\params\smpsDynamic\enum,       "1",        0,  %Enable%
HKR, Ndi\params\smpsDynamic\enum,       "0",        0,  %Disable%

[amp.reg]
HKR, ,                                  ampEnable,                      0x00002,  "1"
HKR, Ndi\params\ampEnable,              ParamDesc,                      0,        %bt30%
HKR, Ndi\params\ampEnable,              default,                        0,        "1"
HKR, Ndi\params\ampEnable,              type,                           0,        "enum"
HKR, Ndi\params\ampEnable\enum,         "1",                            0,        %bt30enable%
HKR, Ndi\params\ampEnable\enum,         "0",                            0,        %bt30disable%

[ampBFilter.reg]
HKR, ,                                  ampFilterName,                  0x00002,  "BTWAMPFL"

[ampFilter.reg]
HKR, ,                                  ampFilterName,                  0x00002,  "ATHAMPFL"

[customer0.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, ,                                  capLinkSp,                      0x00002,  "1" 
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0_HB95.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0_HB93.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0LED.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"

[customer0LED1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"

[customer0LED2.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"

[customer0_11n.reg]
;PCIe Related
HKR, ,                                  radioEnableInterval,            0x00002,  "5"
HKR, ,                                  pcieAspm,                       0x00002,  "2"
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  forceWake,                      0x00002,  "0"
HKR, ,                                  antennaSwitchSwap,              0x00002,  "1"
;LED Related
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
;General Customer0
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,,      %11DModeSwitch%
HKR,NDI\params\ignore11dBeacon,type,,           "enum"
HKR,NDI\params\ignore11dBeacon,Default,,        "1"
HKR,NDI\params\ignore11dBeacon\enum,0,,         %Enable%
HKR,NDI\params\ignore11dBeacon\enum,1,,         %Disable%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,              step,                           0,  "1"
HKR, Ndi\params\roamRssiA,              base,                           0,  "10"
HKR, Ndi\params\roamRssiA,              type,                           0,  "int"

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

[customer1ani.reg]
HKR, Ndi\params\rssiThrHigh,            ParamDesc,                      0,        %rssiThrHigh%
HKR, Ndi\params\rssiThrHigh,            Base,                           0,        "10"
HKR, Ndi\params\rssiThrHigh,            default,                        0,        "40"
HKR, Ndi\params\rssiThrHigh,            type,                           0,        "enum"
HKR, Ndi\params\rssiThrHigh\enum,       "40",                           0,        %rssiThrHighNormal%
HKR, Ndi\params\rssiThrHigh\enum,       "32",                           0,        %rssiThrHighMin%

[customer1roamPolicy.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh%

[customer1GreenTx.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %GreenTx%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "0"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "0",                            0,        %GreenTxEnableOff%
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %GreenTxEnableOn%

[customer2.reg]
HKR,,                                   linkLEDFunc,                    0,        "53"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[customer2.11n.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"

[customer2merlin.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"

[customer3.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  LinkLEDFunc,                    0x00002,  "19"
HKR, ,                                  ActivityLEDFunc,                0x00002,  "21"

[customer3a.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

;[customer3b.reg]
;HKR, ,                                  gpioPinFunc1,                  0x00002,  "3"
;HKR, ,                                  overrideACstatus,              0x00002,  "1"
;HKR, ,                                  halPcieClockReq,               0x00002,  "0"
;HKR, ,                                  gpioLedCustom,                 0x00002,  "4"
;HKR, ,                                  gpioFunc1ActHi,                0x00002,  "0"

[customer3c.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3d.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "0"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer3e.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3f.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3_legacybgwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "12"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "12",                           0,        %wModeLegacy11bg%

[customer4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4as.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4adhoc.reg]
HKR, ,                                  defaultIbssChannel,             0x00002,  "11"

[customer4b.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a_ASPM.reg]
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[customer5Led.reg]
HKR, ,                                  softLEDEnable,                  0x00002,  "1"
HKR, ,                                  swapDefaultLED,                 0x00002,  "1"

[customer5.11nLED.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer5.PCIe11nLed.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer5.3x3.reg]
HKR, ,                                  txChainMask,                    0x00002,  "7"
HKR, ,                                  rxChainMask,                    0x00002,  "7"

[customer7Led.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "2"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "1"

[customer9Led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[Customer15a.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[Customer15b.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[gpioled.reg]
HKR,,                                   linkLEDFunc,                    0,        "49"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[ratecap.reg]
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"

[customer11n.reg]
HKR, Ndi\params\*ReceiveBuffers,        ParamDesc,                      0,        "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,        default,                        0,        "256"
HKR, Ndi\params\*ReceiveBuffers,        min,                            0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        max,                            0,        "00000512"
HKR, Ndi\params\*ReceiveBuffers,        step,                           0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        Base,                           0,        "10"
HKR, Ndi\params\*ReceiveBuffers,        type,                           0,        "int"
HKR, Ndi\params\*TransmitBuffers,       ParamDesc,                      0,        "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,       default,                        0,        "512"
HKR, Ndi\params\*TransmitBuffers,       min,                            0,        "1"
HKR, Ndi\params\*TransmitBuffers,       max,                            0,        "00000512"
HKR, Ndi\params\*TransmitBuffers,       step,                           0,        "1"
HKR, Ndi\params\*TransmitBuffers,       Base,                           0,        "10"
HKR, Ndi\params\*TransmitBuffers,       type,                           0,        "int"
HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,        %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,        "10"
HKR, Ndi\params\shortPreamble,          default,                        0,        "1"
HKR, Ndi\params\shortPreamble,          type,                           0,        "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,        %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,        %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer11.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "256"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

[customer11custom.reg]
HKR, Ndi\params\bkScanEnable,           ParamDesc,                      0,        %bkScanEnable%
HKR, Ndi\params\bkScanEnable,           Base,                           0,        "10"
HKR, Ndi\params\bkScanEnable,           default,                        0,        "1"
HKR, Ndi\params\bkScanEnable,           type,                           0,        "enum"
HKR, Ndi\params\bkScanEnable\enum,      "1",                            0,        %bkScanEnableOn%
HKR, Ndi\params\bkScanEnable\enum,      "0",                            0,        %bkScanEnableOff%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,        %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,        "10"
HKR, Ndi\params\radioEnable,            default,                        0,        "1"
HKR, Ndi\params\radioEnable,            type,                           0,        "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,        %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,        %radioEnableOff%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssi11A%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

HKR, Ndi\params\roamRssiBOnly,          ParamDesc,                      0,        %roamRssi11BOnly%
HKR, Ndi\params\roamRssiBOnly,          default,                        0,        "8"
HKR, Ndi\params\roamRssiBOnly,          min,                            0,        "0"
HKR, Ndi\params\roamRssiBOnly,          max,                            0,        "95"
HKR, Ndi\params\roamRssiBOnly,          step,                           0,        "1"
HKR, Ndi\params\roamRssiBOnly,          base,                           0,        "10"
HKR, Ndi\params\roamRssiBOnly,          type,                           0,        "int"

HKR, Ndi\params\roamRssiB,              ParamDesc,                      0,        %roamRssi11B%
HKR, Ndi\params\roamRssiB,              default,                        0,        "24"
HKR, Ndi\params\roamRssiB,              min,                            0,        "0"
HKR, Ndi\params\roamRssiB,              max,                            0,        "95"
HKR, Ndi\params\roamRssiB,              step,                           0,        "1"
HKR, Ndi\params\roamRssiB,              base,                           0,        "10"
HKR, Ndi\params\roamRssiB,              type,                           0,        "int"

HKR, Ndi\params\roamRateA,              ParamDesc,                      0,        %roamRateA%
HKR, Ndi\params\roamRateA,              Base,                           0,        "10"
HKR, Ndi\params\roamRateA,              default,                        0,        "24000"
HKR, Ndi\params\roamRateA,              type,                           0,        "enum"
HKR, Ndi\params\roamRateA\enum,         "6000",                         0,        %roamRateA6M%
HKR, Ndi\params\roamRateA\enum,         "9000",                         0,        %roamRateA9M%
HKR, Ndi\params\roamRateA\enum,         "12000",                        0,        %roamRateA12M%
HKR, Ndi\params\roamRateA\enum,         "18000",                        0,        %roamRateA18M%
HKR, Ndi\params\roamRateA\enum,         "24000",                        0,        %roamRateA24M%
HKR, Ndi\params\roamRateA\enum,         "36000",                        0,        %roamRateA36M%
HKR, Ndi\params\roamRateA\enum,         "48000",                        0,        %roamRateA48M%
HKR, Ndi\params\roamRateA\enum,         "54000",                        0,        %roamRateA54M%

HKR, Ndi\params\roamRateBOnly,          ParamDesc,                      0,        %roamRateBOnly%
HKR, Ndi\params\roamRateBOnly,          Base,                           0,        "10"
HKR, Ndi\params\roamRateBOnly,          default,                        0,        "5000"
HKR, Ndi\params\roamRateBOnly,          type,                           0,        "enum"
HKR, Ndi\params\roamRateBOnly\enum,     "1000",                         0,        %roamRateBOnly1M%
HKR, Ndi\params\roamRateBOnly\enum,     "2000",                         0,        %roamRateBOnly2M%
HKR, Ndi\params\roamRateBOnly\enum,     "5000",                         0,        %roamRateBOnly5M%
HKR, Ndi\params\roamRateBOnly\enum,     "11000",                        0,        %roamRateBOnly11M%

HKR, Ndi\params\roamRateB,              ParamDesc,                      0,        %roamRateB%
HKR, Ndi\params\roamRateB,              Base,                           0,        "10"
HKR, Ndi\params\roamRateB,              default,                        0,        "9000"
HKR, Ndi\params\roamRateB,              type,                           0,        "enum"
HKR, Ndi\params\roamRateB\enum,         "1000",                         0,        %roamRateB1M%
HKR, Ndi\params\roamRateB\enum,         "2000",                         0,        %roamRateB2M%
HKR, Ndi\params\roamRateB\enum,         "5000",                         0,        %roamRateB5M%
HKR, Ndi\params\roamRateB\enum,         "6000",                         0,        %roamRateB6M%
HKR, Ndi\params\roamRateB\enum,         "9000",                         0,        %roamRateB9M%
HKR, Ndi\params\roamRateB\enum,         "11000",                        0,        %roamRateB11M%

HKR, Ndi\params\pcieAspm,               ParamDesc,                      0,        %pcieAspm%
HKR, Ndi\params\pcieAspm,               Base,                           0,        "10"
HKR, Ndi\params\pcieAspm,               default,                        0,        "0"
HKR, Ndi\params\pcieAspm,               type,                           0,        "enum"
HKR, Ndi\params\pcieAspm\enum,          "0",                            0,        %pcieAspmOff%
HKR, Ndi\params\pcieAspm\enum,          "1",                            0,        %pcieAspmL0sOn%
HKR, Ndi\params\pcieAspm\enum,          "2",                            0,        %pcieAspmL1On%
HKR, Ndi\params\pcieAspm\enum,          "3",                            0,        %pcieAspmL0sandL1On%

[customer11_11n40wmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "129055"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "26628",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "102403",                       0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "26652",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "129055",                       0,        %wModeSelect11abgn%

[customer11_11nwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "6175"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "2052",                         0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "4099",                         0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "2076",                         0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "6175",                         0,        %wModeSelect11abgn%

[customer11_legacywmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "31"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "3",                            0,        %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum,       "28",                           0,        %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum,       "31",                           0,        %wModeLegacy11abg%

[customer11Ant.reg]
HKR, Ndi\params\antennaSwitch,          ParamDesc,                      0,        %antennaSwitch%
HKR, Ndi\params\antennaSwitch,          Base,                           0,        "10"
HKR, Ndi\params\antennaSwitch,          default,                        0,        "2"
HKR, Ndi\params\antennaSwitch,          type,                           0,        "enum"
HKR, Ndi\params\antennaSwitch\enum,     "0",                            0,        %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum,     "1",                            0,        %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum,     "2",                            0,        %antennaSwitchAuto%

[customer_Samsung.reg]
HKR, Ndi\params\sleepMode,                ParamDesc,                      0,  %PowerSaveMode%
HKR, Ndi\params\sleepMode,                Base,                           0,  "10"
HKR, Ndi\params\sleepMode,                default,                        0,  "2"
HKR, Ndi\params\sleepMode,                type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,           "0",                            0,  %Off%
HKR, Ndi\params\sleepMode\enum,           "1",                            0,  %Maximum%
HKR, Ndi\params\sleepMode\enum,           "2",                            0,  %Normal%
HKR, NDI\params\ignore11dBeacon,ParamDesc,,     %802_11d%
HKR, NDI\params\ignore11dBeacon,type,,          "enum"
HKR, NDI\params\ignore11dBeacon,Default,,       "1"
HKR, NDI\params\ignore11dBeacon\enum,0,,        %Enable%
HKR, NDI\params\ignore11dBeacon\enum,1,,        %Disable%
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 

[ignore11denable.reg]
HKR, ,                                  ignore11dBeacon,                0x00002,  "1"

[xb72.via.reg]
HKLM, SYSTEM\CurrentControlSet\Services\pci\Parameters,168c0024,0x00000001, 00,00,00,20,00,00,00,00

[rssiAdjust.reg]
HKR, ,                                  rssiAdjust,                     0x00002,  "7"

[cmdRegister.reg]
HKR, ,                                  cmdRegister,                    0x00002,  "838"

[htAdhocdisable.reg]
HKR, ,                                  htAdhocEnable,                  0x00002,  "0"

[htAdhoc.reg]
HKR, NDI\params\htAdhocEnable,ParamDesc,,       %AdHoc11n%
HKR, NDI\params\htAdhocEnable,type,,            "enum"
HKR, NDI\params\htAdhocEnable,Default,,         "0"
HKR, NDI\params\htAdhocEnable\enum,0,,          %Disable%
HKR, NDI\params\htAdhocEnable\enum,1,,          %Enable%

[htWepTkipOpt.reg]
HKR, Ndi\params\htEnableWepTkip,ParamDesc,  0,  %WepTkip11n%
HKR, NDI\params\htEnableWepTkip,type,,          "enum"
HKR, NDI\params\htEnableWepTkip,Default,,       "1"
HKR, NDI\params\htEnableWepTkip\enum,0,,        %Disable%
HKR, NDI\params\htEnableWepTkip\enum,1,,        %Enable%

[htEnableWepTkip.reg]
HKR, ,                                  htEnableWepTkip,                  0x00002,  "1"

[cemspecled_func1_1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_3.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_8.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func2_1.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func2_8.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func0_1.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[d3forcel1disable.reg]
HKR, ,                                  halPcieWaen,                    0x00002,  "4212539"

[d3forcel1disable1.reg]
HKR, ,                                  halPcieWaen,                         0x00002,  "4212539"
HKR, ,                                  halPcieDetach,                    0x00002,  "1"

[maxpowersave.reg]
HKR, ,                                  sleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"

[customer_IODATA.reg]
HKR, ,                                  LinkLedFunc,                    0, "49"
HKR, ,                                  ActivityLedFunc,                0, "51"

[ledcontrol2.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"

[led_func0_4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
;HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
;HKR, ,                                  sharedGpioFunc0 ,               0x00002,  "0"
;HKR, ,                                  gpioPinFunc1,                   0x00002,  "4"
;HKR, ,                                  gpioPinFunc2,                   0x00002,  "4"

[led_func0_10.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "10"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  gpioLedCustom,                  0x00002,  "10"
HKR, ,                                  sharedGpioFunc0 ,               0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "10"
HKR, ,                                  gpioPinFunc2,                   0x00002,  "10"

[btcoex.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "1"

[janusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "1"

[janusda_coexPTA_40_21.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "21"

[heliusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btModule,                       0x00002,  "2"
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "2"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "2"

[ampDisablePolicy.reg]
HKR, ,                                  ampEnable,                      0x00002,  "0"

[merlinshiftdelay.reg]
HKR, ,                                  analogShiftRegDelay,            0x00002,  "10"

[minpower.reg]
HKR, ,                                  legacyMinTxPowerLimit,            0x00002,  "10"

[wowenable.reg]
HKR, ,                                  wowEnable,                      0x00002,  "1"

[triggerlevelkiteonly.reg]
HKR, ,                                  txTrigLevelMax ,                0x00002,  "32"

[c3war.reg]
HKR, ,                                  c3WarTimerPeriod,               0x00002,  "130"

[indicaterxlinkspeed.reg]
HKR, ,                                  indicateRxLinkSpeed ,           0x00002,  "1"

[fullhwresethb93.reg]
HKR, ,                                  halFullResetWarEnable ,         0x00002,  "0"

[sharegpio.reg]
HKR, ,                                  sharedGpioFunc0 ,               0x00002,  "1"

[rxLatencyWar.reg]
HKR, ,                                  rxLatencyWar ,                  0x00002,  "1"

[aphroditeant2.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  mciConfig,                      0x00000,  "33596642"
HKR, ,                                  btCoexLowACKPwr,                0x00000,  "2622209"
HKR, ,                                  btCoexStompA2DPCfg,             0x00000,  "24323329"
HKR, ,                                  btCoexStompSCOCfg,              0x00000,  "25502465"

[MSI.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 4

[l2devices.reg]
;HKR, Ndi,                           Service,    0, "Ak27Hx86"
;HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
;HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet"
; Force high priority Tx queue for QoS data frames
HKR, Ndi\params\ForceHighTxQ,           ParamDesc,          0,        %ForceHighTxQ%
HKR, Ndi\params\ForceHighTxQ,           Base,               0,        "10"
HKR, Ndi\params\ForceHighTxQ,           default,            0,        "0"
HKR, Ndi\params\ForceHighTxQ,           type,               0,        "enum"
HKR, Ndi\params\ForceHighTxQ\enum,      "0",                0,        %ForceHighTxQOff%
HKR, Ndi\params\ForceHighTxQ\enum,      "1",                0,        %ForceHighTxQOn%

;;  Added for Jupiter
;;
[halShortRetry.reg]
HKR, ,                                  halShortRetry,                  0x00002,  "11"

[IdleConfiguration.reg]
HKR, ,                                  IdleConfiguration,              0x00002,  "0"

[ConnectionFailure.reg]
HKR, ,                                  delayNWSleep,                   0x00002,  "1"
HKR, ,                                  swBeaconProcess,                0x00002,  "1"

;;End of Customized Section

[killer.Service]
DisplayName     = %BFOOT.Service.DispName%
ServiceType     = 1         ;SERVICE_KERNEL_DRIVER
StartType       = 3         ;SERVICE_DEMAND_START
ErrorControl    = 1         ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\akw8x86.sys
LoadOrderGroup  = NDIS


[atheros.EventLog]
AddReg = atheros.AddEventLog.reg

[atheros.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[killer.CopyFiles]
akw8x86.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%,akw8x86.sys,,

[SourceDisksFiles]
akw8x86.sys = 1,,

[DestinationDirs]
killer.CopyFiles            = 12
DefaultDestDir               = 11


[Strings]
Msft                         = "Microsoft"
Atheros                      = "Qualcomm Atheros, Inc."
ATHR.Service.DispName        = "Killer Wireless-N 1103 device driver"
BFOOT.Service.DispName       = "Killer Wireless-N 1102 LAN device driver"
DiskDescription              = "Atheros Sample Driver Disk 1"
TransmitBuffers              = "Transmit Buffers"
ReceiveBuffers               = "Receive Buffers"
NetworkAddress               = "Network Address"
scanTimeValid                = "Scan Valid Interval"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
;radioEnable                 = "Radio On/Off"
;radioEnableOn               = "On"
;radioEnableOff              = "Off"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
WirelessMode                 = "Wireless Mode Selection"
WirelessMode11bgOnly         = "802.11b/g"
WirelessModeAuto             = "Auto"
adhocchannel                 = "Adhoc channel Selection"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOn               = "On"
bkScanEnableOff              = "Off"
TransmitRateSet              = "Transmit Rate Set"
TransmitRateSetRC            = "Rate Control"
TransmitRateSet2M            = " 2Mbps"
TransmitRateSet5M            = " 5Mbps"
TransmitRateSet6M            = " 6Mbps"
TransmitRateSet9M            = " 9Mbps"
TransmitRateSet11M           = "11Mbps"
TransmitRateSet12M           = "12Mbps"
TransmitRateSet18M           = "18Mbps"
TransmitRateSet24M           = "24Mbps"
TransmitRateSet36M           = "36Mbps"
TransmitRateSet48M           = "48Mbps"
TransmitRateSet54M           = "54Mbps"
AIFS                         = "AFIS Value"
CWmin                        = "CW Minimum AIFS value"
CWmax                        = "CW Maximum AIFS value"
BackoffTheshold              = "Backoff Threshold setting"
BackoffTheshold2             = "   2 (default)"
BackoffTheshold4             = "   4"
BackoffTheshold8             = "   8"
BackoffTheshold16            = "  16"
BackoffTheshold32            = "  32"
BackoffTheshold64            = "  64"
BackoffTheshold128           = " 128"
BackoffTheshold256           = " 256"
BackoffTheshold512           = " 512"
BackoffTheshold1024          = "1024"
VirtualCollisionPolicy       = "Virtual Collision handling policy"
VirtualCollisionPolicyDefault= "Default"
VirtualCollisionPolicyIgnore = "Ignore"
ForceHighTxQ                 = "Force Tx with high priority"
ForceHighTxQOn               = "High Priority"
ForceHighTxQOff              = "Default Priority"
noackPolicy                  = "no-ACK Tx policy"
noackPolicyOn                = "Force no-ACK policy"
noackPolicyOff               = "Default ACK policy"
htBssAggrEnable              = "BSS HT frame aggregation enable"
CWbackoff                    = "Binary exponential CW backoff"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
bt30                         = "802.11 Bluetooth High Speed"
bt30enable                   = "Enable"
bt30disable                  = "Disable"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRateA                    = "roamRateA"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRateBOnly11M             = "11Mbps"
roamRateB                    = "roamRateB"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateB11M                 = "11Mbps"
pcieAspm                     = "pcieAspm"
pcieAspmOff                  = "L0s Off, L1 Off"
pcieAspmL0sOn                = "L0s On,  L1 Off"
pcieAspmL1On                 = "L0s Off, L1 On"
pcieAspmL0sandL1On           = "L0s On,  L1 On"
wModeSelect                  = "Wireless Mode"
wModeSelect11bonly           = "11b only"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11abgn            = "11abgn"
wModeLegacy11a               = "11a only"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11abg             = "11abg"
antennaSwitch                = "AntennaSwitch"
antennaSwitchAuto            = "Auto"
antennaSwitchA               = "Antenna A"
antennaSwitchB               = "Antenna B"
Auto                         = "Auto"
5GOnly                       = "5Ghz Only"
2GOnly                       = "2Ghz Only"
11DModeSwitch                = "11d Mode Switch"
Enable                       = "Enable"
Disable                      = "Disable"
WepTkip11n                   = "WepTKIP 11n"
PowerSaveMode                = "Power Save Mode"
Off                          = "Off"
Maximum                      = "Maximum"
Normal                       = "Normal"
802_11d                      = "802.11d"
smpsDynamic                  = "Dynamic MIMO Power Save"
AdHoc11n                     = "AdHoc 11n"
roamPolicy                   = "Roaming Policy"
roamPolicyVeryHigh           = "Very High"
roamPolicyHigh               = "High"
roamPolicyNormal             = "Normal"
roamPolicyLow                = "Low"
roamPolicyVeryLow            = "Very Low"
GreenTx                      = "Green Tx"
GreenTxEnableOn              = "On"
GreenTxEnableOff             = "Off"
BFOOT.DeviceDesc.3096        = "Killer Wireless-N 1102 Network Adapter"
ATHR.DeviceDesc.osprey       = "Killer Wireless-N 1103 Network Adapter"
ATHR.DeviceDesc.946x         = "Killer Wireless-N 1202 (2.4GHz and 5GHz)"
ATHR.DeviceDesc.956x         = "Qualcomm Atheros AR956x Wireless Network Adapter"


;/* Enable these if VLAN or 802.1p is to be enabled */
;PriorityVLAN                = "Priority & VLAN"
;PriorityVLANDisabled        = "Priority & VLAN Disabled"
;PriorityEnabled             = "Priority Enabled"
;VLANEnabled                 = "VLAN Enabled"
;PriorityVLANEnabled         = "Priority & VLAN Enabled"