;
; SAS2XP86.INF - version XP.1 (Windows XP)
;
; This is the INF file for Windows XP for the SAS2XP86 SAS Gen2 driver
;
; ********************************************************************
;                                                                    *
;   Copyright 2008 LSI Corporation, Inc. All rights reserved.        *
;                                                                    *
;   This file is property of LSI Corporation, Inc. and is licensed   *
;   for use as is.  The receipt of or possession of this file does   *
;   convey any rights to modify its contents, in whole, or in part,  *
;   without the specific written consent of LSI Corporation.         *
;                                                                    *
; ********************************************************************

[version]
signature="$Windows NT$"
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%LSI%
DriverVer=07/03/2012,2.00.57.01
CatalogFile.ntx86=sas2xp86.cat

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS
; LSI_EXE_CopyFiles = 11 ; %SystemDrive%\windows\system32
; LSI_CFGDEF_CopyFiles = 24, ProgramData\LSI\Wdcfg

[SourceDisksFiles.x86]
sas2xp86.sys = 1
lsinodrv.inf = 1
; wdcfg.exe = 1
; DriverConfigParam.def = 1

[SourceDisksNames]
1 = %DiskDesc%,,

[Manufacturer]
%LSI%=LSI
%DELL%=DELL
%INTEL%=INTEL


[LSI]
%DevDesc1% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0064
%DevDesc2% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0065
%DevDesc3% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0070
%DevDesc4% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0072
%DevDesc5% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0074
%DevDesc6% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0076
%DevDesc7% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0077
%DevDesc8% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0080
%DevDesc8% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0081
%DevDesc8% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0082
%DevDesc8% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0083
%DevDesc8% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0084
%DevDesc8% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0085
%DevDesc9% = SAS2XP86_Inst, PCI\VEN_1000&DEV_006E
%DevDesc9% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0086
%DevDesc9% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0087
%DevDescH1% = SAS2XP86_HP_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_3371103C

[DELL]
%DevDescD1% = SAS2XP86_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1C1028
%DevDescD2% = SAS2XP86_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1D1028
%DevDescD3% = SAS2XP86_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1E1028
%DevDescD4% = SAS2XP86_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1F1028
%DevDescD5% = SAS2XP86_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F201028
%DevDescD6% = SAS2XP86_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F211028
%DevDescD7% = SAS2XP86_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F221028

[INTEL]
%DevDescI1% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_350E8086
%DevDescI2% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_350F8086
%DevDescI3% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0087&SUBSYS_30008086
%DevDescI4% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_37008086
%DevDescI5% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0087&SUBSYS_35168086
%DevDescI6% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0087&SUBSYS_35178086
%DevDescI7% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0087&SUBSYS_35188086
%DevDescI8% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0087&SUBSYS_35198086 
%DevDescI9% = SAS2XP86_Inst, PCI\VEN_1000&DEV_0087&SUBSYS_30608086

[ControlFlags]
ExcludeFromSelect = *

[SAS2XP86_Inst]
CopyFiles = SAS2XP86_CopyFiles
; CopyFiles = LSI_EXE_CopyFiles
; CopyFiles = LSI_CFGDEF_CopyFiles
AddReg = SAS2XP86_AddReg
AddReg = LSI_WDCFG_AddReg
CopyINF = lsinodrv.inf

[SAS2XP86_Inst.HW]
AddReg = Shutdown_addreg
DelReg = LegacyScsiportValues

[SAS2XP86_Inst.Services]
AddService = SAS2XP86, %SPSVCINST_ASSOCSERVICE%, SAS2XP86_Service_Inst, Miniport_EventLog_Inst

[SAS2XP86_AddReg]
HKLM,SYSTEM\CurrentControlSet\Services\sas2xp86\Parameters\Device,DriverParameter,0x00000002,"EnablePseudoDevice=1;"
HKLM,SYSTEM\CurrentControlSet\Services\sas2xp86\Parameters\Device,MaximumSGList,0x00010001,0xFF
HKLM,SYSTEM\CurrentControlSet\Services\sas2xp86\Parameters\Device,NumberOfRequests,0x00010001,0xFF

[SAS2XP86_HP_Inst]
CopyFiles = SAS2XP86_CopyFiles
AddReg = SAS2XP86_HP_AddReg

[SAS2XP86_HP_Inst.HW]
AddReg = Shutdown_addreg
DelReg = LegacyScsiportValues

[SAS2XP86_HP_Inst.Services]
AddService = SAS2XP86, %SPSVCINST_ASSOCSERVICE%, SAS2XP86_Service_Inst, Miniport_EventLog_Inst

[SAS2XP86_HP_AddReg]
HKLM,SYSTEM\CurrentControlSet\Services\sas2xp86\Parameters\Device,DriverParameter,0x00000002,"EnablePseudoDevice=1;"
HKLM,SYSTEM\CurrentControlSet\Services\sas2xp86\Parameters\Device,MaximumSGList,0x00010001,0xFF
HKLM,SYSTEM\CurrentControlSet\Services\sas2xp86\Parameters\Device,NumberOfRequests,0x00010001,0xFF
HKLM,SYSTEM\CurrentControlSet\Services\Disk,TimeOutValue,0x00010001,0x0000003C

[SAS2XP86_Dell_Inst]
CopyFiles = SAS2XP86_CopyFiles
AddReg = SAS2XP86_Dell_AddReg

[SAS2XP86_Dell_Inst.HW]
AddReg = Shutdown_addreg
DelReg = LegacyScsiportValues

[SAS2XP86_Dell_Inst.Services]
AddService = SAS2XP86, %SPSVCINST_ASSOCSERVICE%, SAS2XP86_Service_Inst, Miniport_EventLog_Inst

[SAS2XP86_Dell_AddReg]
HKLM,SYSTEM\CurrentControlSet\Services\sas2xp86\Parameters\Device,DriverParameter,0x00000002,"EnablePseudoDevice=1;"
HKLM,SYSTEM\CurrentControlSet\Services\Disk,TimeOutValue,0x00010001,0x00000041

[LSI_WDCFG_AddReg]
HKLM,SYSTEM\CurrentControlSet\Control\Wdcfg,TargetDriver,0x00000000,"SAS2XP86"

[SAS2XP86_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\sas2xp86.sys
LoadOrderGroup = SCSI Miniport
AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type_scsi

[SAS2XP86_CopyFiles]
sas2xp86.sys,,,1

; [LSI_EXE_CopyFiles]
; wdcfg.exe,,,2

; [LSI_CFGDEF_CopyFiles]
; DriverConfigParam.def,,,2

[Shutdown_addreg]
HKR,"ScsiPort","NeedsSystemShutdownNotification",0x00010001,1

[LegacyScsiportValues]
HKR,Scsiport,BusNumber
HKR,Scsiport,LegacyInterfaceType
HKR,Scsiport,SlotNumber

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

[bus_type_scsi]
HKR, "Parameters", "BusType", 0x00010001, 0x00000001

[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7

[Strings]
LSI = "LSI Corporation"
DELL = "Dell Inc."
INTEL = "Intel Corporation"
DiskDesc = "LSI PCI Fusion-MPT SAS2 Driver Install Disk (ScsiPort)"
DevDesc1 = "LSI Adapter, SAS2 2116 Meteor ROC(E)"
DevDesc2 = "LSI Adapter, SAS2 2116 Meteor ROC"
DevDesc3 = "LSI Adapter, SAS2 2004 Spitfire"
DevDesc4 = "LSI Adapter, SAS2 2008 Falcon"
DevDesc5 = "LSI Adapter, SAS2 2108 Liberator"
DevDesc6 = "LSI Adapter, SAS2 2108 Liberator ROC(E)"
DevDesc7 = "LSI Adapter, SAS2 2108 Liberator ROC"
DevDesc8 = "LSI Adapter, SAS2 2208 Thunderbolt ROC -ScsiPort"
DevDesc9 = "LSI Adapter, SAS2 2308 Mustang -ScsiPort"
DevDescH1 = "HP SC08e 6Gb SAS HBA"
DevDescD1 = "Dell 6Gbps SAS HBA"
DevDescD2 = "Dell PERC H200 Adapter"
DevDescD3 = "Dell PERC H200 Integrated"
DevDescD4 = "Dell PERC H200 Modular"
DevDescD5 = "Dell PERC H200 Embedded"
DevDescD6 = "Dell PERC H200"
DevDescD7 = "Dell Internal Tape Adapter"
DevDescI1 = "Intel Integrated RAID Module RMS2LL080"
DevDescI2 = "Intel Integrated RAID Module RMS2LL040"
DevDescI3 = "Intel(R) RAID Controller RS25GB008"
DevDescI4 = "Intel(R) SSD 910 Series"
DevDescI5 = "Intel(R) Integrated RAID Module RMS25JB080"
DevDescI6 = "Intel(R) Integrated RAID Module RMS25JB040"
DevDescI7 = "Intel(R) Integrated RAID Module RMS25KB080"
DevDescI8 = "Intel(R) Integrated RAID Module RMS25KB040" 
DevDescI9 = "Intel(R) RAID Controller RS25FB044"

;*******************************************
;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
