; Copyright (c) 2009-2012 Intel Corporation   
; **********************************************************************************************   
; **********************************************************************************************   
; **    Filename:  iaStorB.inf  
; **    Revision:  09/03/2013,3.8.0.1108 
; **    Abstract:  Windows* INF File for AHCI Intel(R) Rapid Storage Technology Enterprise Driver   
; **               Installs: RSTe AHCI RAID Controller Miniport + RST Filter Driver   
; **********************************************************************************************   
[Version]   
Signature="$Windows NT$"   
Provider=%INTEL%   
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}   
Class=SCSIAdapter   
CatalogFile=iaStorB.cat  
DriverVer=09/03/2013,3.8.0.1108
;  
[PackageInfo]   
Name=AHCIB   
;  
[SourceDisksNames]   
1 = %DiskId1%,,,""   
[DestinationDirs]   
DefaultDestDir = 12   
;  
[ControlFlags]   
ExcludeFromSelect = *   
;  
[Manufacturer]   
%INTEL% = INTEL, NTamd64.5.2, NTamd64.6.2   
;  
[iaStorB_Service_Inst]  
ServiceType    = %SERVICE_KERNEL_DRIVER%   
StartType      = %SERVICE_BOOT_START%   
ErrorControl   = %SERVICE_ERROR_NORMAL%   
ServiceBinary  = %12%\iaStorB.sys  
LoadOrderGroup = SCSI miniport   
AddReg         = pnpsafe_pci_addreg   
;  
[iaStorB_EventLog_Inst]  
AddReg = iaStorB_EventLog_AddReg  
;  
[iaStorB_EventLog_AddReg]  
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorB.sys" 
HKR,,TypesSupported,%REG_TYPE_DWORD%,7   
;  
[iaStorF_Service_Inst]   
ServiceType    = %SERVICE_KERNEL_DRIVER%   
StartType      = %SERVICE_BOOT_START%   
ErrorControl   = %SERVICE_ERROR_NORMAL%   
ServiceBinary  = %12%\iaStorF.sys   
;  
[iaStorF_EventLog_Inst]   
AddReg = iaStorF_EventLog_AddReg   
;  
[iaStorF_EventLog_AddReg]   
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"  
HKR,,TypesSupported,%REG_TYPE_DWORD%,7   
;  
;********************************************************   
;*   
;* 64-BIT X86 ARCHITECTURE   
;*   
;* This section specifies the 64-bit architecture specific INF file entries   
;* required to install a driver as a 64-bit compatible driver.   
;*   
;******************************************************************************   
[SourceDisksFiles.amd64]    
iaStorB.sys = 1,,,   
iaStorF.sys = 1,,,    
;  
[INTEL.NTamd64.6.2]     
;windows_8_64-bit    
;      
[INTEL.NTamd64.5.2]     
;server_2003_enterprise_x64  
%PCI\VEN_8086&DEV_2827&CC_0104.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_2827&CC_0104 
;  
[iaStorB_inst.NTamd64]  
CopyFiles=@iaStorB.sys  
CopyFiles=@iaStorF.sys   
;  
[iaStorB_inst.NTamd64.HW]  
AddReg = iaStorF_addreg   
AddReg = msi_addreg   
AddReg = storport_addreg  
AddReg = sgpio_addreg  
;  
[iaStorB_inst.ntamd64.Services]  
AddService = iaStorB, %SPSVCINST_ASSOCSERVICE%, iaStorB_Service_Inst, iaStorB_EventLog_Inst  
AddService = iaStorF, , iaStorF_Service_Inst, iaStorF_EventLog_Inst   
;  
[iaStorF_addreg]   
; Layer the RST Filter driver under all Disk class devices as a lower disk class filter   
;  
HKLM, System\CurrentControlSet\Control\Class\{4d36e967-e325-11ce-bfc1-08002be10318}, LowerFilters, 0x00010008, iaStorF   
;  
[pnpsafe_pci_addreg]  
; Use raw values for BusType, not a DEFINE, ChkInf fails on hex alpha chars   
; BusType_ATA == 0x3, BusTypeATA, BusType_RAID == 0x8, BusType_SATA == 0xb   
HKR, Parameters\PnpInterface,  5,                           %REG_TYPE_DWORD%,  0x00000001   
HKR, Parameters,               BusType,                     %REG_TYPE_DWORD%,  0x00000008  
; Tell Storport in Win7/Srv08R2(KB982018) that driver can report 4K sector size (not needed in Win8)  
HKR, Parameters\Device,        EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001  
;  
[DefaultInstall] 
OptionDesc = %ServiceDescription% 
CopyINF = iaStorB.inf 
; 
[DefaultInstall.Services] 
AddService = iaStorB, %SPSVCINST_ASSOCSERVICE%, iaStorB_Service_Inst, iaStorB_EventLog_Inst  
AddService = iaStorF, , iaStorF_Service_Inst, iaStorF_EventLog_Inst  
; 
[Strings]   
; Localizable Strings   
;  
diskId1 = "RSTe Installation Disk"   
;server  
PCI\VEN_8086&DEV_2827&CC_0104.DeviceDesc = "Intel(R) C600+/C220+ series chipset sSATA RAID Controller" 
;  
INTEL = "Intel Corporation"   
ServiceDescription = "Intel(R) C600+/C220+ series chipset sSATA RAID Controller Driver" 
;  
; Non-Localizable Strings   
;  
SPSVCINST_ASSOCSERVICE = 0x00000002   
REG_MULTI_SZ           = 0x00010000   
REG_EXPAND_SZ          = 0x00020000   
REG_TYPE_DWORD         = 0x00010001   
SERVICE_KERNEL_DRIVER  = 1   
SERVICE_BOOT_START     = 0   
SERVICE_ERROR_NORMAL   = 1  
;  
; MSI enables.   
;  
[msi_addreg]    
HKR, Interrupt Management, 0x00000010    
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010    
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_TYPE_DWORD%,   1    
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_TYPE_DWORD%,   1   
;  
[storport_addreg]  
;;; Enables/Disables Idle Power Management for StorPort  
HKR, "StorPort", "EnableIdlePowerManagement", %REG_TYPE_DWORD%, 0x00000000  
;;; Force StorPort to keep all sense data in Pre-Win8 OSes (max value is 255)  
HKR, StorPort, TotalSenseDataBytes, %REG_TYPE_DWORD%, 0x000000FF  
;  
[sgpio_addreg]  
;;; Enable/disable SGPIO support  
HKLM, System\CurrentControlSet\Services\iaStorB\Parameters\Device, LED_Supported, %REG_TYPE_DWORD%, 0x00000001 
; 
