; Copyright (c) 2009-2012 Intel Corporation  
; **********************************************************************************************  
; **********************************************************************************************  
; **    Filename:  iaStorS.inf  
; **    Revision:  08/14/2013,3.8.0.1106 
; **    Abstract:  Windows* INF File for SCU Intel(R) Rapid Storage Technology Enterprise Driver  
; **               Installs: RSTe SCU RAID Controller Miniport (without RST Filter Driver)  
; **               Only for Windows 8 releases  
; **********************************************************************************************  
;  
[Version]  
Signature = "$Windows NT$"  
Class=SCSIAdapter  
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}  
Provider=%INTEL%  
CatalogFile=iaStorS.cat  
DriverVer=08/14/2013,3.8.0.1106
;  
[PackageInfo]  
Name=SCU  
;  
[SourceDisksNames]  
1 = %DiskId1%,,,""  
;  
[DestinationDirs]  
DefaultDestDir = 12  
;  
[ControlFlags]  
ExcludeFromSelect = *  
;  
[Manufacturer]  
%INTEL% = INTEL, NTx86.6.2 
;  
[Intel_SCU_iaStorS_Service_Inst]  
ServiceType    = %SERVICE_KERNEL_DRIVER%  
StartType      = %SERVICE_BOOT_START%  
ErrorControl   = %SERVICE_ERROR_NORMAL%  
ServiceBinary  = %12%\iaStorS.sys  
LoadOrderGroup = SCSI Miniport  
AddReg         = pnpsafe_pci_addreg  
AddReg         = UserParameters  
;AddReg         = msienable_addreg  
;  
[Intel_SCU_EventLog_Inst]  
AddReg = Intel_SCU_EventLog_Inst.AddReg  
;  
[Intel_SCU_EventLog_Inst.AddReg]  
HKR,,EventMessageFile,%REG_TYPE_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorS.sys"  
HKR,,TypesSupported,%REG_TYPE_DWORD%,7  
;  
;******************************************************************************  
;*  
;* 32-BIT X86 ARCHITECTURE  
;*  
;* This section specifies the 32-bit architecture specific INF file entries  
;* required to install a driver as a 32-bit compatible driver.  
;*  
;******************************************************************************  
[SourceDisksFiles.x86]  
iaStorS.sys = 1,,,  
;  
[INTEL.NTx86.6.2]  
;windows_8_32-bit  
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D60  
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D61  
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D64  
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D65  
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D68  
%Intel_SAS_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D69  
%Intel_SATA_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D6A  
%Intel_SATA_RAID.Desc% = Intel_SCU_iaStorS_Inst,PCI\VEN_8086&DEV_1D6B  
;  
[Intel_SCU_iaStorS_Inst.NTx86]  
CopyFiles = @iaStorS.sys  
;  
[Intel_SCU_iaStorS_Inst.NTx86.HW]  
AddReg = msienable_addreg  
Include = machine.inf  
Needs = PciIoSpaceNotRequired  
;  
[Intel_SCU_iaStorS_Inst.NTx86.Services]  
AddService = iaStorS,%SPSVCINST_ASSOCSERVICE%,Intel_SCU_iaStorS_Service_Inst, Intel_SCU_EventLog_Inst  
; 
;******************************************************************************  
;*  
;* PLUG-N-PLAY REGISTRY CHANGES  
;*  
;* This section specifies the registry entries necessary to indicate support  
;* for Plug-n-Play.  
;*  
;******************************************************************************  
[pnpsafe_pci_addreg]  
HKR, Parameters\PnpInterface,  5,                           %REG_TYPE_DWORD%,  0x00000001  
;  
; BusType 0xA == BusTypeSas (winioctl.h)  
; PCI subclass code indicates SAS (not RAID), so for WHQL, the BusType  
;  needs to match  
HKR, Parameters,               BusType,                     %REG_TYPE_DWORD%,  0x0000000A  
HKR, Parameters\Device,        EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001  
;******************************************************************************  
;*  
;* MSI/MSI-X REGISTRY CHANGES  
;*  
;* This section specifies the registry entries necessary in order to indicate  
;* this driver supports MSI-X.  
;*  
;******************************************************************************  
[msienable_addreg]  
;;;  Indicate we support MSIx up to 2 message vectors  
;HKR, Interrupt Management,                                    ,                   %REG_TYPE_KEY_ONLY%  
HKR, Interrupt Management, 0x00000010  
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010  
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_TYPE_DWORD%,   1  
;******************************************************************************  
;*  
;* USER PARAMETER REGISTRY CHANGES  
;*  
;* This section specifies the parameters that users can modify in the  
;* registry that will change the operation of the driver after a power  
;* cycle of the system or a reinstall of the driver.  
;*  
;******************************************************************************  
[UserParameters]  
;;; Build the Registry Directories  
HKR, Parameters, Device, %REG_TYPE_KEY_ONLY%  
;  
;;; Add the RAID features  
HKR, Parameters\Device, ReadPatrol,                               %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, RebuildOnHotInsert,                       %REG_TYPE_BINARY%,     0x00000000  
;  
;;; Add the Controller wide user parameters  
HKR, Parameters\Device, ControllerDeviceSpinUpDelayInterval,      %REG_TYPE_DWORD%,      0x000001F4  
HKR, Parameters\Device, ControllerInterruptCoalescenceNumber,     %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, ControllerInterruptCoalescenceTimer,      %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, ControllerSataNcqEnable,                  %REG_TYPE_DWORD%,      0x00000001  
HKR, Parameters\Device, ControllerSataNcqDepthMaximum,            %REG_TYPE_DWORD%,      0x00000020  
HKR, Parameters\Device, ControllerSataStandbyTimerEnable,         %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, ControllerSataNonZeroBufferOffsetEnable,  %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, ControllerInitialResetType,               %REG_TYPE_DWORD%,      0x00000008  
HKR, Parameters\Device, ControllerClearAffiliationEnable,         %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, StpInactivityTimeout,                     %REG_TYPE_DWORD%,      0x00000005  
HKR, Parameters\Device, SspInactivityTimeout,                     %REG_TYPE_DWORD%,      0x00000005  
HKR, Parameters\Device, StpMaxOccupancyTimeout,                   %REG_TYPE_DWORD%,      0x00000005  
HKR, Parameters\Device, SspMaxOccupancyTimeout,                   %REG_TYPE_DWORD%,      0x00000014  
HKR, Parameters\Device, NoOutBoundTaskTimeout,                    %REG_TYPE_DWORD%,      0x00000002  
HKR, Parameters\Device, IgnoreFUA,                                %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, PerformanceOptimizationsEnable,           %REG_TYPE_DWORD%,      0x00000000  
;  
HKR, Parameters\Device, InterruptCoalescingSampleSize,      %REG_TYPE_DWORD%,      0x0000000a  
HKR, Parameters\Device, InterruptCoalescingSampleFrequency, %REG_TYPE_DWORD%,      0x00000064  
HKR, Parameters\Device, InterruptCoalescingThreshold,       %REG_TYPE_DWORD%,      0x00002800  
HKR, Parameters\Device, InterruptCoalescingLowNumber,       %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, InterruptCoalescingLowTimeout,      %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, InterruptCoalescingHighNumber,      %REG_TYPE_DWORD%,      0x00000010  
HKR, Parameters\Device, InterruptCoalescingHighTimeout,     %REG_TYPE_DWORD%,      0x00000002  
;  
;;; Add the Phy specific user parameters  
HKR, Parameters\Device, Phy0NotifyEnableSpinupInsertionFrequency, %REG_TYPE_DWORD%,      0x00000033  
HKR, Parameters\Device, Phy0AlignInsertionFrequency,              %REG_TYPE_DWORD%,      0x0000007f  
HKR, Parameters\Device, Phy0InConnectionAlignInsertionFrequency,  %REG_TYPE_DWORD%,      0x000000ff  
HKR, Parameters\Device, Phy1NotifyEnableSpinupInsertionFrequency, %REG_TYPE_DWORD%,      0x00000033  
HKR, Parameters\Device, Phy1AlignInsertionFrequency,              %REG_TYPE_DWORD%,      0x0000007f  
HKR, Parameters\Device, Phy1InConnectionAlignInsertionFrequency,  %REG_TYPE_DWORD%,      0x000000ff  
HKR, Parameters\Device, Phy2NotifyEnableSpinupInsertionFrequency, %REG_TYPE_DWORD%,      0x00000033  
HKR, Parameters\Device, Phy2AlignInsertionFrequency,              %REG_TYPE_DWORD%,      0x0000007f  
HKR, Parameters\Device, Phy2InConnectionAlignInsertionFrequency,  %REG_TYPE_DWORD%,      0x000000ff  
HKR, Parameters\Device, Phy3NotifyEnableSpinupInsertionFrequency, %REG_TYPE_DWORD%,      0x00000033  
HKR, Parameters\Device, Phy3AlignInsertionFrequency,              %REG_TYPE_DWORD%,      0x0000007f  
HKR, Parameters\Device, Phy3InConnectionAlignInsertionFrequency,  %REG_TYPE_DWORD%,      0x000000ff  
HKR, Parameters\Device, Controller0Phy0MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002  
HKR, Parameters\Device, Controller0Phy1MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002  
HKR, Parameters\Device, Controller0Phy2MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002  
HKR, Parameters\Device, Controller0Phy3MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002  
HKR, Parameters\Device, Controller1Phy0MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002  
HKR, Parameters\Device, Controller1Phy1MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002  
HKR, Parameters\Device, Controller1Phy2MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002  
HKR, Parameters\Device, Controller1Phy3MaxSpeedGeneration,        %REG_TYPE_DWORD%,      0x00000002  
;  
;;; Add the Port specific OEM parameters  
HKR, Parameters\Device, OemHeaderVersion,                         %REG_TYPE_DWORD%,      0x00000010  
HKR, Parameters\Device, Controller0OemModeType,                   %REG_TYPE_DWORD%,      0x00000001  
HKR, Parameters\Device, Controller0OemConcurrentDeviceSpinUpCount,%REG_TYPE_DWORD%,      0x00000001  
HKR, Parameters\Device, Controller0OemSscEnable,                  %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller0OemPort0PhyMask,               %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller0OemPort1PhyMask,               %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller0OemPort2PhyMask,               %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller0OemPort3PhyMask,               %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller0OemPhy0SasAddressLow,          %REG_TYPE_DWORD%,      0x00000001  
HKR, Parameters\Device, Controller0OemPhy0SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF  
HKR, Parameters\Device, Controller0OemPhy1SasAddressLow,          %REG_TYPE_DWORD%,      0x00000001  
HKR, Parameters\Device, Controller0OemPhy1SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF  
HKR, Parameters\Device, Controller0OemPhy2SasAddressLow,          %REG_TYPE_DWORD%,      0x00000001  
HKR, Parameters\Device, Controller0OemPhy2SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF  
HKR, Parameters\Device, Controller0OemPhy3SasAddressLow,          %REG_TYPE_DWORD%,      0x00000001  
HKR, Parameters\Device, Controller0OemPhy3SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF  
HKR, Parameters\Device, Controller0OemPhy0AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08  
HKR, Parameters\Device, Controller0OemPhy0AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069  
HKR, Parameters\Device, Controller0OemPhy0AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09  
HKR, Parameters\Device, Controller0OemPhy0AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E  
HKR, Parameters\Device, Controller0OemPhy1AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08  
HKR, Parameters\Device, Controller0OemPhy1AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069  
HKR, Parameters\Device, Controller0OemPhy1AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09  
HKR, Parameters\Device, Controller0OemPhy1AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E  
HKR, Parameters\Device, Controller0OemPhy2AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08  
HKR, Parameters\Device, Controller0OemPhy2AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069  
HKR, Parameters\Device, Controller0OemPhy2AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09  
HKR, Parameters\Device, Controller0OemPhy2AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E  
HKR, Parameters\Device, Controller0OemPhy3AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08  
HKR, Parameters\Device, Controller0OemPhy3AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069  
HKR, Parameters\Device, Controller0OemPhy3AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09  
HKR, Parameters\Device, Controller0OemPhy3AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E  
;  
HKR, Parameters\Device, Controller1OemModeType,                   %REG_TYPE_DWORD%,      0x00000001  
HKR, Parameters\Device, Controller1OemConcurrentDeviceSpinUpCount,%REG_TYPE_DWORD%,      0x00000001  
HKR, Parameters\Device, Controller1OemSscEnable,                  %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller1OemPort0PhyMask,               %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller1OemPort1PhyMask,               %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller1OemPort2PhyMask,               %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller1OemPort3PhyMask,               %REG_TYPE_DWORD%,      0x00000000  
HKR, Parameters\Device, Controller1OemPhy0SasAddressLow,          %REG_TYPE_DWORD%,      0x00000004  
HKR, Parameters\Device, Controller1OemPhy0SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF  
HKR, Parameters\Device, Controller1OemPhy1SasAddressLow,          %REG_TYPE_DWORD%,      0x00000004  
HKR, Parameters\Device, Controller1OemPhy1SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF  
HKR, Parameters\Device, Controller1OemPhy2SasAddressLow,          %REG_TYPE_DWORD%,      0x00000004  
HKR, Parameters\Device, Controller1OemPhy2SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF  
HKR, Parameters\Device, Controller1OemPhy3SasAddressLow,          %REG_TYPE_DWORD%,      0x00000004  
HKR, Parameters\Device, Controller1OemPhy3SasAddressHigh,         %REG_TYPE_DWORD%,      0x5FCFFFFF  
HKR, Parameters\Device, Controller1OemPhy0AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08  
HKR, Parameters\Device, Controller1OemPhy0AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069  
HKR, Parameters\Device, Controller1OemPhy0AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09  
HKR, Parameters\Device, Controller1OemPhy0AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E  
HKR, Parameters\Device, Controller1OemPhy1AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08  
HKR, Parameters\Device, Controller1OemPhy1AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069  
HKR, Parameters\Device, Controller1OemPhy1AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09  
HKR, Parameters\Device, Controller1OemPhy1AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E  
HKR, Parameters\Device, Controller1OemPhy2AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08  
HKR, Parameters\Device, Controller1OemPhy2AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069  
HKR, Parameters\Device, Controller1OemPhy2AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09  
HKR, Parameters\Device, Controller1OemPhy2AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E  
HKR, Parameters\Device, Controller1OemPhy3AfeTxAmpControl0,       %REG_TYPE_DWORD%,      0x000BDD08  
HKR, Parameters\Device, Controller1OemPhy3AfeTxAmpControl1,       %REG_TYPE_DWORD%,      0x000B7069  
HKR, Parameters\Device, Controller1OemPhy3AfeTxAmpControl2,       %REG_TYPE_DWORD%,      0x000B7C09  
HKR, Parameters\Device, Controller1OemPhy3AfeTxAmpControl3,       %REG_TYPE_DWORD%,      0x000AFC6E  
HKR, Parameters\Device, BackplaneIsPassive,                       %REG_TYPE_DWORD%,      0x00000000  
;******************************************************************************  
;*  
;* INF FILE STRINGS (VARIABLES)  
;*  
;* This section specifies variables that can be reused elsewhere in this  
;* INF file.  
;*  
;******************************************************************************  
[Strings]  
;;;  *******Localizable Strings*******  
diskId1                = "iaStorS Installation Disk"  
Intel_SAS_RAID.Desc    = "Intel(R) C600 Series Chipset SAS RAID Controller"  
Intel_SATA_RAID.Desc   = "Intel(R) C600 Series Chipset SAS RAID (SATA mode)"  
INTEL = "Intel Corporation"  
;  
;;;  *******Non Localizable Strings*******  
SERVICE_BOOT_START     = 0x0  
SERVICE_SYSTEM_START   = 0x1  
SERVICE_AUTO_START     = 0x2  
SERVICE_DEMAND_START   = 0x3  
SERVICE_DISABLED       = 0x4  
SERVICE_KERNEL_DRIVER  = 0x1  
;  
SERVICE_ERROR_IGNORE   = 0x0  
SERVICE_ERROR_NORMAL   = 0x1  
SERVICE_ERROR_SEVERE   = 0x2  
SERVICE_ERROR_CRITICAL = 0x3  
;  
REG_TYPE_BINARY    = 0x00000001  
REG_TYPE_KEY_ONLY  = 0x00000010  
REG_TYPE_DWORD     = 0x00010001  
REG_TYPE_EXPAND_SZ = 0x00020000  
;  
SPSVCINST_ASSOCSERVICE = 0x00000002  
