;/*++
;
;Copyright (c) Broadcom Corporation.  All rights reserved.
;
;Module Name:
;
;    CVUSBDRV.INF
;
;Abstract:
;    Installation inf for Dell ControlVault USB Driver
;
;--*/

[Version]
DriverPackageType=PlugAndPlay
Signature="$WINDOWS NT$"
Class=CVAULT
ClassGuid={09E9A11D-CCB2-45ae-9BE8-65C263E60490}
Provider=%ProviderName%
DriverVer=08/27/2013,6.1.7600.16385
CatalogFile=CVAULT.cat


; ================= Class section =====================

[ClassInstall32]
Addreg=CvaultClassReg     

[CvaultClassReg]
HKR,,ClassDesc,,%CVaultClassName% 
HKR,,Icon,,-5


; ================= Device section =====================

[Manufacturer]
%MfgName%=Dell,NTAMD64

; For Win2K
[Dell]
%USB\VID_0A5C&PID_0000.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_0000
%USB\VID_0A5C&PID_0000.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_0000&REV_0101
%USB\VID_0A5C&PID_5800.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5800&REV_0101&MI_00
%USB\VID_0A5C&PID_5800.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5800&REV_0102
%USB\VID_0A5C&PID_5800.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5800&REV_0102&MI_00
%USB\VID_0A5C&PID_5801.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5801&REV_0101&MI_00
%USB\VID_0A5C&PID_5801.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5801&REV_0102
%USB\VID_0A5C&PID_5801.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5801&REV_0102&MI_00
%USB\VID_0A5C&PID_5802.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5802&REV_0101&MI_00
%USB\VID_0A5C&PID_5802.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5802&REV_0102
%USB\VID_0A5C&PID_5802.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5802&REV_0102&MI_00
%USB\VID_0A5C&PID_5803.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5803&REV_0101&MI_01
%USB\VID_0A5C&PID_5804.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5804&REV_0101&MI_00
%USB\VID_0A5C&PID_5804.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5804&REV_0102
%USB\VID_0A5C&PID_5804.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5804&REV_0102&MI_00
%USB\VID_0A5C&PID_5805.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5805&REV_0101&MI_00
%USB\VID_0A5C&PID_5805.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5805&REV_0102
%USB\VID_0A5C&PID_5805.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5805&REV_0102&MI_00
%USB\VID_0A5C&PID_5810.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5810
%USB\VID_0A5C&PID_5810.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5810&REV_0101


; For XP and later
[Dell.NTAMD64]
%USB\VID_0A5C&PID_0000.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_0000
%USB\VID_0A5C&PID_0000.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_0000&REV_0101
%USB\VID_0A5C&PID_5800.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5800&REV_0101&MI_00
%USB\VID_0A5C&PID_5800.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5800&REV_0102
%USB\VID_0A5C&PID_5800.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5800&REV_0102&MI_00
%USB\VID_0A5C&PID_5801.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5801&REV_0101&MI_00
%USB\VID_0A5C&PID_5801.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5801&REV_0102
%USB\VID_0A5C&PID_5801.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5801&REV_0102&MI_00
%USB\VID_0A5C&PID_5802.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5802&REV_0101&MI_00
%USB\VID_0A5C&PID_5802.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5802&REV_0102
%USB\VID_0A5C&PID_5802.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5802&REV_0102&MI_00
%USB\VID_0A5C&PID_5803.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5803&REV_0101&MI_01
%USB\VID_0A5C&PID_5804.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5804&REV_0101&MI_00
%USB\VID_0A5C&PID_5804.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5804&REV_0102
%USB\VID_0A5C&PID_5804.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5804&REV_0102&MI_00
%USB\VID_0A5C&PID_5805.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5805&REV_0101&MI_00
%USB\VID_0A5C&PID_5805.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5805&REV_0102
%USB\VID_0A5C&PID_5805.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5805&REV_0102&MI_00
%USB\VID_0A5C&PID_5810.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5810
%USB\VID_0A5C&PID_5810.DeviceDesc%=cvusbdrv.Dev, USB\VID_0A5C&PID_5810&REV_0101


[cvusbdrv.Dev.NT]
CopyFiles=cvusbdrv.Files.Ext


;[Switch.Dev.NT]
;;dummy section

;[Switch.Dev.NT.Services]
;AddService = , %SPSVCINST_ASSOCSERVICE%, 

[cvusbdrv.Dev.NT.Services]
Addservice = cvusbdrv, 2, cvusbdrv.AddService

[cvusbdrv.AddService]
DisplayName    = %cvusbdrv.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\cvusbdrv.sys
AddReg         = cvusbdrv.AddReg
LoadOrderGroup = Base

[cvusbdrv.AddReg]
HKR, Parameters\Wdf, VerboseOn,       0x00010001, 1
HKR, Parameters\Wdf, VerifierOn,      0x00010001, 1
HKR, Parameters\Wdf, DbgBreakOnError, 0x00010001, 1

[cvusbdrv.Files.Ext]
cvusbdrv.sys

[SourceDisksNames]
1=%Disk_Description%,,,

[SourceDisksFiles]
cvusbdrv.sys = 1
WdfCoInstaller01009.dll=1 ; make sure the number matches with SourceDisksNames

[DestinationDirs]
DefaultDestDir = 12
CoInstaller_CopyFiles = 11

;-------------- WDF Coinstaller installation

[cvusbdrv.Dev.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
WdfCoInstaller01009.dll

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"

[cvusbdrv.Dev.NT.Wdf]
KmdfService = cvusbdrv, cvusbdrv_wdfsect
[cvusbdrv_wdfsect]
KmdfLibraryVersion = 1.9

;---------------------------------------------------------------;

[Strings]
ProviderName="Dell"
MfgName="Dell"
Disk_Description="Dell ControlVault(cvusbdrv) Installation Disk"
USB\VID_0A5C&PID_0000.DeviceDesc="Dell ControlVault"
USB\VID_0A5C&PID_5800.DeviceDesc="Dell ControlVault w/o Fingerprint Sensor"
USB\VID_0A5C&PID_5801.DeviceDesc="Dell ControlVault w/ Fingerprint Swipe Sensor"
USB\VID_0A5C&PID_5802.DeviceDesc="Dell ControlVault w/ Fingerprint Touch Sensor"
USB\VID_0A5C&PID_5803.DeviceDesc="Dell ControlVault w/ Secure Keyboard"
USB\VID_0A5C&PID_5804.DeviceDesc="Dell ControlVault w/ Fingerprint Swipe Sensor"
USB\VID_0A5C&PID_5805.DeviceDesc="Dell ControlVault w/ Fingerprint Touch Sensor"
USB\VID_0A5C&PID_5810.DeviceDesc="Dell ControlVault 2"
cvusbdrv.SvcDesc="Dell ControlVault"
CVaultClassName="ControlVault Device"

