; wacom2fgt.inf
;
; inf for enabling selective suspend on HID-only units
;
; (c) Copyright 2011 Wacom Technology
;


[Version]
signature = "$Windows NT$"
Class=HIDClass
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
Provider=%Wacom%
CatalogFile=wacom2fgt.cat
DriverVer=04/11/2013,7.0.3.1

[Manufacturer]
%Wacom%=Wacom, NTamd64

[Wacom]
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_0090
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_0093&MI_01
"Wacom Touch" 				= WHF_Install, USB\VID_056A&PID_0093&MI_00
"Wacom Gesture Touch" 	= WHF_Install, USB\VID_056A&PID_00E2
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00E3&MI_01
"Wacom Gesture Touch" 	= WHF_Install, USB\VID_056A&PID_00E3&MI_00
"Wacom Gesture Touch" 	= WHF_Install, USB\VID_056A&PID_00E4
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_00E5
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00E6&MI_01
"Wacom Gesture Touch" 	= WHF_Install, USB\VID_056A&PID_00E6&MI_00
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00EC
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00ED&MI_00
"Wacom Touch" 				= WHF_Install, USB\VID_056A&PID_00ED&MI_01
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00EF
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_0100
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_0101&MI_00
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_0101&MI_01
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_010D&MI_00
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_010D&MI_01
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_0117&MI_00
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_0117&MI_01
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_0118

[Wacom.NTamd64]
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_0090
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_0093&MI_01
"Wacom Touch" 				= WHF_Install, USB\VID_056A&PID_0093&MI_00
"Wacom Gesture Touch" 	= WHF_Install, USB\VID_056A&PID_00E2
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00E3&MI_01
"Wacom Gesture Touch" 	= WHF_Install, USB\VID_056A&PID_00E3&MI_00
"Wacom Gesture Touch" 	= WHF_Install, USB\VID_056A&PID_00E4
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_00E5
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00E6&MI_01
"Wacom Gesture Touch" 	= WHF_Install, USB\VID_056A&PID_00E6&MI_00
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00EC
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00ED&MI_00
"Wacom Touch" 				= WHF_Install, USB\VID_056A&PID_00ED&MI_01
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_00EF
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_0100
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_0101&MI_00
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_0101&MI_01
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_010D&MI_00
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_010D&MI_01
"Wacom Pen" 				= WHF_Install, USB\VID_056A&PID_0117&MI_00
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_0117&MI_01
"Wacom MultiTouch" 		= WHF_Install, USB\VID_056A&PID_0118

[WHF_Install.NT]
Include=input.inf
Needs=HID_SelSus_Inst.NT

[WHF_Install.NT.HW]
Include=input.inf
Needs=HID_SelSus_Inst.NT.HW

[WHF_Install.NT.Services]
Include=input.inf
Needs=HID_SelSus_Inst.NT.Services

[Strings]
Wacom = "Wacom"
