[Version]
Signature=$Windows NT$
Class=HIDClass
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
Provider=%MFGNAME%
LayoutFile=layout.inf
CatalogFile=waltop.cat
DriverVer=08/28/2009,6.1.7600.16385

[DestinationDirs]
DefaultDestDir = 12 
System32Dir    = 11
WindowsDir     = 10

[Manufacturer]
%MFGNAME%=Tablet_Section,NTamd64

[Tablet_Section.NTamd64]
%Product%=acpiinst	,ACPI\AIP1040
%Product%=serinst	,SERENUM\AIP1040

[serinst]
CopyFiles=Tablet.CopyFiles
AddReg=Tablet.AddReg

[serinst.Services]
AddService = Tablet, 0x00000002, tablet_Service_Inst, tablet_EventLog_Inst


[serinst.HW]
AddReg = serinst.HW.AddReg

[serinst.HW.AddReg]


[acpiinst]
CopyFiles=tablet.CopyFiles
AddReg=Tablet.AddReg

[acpiinst.Services]
AddService = Tablet, 0x00000002, tablet_Service_Inst, tablet_EventLog_Inst

AddService = serial,           , SerialServiceInst, SerialEventLogInst

[acpiinst.HW]
AddReg = acpiinst.HW.AddReg

[acpiinst.HW.AddReg]

HKR,,"LowerFilters",0x00010000,"serial"
HKR,,"MultiportDevice",0x00010001,0
HKR,,"SerialRelinquishPowerPolicy",0x00010001,1


[Tablet.CopyFiles]
waltoppen.sys


[Tablet.AddReg]
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Run,"TabletPC Utility",,wisptis.exe









; -------------- Pointer Port Driver install sections ------------------------------------------
[tablet_Service_Inst]
DisplayName    = "Tablet Serial Driver"
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; 
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\waltoppen.sys
LoadOrderGroup = Pointer Port

[tablet_EventLog_Inst]
AddReg = tablet_EventLog_AddReg

[tablet_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\waltoppen.sys"
HKR,,TypesSupported,0x00010001,7
; -------------- Pointer Port Driver install sections End ------------------------------------------
[tbfilter_Service_Inst]
DisplayName    = "Tablet HID Driver"
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\waltoppen.sys
LoadOrderGroup = Extended Base

; -------------- Serial Port Driver install sections ------------------------------------------
[SerialServiceInst]
DisplayName    = %Serial.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_SYSTEM_START (this driver may do detection)
ErrorControl   = 0               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\serial.sys
LoadOrderGroup = Extended base

[SerialEventLogInst]
AddReg         = SerialEventLogAddReg

[SerialEventLogAddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\serial.sys"
HKR,,TypesSupported,0x00010001,7
; -------------- Serial Port Driver install sections End ------------------------------------------











[SourceDisksNames]
0=%DiskName%

[SourceDisksFiles]
waltoppen.sys=0,,  

[Strings]
MFGNAME="WALTOP International Corp."
Product="Serial Pen Pad"
DiskName="Pen Pad Install Disk"
Serial.SVCDESC="Serial Port Driver"