; Windows Modem Setup File
; Copyright 1997 Microsoft Corp.
; Manufacturer: ZyXEL Communications Corp.

[Version]
; created on 11/18/1998 by Manfred Recla <support@zyxel.co.at>
; for ZyXEL Comet 3356 Modem(K.56)+Fax+Voice, 1.009-K56_DSL
; using the Rockwell chipset: 'RCVDL56ACF/SVD' (chip code: R6762-27)
; with enhanced voice support for Windows98 and WindowsNT 5.0 Beta 2
; based on MS-MDK v1.47 (MDK147.DOC & REG147.DOC, October 1998)

Signature="$CHICAGO$"
Class=Modem
Provider=%Mfg%
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
;LayoutFile=layout.inf

[Strings]
Mfg        = "ZyXEL Communications Corp."
ZC56K      = "ZyXEL Comet 3356 Modem(K.56)+Fax+Voice"
ZC56K.PnP  = "ZyXEL Comet 3356 Modem(K.56)+Fax+Voice, Plug&Play"

[ZC56K.NoResDup]
UNIMODEME5F844FE

[ControlFlags]
ExcludeFromSelect=SERENUM\AKY1007

[Manufacturer]
%Mfg% = ZyXEL

[ZyXEL]
%ZC56K%     = ZC56K, UNIMODEME5F844FE ; EWS-04 CE (ZYL) 10/16/1997
%ZC56K.PnP% = ZC56K, SERENUM\AKY1007

[ZC56K]
AddReg=AllMfg.AddReg, ZC56K.Data, ZC56K.Voice, ZC56K.Fax, K56, EXTERNAL

[K56]
HKR, K56mode,  1,,"AT+MS=56,1,32000,56000,1<cr>"

[ZC56K.Data]
HKR,,Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, 7f,07,00,00, 00,c2,01,00, c0,da,00,00
HKR,, DCB,       1, 1c,00,00,00, 00,c2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,, Default,   1, 3c,00,00,00,00,00,00,00, 01,00,00,00,01,00,00,00, 53,03,00,00
HKR, Settings, Blind_Off,,                                 "X4"
HKR, Settings, Blind_On,,                                  "X3"
HKR, Settings, CallSetupFailTimer,,                        "S7=<#>"
HKR, Settings, Compression_Off,,                           "%%C0"
HKR, Settings, Compression_On,,                            "%%C3"
HKR, Settings, DialPrefix,,                                "D"
HKR, Settings, DialSuffix,,                                ""
HKR, Settings, ErrorControl_Off,,                          "&Q6\N0"
HKR, Settings, ErrorControl_On,,                           "&Q5\N3"
HKR, Settings, ErrorControl_Forced,,                       "&Q5\N2"
HKR, Settings, ErrorControl_Cellular,,                     "\N3\X0&Q5-K1*H1)M1-C1-Q0"
HKR, Settings, ErrorControl_Cellular_Forced,,              "\N4\X0&Q5-K1*H1)M1-C1-Q0"
HKR, Settings, FlowControl_Off,,                           "&K0"
HKR, Settings, FlowControl_Hard,,                          "&K3"
HKR, Settings, FlowControl_Soft,,                          "&K4"
HKR, Settings, InactivityTimeout,,                         "S30=<#>"
HKR, Settings, Modulation_CCITT,,                          "B0"
HKR, Settings, Modulation_CCITT_V23,,                      "+MS=3"
HKR, Settings, Modulation_Bell,,                           "B1"
HKR, Settings, Prefix,,                                    "AT"
HKR, Settings, Pulse,,                                     "P"
HKR, Settings, SpeakerVolume_Low,,                         "L1"
HKR, Settings, SpeakerVolume_Med,,                         "L2"
HKR, Settings, SpeakerVolume_High,,                        "L3"
HKR, Settings, SpeakerMode_Off,,                           "M0"
HKR, Settings, SpeakerMode_Dial,,                          "M1"
HKR, Settings, SpeakerMode_On,,                            "M2"
HKR, Settings, SpeakerMode_Setup,,                         "M3"
;HKR, Settings, SpeedNegotiation_Off,,                     "N0"
;HKR, Settings, SpeedNegotiation_On,,                      "N1"
HKR, Settings, Terminator,,                                "<cr>"
HKR, Settings, Tone,,                                      "T"

[ZC56K.Fax]
HKR, Fax\Class1\AdaptiveAnswer,SetupCommand,,              "AT+FAE=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand,              1,, "AT&FE0V1Q0S95=46S0=0"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand,              2,, "ATS7=60S30=0L0M1&Q5\N3%C3&K3B0N1X4"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand,              3,, "AT+FAE=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand,              4,, "ATA"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseFaxDetect,,    "FAX"
HKR, Fax\Class1\AdaptiveAnswer,SerialSpeedFaxDetect,,      "19200"
HKR, Fax\Class1\AdaptiveAnswer,HostCommandFaxDetect,,      "ATO"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseFaxConnect,,   "CONNECT"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseDataDetect,,   "DATA"
HKR, Fax\Class1\AdaptiveAnswer,SerialSpeedDataDetect,,     "19200"
HKR, Fax\Class1\AdaptiveAnswer,HostCommandDataDetect,,     "ATO"
HKR, Fax\Class1\AdaptiveAnswer,ModemResponseDataConnect,,  "CONNECT"

[EXTERNAL]
HKR,, DeviceType, 1, 01

[ZC56K.Voice]
HKR,,Enumerator,,serwave.vxd
HKR,, VoiceProfile,                        1, 27,03,08,02
;HKR,,VoiceProfile,                        1, 27,22,09,02

; ------- start section for NT5 voice support --------------
; see REG147.DOC for details on next NT5 voice section.
HKR, WaveDriver,  BaudRate,                1, 00,c2,01,00
HKR, WaveDriver,  XformID,                 1, 01,00
HKR, WaveDriver,  WaveDevices,             1, 02,00
HKR, WaveDriver,  XformModule,,            "umdmxfrm.dll"
HKR, WaveDriver,  WaveHardwareID,,  "ZyXEL_Comet_3356_(K.56)_VoiceModemWave"
; ------- end section for NT5 voice support --------------

HKR,, VoiceBaudRate,                       1, 00,c2,01,00
HKR,, VoiceMixerMid,                       1, 02,00
HKR,, VoiceMixerPid,                       1, 99,01
HKR,, VoiceMixerLineID,                    1, 00,00,05,00
HKR,, SpeakerPhoneSpecs,                   1, 00,00,00,00, 0f,00,00,00, 03,00,00,00, 00,00,00,00
HKR, SpeakerPhoneEnable,                   1,, "at#vls=6<cr>"
HKR, SpeakerPhoneDisable,                  1,, "at#vls=6<cr>"
HKR, SpeakerPhoneDisable,                  2,, "at#spk=0,15,,<cr>"
HKR, SpeakerPhoneDisable,                  3,, "at#vls=0<cr>"
HKR, SpeakerPhoneMute,                     1,, "at#vls=6<cr>"
HKR, SpeakerPhoneMute,                     2,, "at#spk=0,,,<cr>"
HKR, SpeakerPhoneUnMute,                   1,, "at#vls=6<cr>"
HKR, SpeakerPhoneUnMute,                   2,, "at#spk=1,,,<cr>"
HKR, SpeakerPhoneSetVolumeGain,            1,, "at#vls=6<cr>"
HKR, SpeakerPhoneSetVolumeGain,            2,, "at#spk=,<Vol>,<Gain><cr>"
HKR, EnableCallerID,                       1,, "at#cid=1<cr>"
HKR, EnableDistinctiveRing,                1,, "at-sdr=7<cr>"
HKR,, HandsetCloseDelay,                   1, 1e,00,00,00
HKR, StartPlay,                            1,, "at#vtx<cr>"
HKR, StopPlay,                             1,, "None"
HKR, StopPlay,                             2,, "NoResponse"
HKR, StartRecord,                          1,, "at#vrx<cr>"
HKR, StopRecord,                           1,, "None"
HKR, StopRecord,                           2,, "NoResponse"
HKR,, TerminateRecord,,                    "!"
HKR,, TerminatePlay,,                      "<h10><h03>"
HKR,, AbortPlay,,                          "<h10><h18>"
HKR, LineSetPlayFormat,                    1,, "at#vls=0<cr>"
HKR, LineSetRecordFormat,                  1,, "None"
HKR, LineSetRecordFormat,                  2,, "NoResponse"
HKR, HandsetSetRecordFormat,               1,, "at#vsr=7200<cr>"
HKR, HandsetSetRecordFormat,               2,, "at#vbs=4<cr>"
HKR, HandsetSetPlayFormat,                 1,, "at#vsr=7200<cr>"
HKR, HandsetSetPlayFormat,                 2,, "at#vbs=4<cr>"
HKR, OpenHandset,                          1,, "at#cls=8<cr>"
HKR, OpenHandset,                          2,, "at#vls=1<cr>"
HKR,, ForwardDelay,                        1, 88,13
HKR, CloseHandset,                         1,, "at#cls=0<cr>"
HKR, VoiceToDataAnswer,                    1,, "at#cls=0<cr>"
HKR, VoiceToDataAnswer,                    2,, "ata<cr>"
HKR, VoiceAnswer,                          1,, "at#cls=8<cr>"
HKR, VoiceAnswer,                          2,, "at#vls=0<cr>"
HKR, VoiceAnswer,                          3,, "at#vbt=1<cr>"
HKR, VoiceAnswer,                          4,, "at#vsr=7200<cr>"
HKR, VoiceAnswer,                          5,, "at#vbs=4<cr>"
HKR, VoiceAnswer,                          6,, "ata<cr>"
HKR, VoiceDialNumberSetup,                 1,, "at#cls=8<cr>"
HKR, VoiceDialNumberSetup,                 2,, "at#vls=0<cr>"
HKR, VoiceDialNumberSetup,                 3,, "at#vrn=0<cr>"
HKR, VoiceDialNumberSetup,                 4,, "at#vbt=1<cr>"
HKR, VoiceDialNumberSetup,                 5,, "at#vsr=7200<cr>"
HKR, VoiceDialNumberSetup,                 6,, "at#vbs=4<cr>"
HKR, GenerateDigit,                        1,, "at#vts=<Digit><cr>"
HKR,, CallerIDPrivate,,                    P
HKR,, CallerIDOutSide,,                    O
HKR,, VariableTerminator,,                 <cr><lf>

HKR, Responses, "<cr><lf>VCON<cr><lf>",    1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATE = ",         1, 93, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "TIME = ",                 1, 94, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NMBR = ",                 1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NAME = ",                 1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "MESG = ",                 1, 97, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING1<cr><lf>",   1, 18, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING2<cr><lf>",   1, 19, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING3<cr><lf>",   1, 1a, 00, 00,00,00,00, 00,00,00,00


[AllMfg.AddReg]
HKR,,Logging, 1, 01
HKR,,LoggingPath,, "ModemLog.txt"
HKR,,ConfigDialog,,modemui.dll
HKR,,DevLoader,,*vcomm
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR,,FriendlyDriver,,Unimodem.VXD
HKR,, InactivityScale, 1, 0a,00,00,00
HKR,,PortSubClass,1,02
HKR,, Reset,, "ATZ<cr>"
HKR, Answer,    1,, "ATA<cr>"
HKR, Hangup,    1,, "ATH<cr>"
HKR, Init,      1,, "AT<cr>"
HKR, Init,      2,, "AT&FE0V1&C1&D2S95=46S0=0<cr>"
HKR, Monitor,   1,, "ATS0=0<cr>"
HKR, Monitor,   2,, "None"

HKR, Responses, "0<cr>",                                   1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "1<cr>",                                   1, 02, 00, 00,00,00,00, 00,00,00,00 ; CONNECT
HKR, Responses, "4<cr>",                                   1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR
HKR, Responses, "3<cr>",                                   1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "6<cr>",                                   1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE
HKR, Responses, "7<cr>",                                   1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY
HKR, Responses, "8<cr>",                                   1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER
HKR, Responses, "2<cr>",                                   1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING

HKR, Responses, "<cr><lf>OK<cr><lf>",                      1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",                 1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",                   1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",              1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>",             1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",                    1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",               1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",                    1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BLACKLISTED<cr><lf>",             1, 1c, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DELAYED ",                        1, 1d, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>+FCERROR<cr><lf>",                1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+F4<cr><lf>",                     1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>FAX<cr><lf>",                     1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATA<cr><lf>",                    1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>VOICE<cr><lf>",                   1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+FCON<cr><lf>",                   1, 03, 00, 00,00,00,00, 00,00,00,00

; standard CARRIER responses
HKR, Responses, "<cr><lf>CARRIER 300<cr><lf>",             1, 01, 00, 2c,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 1200<cr><lf>",            1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 2400<cr><lf>",            1, 01, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 4800<cr><lf>",            1, 01, 00, c0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 7200<cr><lf>",            1, 01, 00, 20,1c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 9600<cr><lf>",            1, 01, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 12000<cr><lf>",           1, 01, 00, e0,2e,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 14400<cr><lf>",           1, 01, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 16800<cr><lf>",           1, 01, 00, a0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 19200<cr><lf>",           1, 01, 00, 00,4b,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 21600<cr><lf>",           1, 01, 00, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 24000<cr><lf>",           1, 01, 00, c0,5d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 26400<cr><lf>",           1, 01, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 28800<cr><lf>",           1, 01, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 31200<cr><lf>",           1, 01, 00, e0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 33600<cr><lf>",           1, 01, 00, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 75/1200<cr><lf>",         1, 01, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 1200/75<cr><lf>",         1, 01, 00, b0,04,00,00, 00,00,00,00

; extended (K56.flex) CARRIER responses
HKR, Responses, "<cr><lf>CARRIER 32000<cr><lf>",           1, 01, 00, 00,7d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 34000<cr><lf>",           1, 01, 00, d0,84,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 36000<cr><lf>",           1, 01, 00, a0,8c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 38000<cr><lf>",           1, 01, 00, 70,94,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 40000<cr><lf>",           1, 01, 00, 40,9c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 42000<cr><lf>",           1, 01, 00, 10,a4,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 44000<cr><lf>",           1, 01, 00, e0,ab,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 46000<cr><lf>",           1, 01, 00, b0,b3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 48000<cr><lf>",           1, 01, 00, 80,bb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 50000<cr><lf>",           1, 01, 00, 50,c3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 52000<cr><lf>",           1, 01, 00, 20,cb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 54000<cr><lf>",           1, 01, 00, f0,d2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 56000<cr><lf>",           1, 01, 00, c0,da,00,00, 00,00,00,00

; extended (V.90) CARRIER responses
HKR, Responses, "<cr><lf>CARRIER 28000<cr><lf>",           1, 01, 00, 60,6d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 29333<cr><lf>",           1, 01, 00, 95,72,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 30667<cr><lf>",           1, 01, 00, cb,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 33333<cr><lf>",           1, 01, 00, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 34667<cr><lf>",           1, 01, 00, 6b,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 37333<cr><lf>",           1, 01, 00, d5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 38667<cr><lf>",           1, 01, 00, 0b,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 41333<cr><lf>",           1, 01, 00, 75,a1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 42667<cr><lf>",           1, 01, 00, ab,a6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 45333<cr><lf>",           1, 01, 00, 15,b1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 46667<cr><lf>",           1, 01, 00, 4b,b6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 49333<cr><lf>",           1, 01, 00, b5,c0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 50667<cr><lf>",           1, 01, 00, eb,c5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 53333<cr><lf>",           1, 01, 00, 55,d0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 54667<cr><lf>",           1, 01, 00, 8b,d5,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>COMPRESSION: NONE<cr><lf>",       1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>COMPRESSION: CLASS 5<cr><lf>",    1, 01, 01, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>COMPRESSION: V.42BIS<cr><lf>",    1, 01, 01, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>PROTOCOL: NONE<cr><lf>",          1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: LAP-M<cr><lf>",         1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: ALT<cr><lf>",           1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: ALT-CELLULAR<cr><lf>",  1, 01, 0a, 00,00,00,00, 00,00,00,00

; if s95=46: responses DTE speed without error correction
HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>",            1, 02, 00, 00,00,00,00, b0,04,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",            1, 02, 00, 00,00,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",            1, 02, 00, 00,00,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",            1, 02, 00, 00,00,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",           1, 02, 00, 00,00,00,00, 00,4b,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",           1, 02, 00, 00,00,00,00, 00,96,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",           1, 02, 00, 00,00,00,00, 00,e1,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",          1, 02, 00, 00,00,00,00, 00,c2,01,00

; if s95=46: responses DTE speed with error correction
HKR, Responses, "<cr><lf>CONNECT 1200/ARQ<cr><lf>",        1, 02, 02, 00,00,00,00, b0,04,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/ARQ<cr><lf>",        1, 02, 02, 00,00,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/ARQ<cr><lf>",        1, 02, 02, 00,00,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/ARQ<cr><lf>",        1, 02, 02, 00,00,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/ARQ<cr><lf>",       1, 02, 02, 00,00,00,00, 00,4b,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/ARQ<cr><lf>",       1, 02, 02, 00,00,00,00, 00,96,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/ARQ<cr><lf>",       1, 02, 02, 00,00,00,00, 00,e1,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/ARQ<cr><lf>",      1, 02, 02, 00,00,00,00, 00,c2,01,00

