; Windows Modem Setup File
; Copyright 1999 Microsoft Corp.
; Manufacturer: ZyXEL Communications Corp.

[Version]
; Created by Che-Ming Lu based on ZyXEL "omni.net LCD" ISDN terminal adapter
;
; history:
; 05/12/1999 -> FCS
; 06/24/1999 -> Support USA(VID_0586&PID_1001)
; 06/28/1999 -> Support Japan(VID_0586&PID_1002)
; -------------------------------------------------------------
;
;
; This INF is based on Microsoft's Modem Development Kit v1.47
; (MDK147.DOC & REG147.DOC, Oct 1998) which is available from:
; WindowsNT 5.0 Beta 2 DDK


Signature="$CHICAGO$"
Class=Modem
Provider=%Mfg%
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
;LayoutFile=layout.inf

[Strings]
Mfg		= "ZyXEL Communications Corp."
OL_DSS1		= "ZyXEL omni.net LCD Plus (COM,DSS1)"
OL_DSS1.PnP	= "ZyXEL omni.net LCD Plus (COM,DSS1), Plug&Play"
OL_JAPAN	= "ZyXEL omni.net LCD Plus (COM,Japan)"
OL_JAPAN.PnP	= "ZyXEL omni.net LCD Plus (COM,Japan), Plug&Play"
OL_USA		= "ZyXEL omni.net LCD Plus (COM,USA)"
OL_USA.PnP	= "ZyXEL omni.net LCD Plus (COM,USA), Plug&Play"

USB_USA		= "ZyXEL omni.net LCD Plus (USB,USA)"
USB_DSS1	= "ZyXEL omni.net LCD Plus (USB,DSS1)"
USB_JAPAN	= "ZyXEL omni.net LCD Plus (USB,Japan)"

[Manufacturer]
%Mfg% = ZyXEL

[OL_USA.NoResDup]
UNIMODEM650CD1234

[OL_DSS1.NoResDup]
UNIMODEM650847DB,UNIMODEMBB55122B,UNIMODEM49867FC4

[OL_JAPAN.NoResDup]
UNIMODEM28BC0068

[ControlFlags]
ExcludeFromSelect=SERENUM\ZYX0FFF
ExcludeFromSelect=SERENUM\ZYX0FFE
ExcludeFromSelect=SERENUM\ZYX0FFD
ExcludeFromSelect=SERENUM\ZYX0FFC
ExcludeFromSelect=SERENUM\ZYX0FFB
ExcludeFromSelect=SERENUM\ZYX0FFA
ExcludeFromSelect=SERENUM\ZYX0FF9
ExcludeFromSelect=SERENUM\ZYX0FF8
ExcludeFromSelect=SERENUM\ZYX0FF7
ExcludeFromSelect=SERENUM\ZYX0FF6
ExcludeFromSelect=SERENUM\ZYX0FF5
ExcludeFromSelect=SERENUM\ZYX0FF4
ExcludeFromSelect=SERENUM\ZYX0FF3
ExcludeFromSelect=SERENUM\ZYX0FF2
ExcludeFromSelect=SERENUM\ZYX0FF1
ExcludeFromSelect=SERENUM\ZYX0FF0
ExcludeFromSelect=SERENUM\ZYX0FEF
ExcludeFromSelect=SERENUM\ZYX0FEE
ExcludeFromSelect=SERENUM\ZYX0FED
ExcludeFromSelect=SERENUM\ZYX0FEC
ExcludeFromSelect=SERENUM\ZYX0FEB
ExcludeFromSelect=SERENUM\ZYX0FEA
ExcludeFromSelect=SERENUM\ZYX0FE9
ExcludeFromSelect=SERENUM\ZYX0FE8
ExcludeFromSelect=SERENUM\ZYX0FE7
ExcludeFromSelect=SERENUM\ZYX0FE6
ExcludeFromSelect=SERENUM\ZYX0FE5
ExcludeFromSelect=SERENUM\ZYX0FE4
ExcludeFromSelect=SERENUM\ZYX0FE3
ExcludeFromSelect=SERENUM\ZYX0FE2
ExcludeFromSelect=SERENUM\ZYX0FE1
ExcludeFromSelect=SERENUM\ZYX0FE0
ExcludeFromSelect=SERENUM\ZYX0FDF
ExcludeFromSelect=SERENUM\ZYX0FDE
ExcludeFromSelect=SERENUM\ZYX0FDD
ExcludeFromSelect=SERENUM\ZYX0FDC
ExcludeFromSelect=SERENUM\ZYX0FDB
ExcludeFromSelect=SERENUM\ZYX0FDA
ExcludeFromSelect=SERENUM\ZYX0FD9
ExcludeFromSelect=SERENUM\ZYX0FD8
ExcludeFromSelect=SERENUM\ZYX0FD7
ExcludeFromSelect=SERENUM\ZYX0FD6
ExcludeFromSelect=SERENUM\ZYX0FD5
ExcludeFromSelect=SERENUM\ZYX0FD4
ExcludeFromSelect=SERENUM\ZYX0FD3
ExcludeFromSelect=SERENUM\ZYX0FD2
ExcludeFromSelect=SERENUM\ZYX0FD1
ExcludeFromSelect=SERENUM\ZYX0FD0
ExcludeFromSelect=SERENUM\ZYX0FCF
ExcludeFromSelect=SERENUM\ZYX0FCE
ExcludeFromSelect=SERENUM\ZYX0FCD
ExcludeFromSelect=SERENUM\ZYX0FCC
ExcludeFromSelect=SERENUM\ZYX0FCB
ExcludeFromSelect=SERENUM\ZYX0FCA
ExcludeFromSelect=SERENUM\ZYX0FC9
ExcludeFromSelect=SERENUM\ZYX0FC8
ExcludeFromSelect=SERENUM\ZYX0FC7
ExcludeFromSelect=SERENUM\ZYX0FC6
ExcludeFromSelect=SERENUM\ZYX0FC5
ExcludeFromSelect=SERENUM\ZYX0FC4
ExcludeFromSelect=SERENUM\ZYX0FC3
ExcludeFromSelect=SERENUM\ZYX0FC2
ExcludeFromSelect=SERENUM\ZYX0FC1
ExcludeFromSelect=SERENUM\ZYX0FC0
ExcludeFromSelect=SERENUM\ZYX0FBF
ExcludeFromSelect=SERENUM\ZYX0FBE
ExcludeFromSelect=SERENUM\ZYX0FBD
ExcludeFromSelect=SERENUM\ZYX0FBC
ExcludeFromSelect=SERENUM\ZYX0FBB
ExcludeFromSelect=SERENUM\ZYX0FBA
ExcludeFromSelect=SERENUM\ZYX0FB9
ExcludeFromSelect=SERENUM\ZYX0FB8
ExcludeFromSelect=SERENUM\ZYX0FB7
ExcludeFromSelect=SERENUM\ZYX0FB6
ExcludeFromSelect=SERENUM\ZYX0FB5
ExcludeFromSelect=SERENUM\ZYX0FB4
ExcludeFromSelect=SERENUM\ZYX0FB3
ExcludeFromSelect=SERENUM\ZYX0FB2
ExcludeFromSelect=SERENUM\ZYX0FB1
ExcludeFromSelect=SERENUM\ZYX0FB0
ExcludeFromSelect=SERENUM\ZYX0F55
ExcludeFromSelect=SERENUM\ZYX0F03	; For USB (Japan)
ExcludeFromSelect=SERENUM\ZYX0F02	; For USB (USA)
ExcludeFromSelect=SERENUM\ZYX0F01	; For USB (DSS1)
;ExcludeFromSelect=SERENUM\ZYX0F00

[ZyXEL]
%OL_USA.PnP%= OL_USA, SERENUM\ZYX0FFF
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FFE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FFD
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FFC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FFB
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FFA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FF0
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FEF
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FEE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FED
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FEC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FEB
%OL_JAPAN.PnP%=OL_JAPAN,SERENUM\ZYX0FEA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FE0
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FDF
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FDE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FDD
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FDC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FDB
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FDA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FD0
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FCF
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FCE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FCD
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FCC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FCB
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FCA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FC0
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FBF
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FBE
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FBD
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FBC
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FBB
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FBA
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB9
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB8
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB7
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB6
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB5
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB4
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB3
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB2
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB1
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0FB0
%OL_DSS1.PnP%=OL_DSS1,SERENUM\ZYX0F55
%USB_JAPAN%=OL_JAPAN,SERENUM\ZYX0F03	; for USB (Japan)
%USB_USA%=OL_USA,SERENUM\ZYX0F02	; for USB (USA)
%USB_DSS1%=OL_DSS1,SERENUM\ZYX0F01	; for USB (DSS1)
;%OL_1TR6.PnP%=OL_1TR6,SERENUM\ZYX0F00

; UNIMODEM-IDs
%OL_USA%= OL_USA,UNIMODEM650CD1234		; 255 (USA)
%OL_DSS1%=OL_DSS1,UNIMODEM650847DB 		; DSS1 Standard
%OL_DSS1%=OL_DSS1,UNIMODEMBB55122B 		; 217,218 (Korea, NTK)
%OL_DSS1%=OL_DSS1,UNIMODEM49867FC4 		; 238 (Taiwan)
%OL_JAPAN%=OL_JAPAN,UNIMODEM28BC0068 		; 234 (Japan)

[OL_USA]
AddReg=All, OL.Data, OL.Responses, ISDN.All, ISDN.USA

[OL_DSS1]
AddReg=All, OL.Data, OL.Responses, ISDN.All, ISDN.DSS1

[OL_JAPAN]
AddReg=All, OL.Data, OL.Responses, ISDN.All, ISDN.JAPAN

[All]
HKR,,Logging, 1, 01
HKR,,LoggingPath,,"modemlog.txt"
HKR,,DeviceType, 1, 01
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,ConfigDialog,,modemui.dll
HKR,,PortSubClass,1,02
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"

HKR, Responses, "0<cr>",                                   1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "9<cr>",                                   1, 01, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "1<cr>",                                   1, 02, 00, 00,00,00,00, 00,00,00,00 ; CONNECT
HKR, Responses, "4<cr>",                                   1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR
HKR, Responses, "3<cr>",                                   1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "6<cr>",                                   1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE
HKR, Responses, "7<cr>",                                   1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY
HKR, Responses, "8<cr>",                                   1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER
HKR, Responses, "2<cr>",                                   1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING

HKR, Responses, "<cr><lf>OK<cr><lf>",                      1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RINGING<cr><lf>",                 1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",                 1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",                   1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",              1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>",             1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",                    1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",               1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",                    1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>FM:",                             1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>TO:",                             1, 96, 00, 00,00,00,00, 00,00,00,00


[OL.Data]
HKR,, Properties, 1, 00,00,00,00, ff,00,00,00, ff,00,00,00, 07,00,00,00, 07,00,00,00, 33,01,00,00, 00,08,07,00, 00,f4,01,00
HKR,, DCB,        1, 1c,00,00,00, 00,c2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00,11, 13, 00, 00, 00
HKR,, Default,    1, 3c,00,00,00,00,00,00,00, 01,00,00,00,01,00,00,00, 12,00,00,00
HKR,, InactivityScale, 1, 0a,00,00,00
HKR,, Reset,,                                              "ATZ<cr>"
;HKR,, UserInit,,                                          "ATB40"
HKR, Init,      1,,                                        "AT&FZE0X8<cr>"
HKR, Init,      2,,                                        "ATV1&D2&C1S0=0<cr>"
HKR, Init,      3,,                                        "AT&L1S38.3=1<cr>"
HKR, Init,      4,,                                        "ATS84.4=1S118.3=0<cr>"
HKR, Init,      5,,                                        "ATCN<0><cr>"
HKR, Init,      6,,                                        "ATCI<00><cr>"
HKR, Monitor,   1,,                                        "ATS0=0<cr>"
HKR, Monitor,   2,,                                        "None"
HKR, Hangup,    1,,                                        "ATH0<cr>"
HKR, Answer,    1,,                                        "ATA<cr>"
HKR, Settings, CallSetupFailTimer,,                        "S7=<#>"
HKR, Settings, Compression_Off,,                           "&K00"
HKR, Settings, Compression_On,,                            "&K44"
HKR, Settings, DialPrefix,,                                "D"
HKR, Settings, DialSuffix,,                                ""
HKR, Settings, ErrorControl_Off,,                          "&K0"
HKR, Settings, ErrorControl_On,,                           "&K3"
HKR, Settings, FlowControl_Hard,,                          "&H3"
HKR, Settings, FlowControl_Off,,                           "&H0"
HKR, Settings, FlowControl_Soft,,                          "&H4"
HKR, Settings, InactivityTimeout,,                         "S50=<#>"
HKR, Settings, Prefix,,                                    "AT"
HKR, Settings, Pulse,,                                     "P"
HKR, Settings, SpeakerMode_Dial,,                          "M1"
HKR, Settings, SpeakerMode_Off,,                           "M0"
HKR, Settings, SpeakerMode_On,,                            "M2"
HKR, Settings, SpeakerMode_Setup,,                         "M3"
HKR, Settings, SpeakerVolume_High,,                        "L3"
HKR, Settings, SpeakerVolume_Low,,                         "L1"
HKR, Settings, SpeakerVolume_Med,,                         "L2"
HKR, Settings, Terminator,,                                "<cr>"
HKR, Settings, Tone,,                                      "T"


[OL.Responses]
HKR, Responses, "<cr><lf>CARRIER 2400<cr><lf>", 		1, 01, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 4800<cr><lf>", 		1, 01, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 9600<cr><lf>", 		1, 01, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 14400<cr><lf>", 		1, 01, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 19200<cr><lf>", 		1, 01, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 38400<cr><lf>", 		1, 01, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 57600<cr><lf>", 		1, 01, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 56000<cr><lf>", 		1, 01, 00, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 64000<cr><lf>", 		1, 01, 00, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 112K<cr><lf>", 		1, 01, 00, 80,B5,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CARRIER 128K<cr><lf>", 		1, 01, 00, 00,F4,01,00, 00,00,00,00

HKR, Responses, "<cr><lf>PROTOCOL: V110<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: PPP<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: SLIP<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75M<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: X.75C<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120M<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: V120C<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>PROTOCOL: BTX<cr><lf>", 		1, 01, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>ERROR CONTROL: NONE<cr><lf>", 	1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: LAPB<cr><lf>", 	1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR CONTROL: LAPD<cr><lf>", 	1, 01, 02, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>COMPRESSION: V42b<cr><lf>", 	1, 01, 01, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>",        	1, 02, 00, 00,00,00,00, b0,04,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",        	1, 02, 00, 00,00,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",         1, 02, 00, 00,00,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",         1, 02, 00, 00,00,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",        1, 02, 00, 00,00,00,00, 00,4b,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",        1, 02, 00, 00,00,00,00, 00,96,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",        1, 02, 00, 00,00,00,00, 00,e1,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",       1, 02, 00, 00,00,00,00, 00,c2,01,00
HKR, Responses, "<cr><lf>CONNECT 230400<cr><lf>",       1, 02, 00, 00,00,00,00, 00,84,03,00
HKR, Responses, "<cr><lf>CONNECT 460800<cr><lf>",       1, 02, 00, 00,00,00,00, 00,08,07,00
HKR, Responses, "<cr><lf>CONNECT    USB<cr><lf>",       1, 02, 00, 00,00,00,00, 00,c2,01,00
;HKR, Responses, "<cr><lf>CONNECT    USB<cr><lf>",       1, 02, 00, 00,00,00,00, 00,00,00,00

; ISDN install section is preliminary for support of external ISDN TAs in
; WindowsNT 5.0 Beta2 (build 1877)
; INF section originally by Jim Hood (Microsoft UNIMODEM development team)
; modified by Manfred Recla (ZyXEL Comm. Corp. Europe - 12/08/1998)

[ISDN.All]
HKR, EnableCallerID,1,, 					"ats84.4=0<cr>"
HKR, ISDN\Init,1,,                          "AT&O2<cr>"
HKR, ISDN\NvSave,1,,                        "AT<cr>"
HKR, ISDN\NvSave,2,,                        "AT<cr>"

HKR, Protocol\ISDN\AUTO_1CH,1,,             "ATB95&J0S80.6=0<cr>"
HKR, Protocol\ISDN\HDLC_PPP_56K,1,,         "ATB40&J0&E1<cr>"
HKR, Protocol\ISDN\HDLC_PPP_64K,1,,         "ATB40&J0&E0<cr>"
HKR, Protocol\ISDN\HDLC_PPP_112K,1,,        "ATB40&J3&E1<cr>"
HKR, Protocol\ISDN\HDLC_PPP_128K,1,,        "ATB40&J3&E0<cr>"
HKR, Protocol\ISDN\HDLC_PPP_128K_PAP,1,,    "ATB40&J3&E0S87.2=1S118.3=0<cr>"
HKR, Protocol\ISDN\HDLC_PPP_128K_CHAP,1,,   "ATB40&J3&E0S87.2=0S118.3=0<cr>"
;HKR, Protocol\ISDN\HDLC_PPP_128K_MSCHAP,1,,"ATB40&J3&E0S87.2=0S118.3=1<cr>"

HKR, Protocol\ISDN\V120_56K,1,,             "ATB20&J0&E1<cr>"
HKR, Protocol\ISDN\V120_64K,1,,             "ATB20&J0&E0S80.6=1<cr>"
HKR, Protocol\ISDN\V120_112,1,,             "ATB20&J3&E1<cr>"
HKR, Protocol\ISDN\V120_128K,1,,            "ATB20&J3&E0S80.6=1<cr>"

HKR, Protocol\ISDN\X75_64K,1,,              "ATB00&J0&E0S80.6=1<cr>"
HKR, Protocol\ISDN\X75_128K,1,,             "ATB00&J3&E0S80.6=1S100.0=0<cr>"
HKR, Protocol\ISDN\X75_T_70,1,,             "ATB01&J0&E0S80.6=1<cr>"
HKR, Protocol\ISDN\X75_BTX,1,,              "ATB04&J0&E0S80.6=1<cr>"

HKR, Protocol\ISDN\V110_2DOT4K,1,,          "ATB13S80.6=1<cr>"
HKR, Protocol\ISDN\V110_4DOT8K,1,,          "ATB14S80.6=1<cr>"
HKR, Protocol\ISDN\V110_9DOT6K,1,,          "ATB15S80.6=1<cr>"
HKR, Protocol\ISDN\V110_14DOT4K,1,,         "ATB16S80.6=1<cr>"
HKR, Protocol\ISDN\V110_19DOT2K,1,,         "ATB17S80.6=1<cr>"
HKR, Protocol\ISDN\V110_38DOT4K,1,,         "ATB18<cr>"

[ISDN.USA]
HKR, ISDN\SwitchType, SWITCH_DMS100,,      "ATP0<cr>"   ;Northern Telecom DMS-100
HKR, ISDN\SwitchType, SWITCH_NI1,,         "ATP1<cr>"   ;National ISDN 1, 1 SPID
HKR, ISDN\SwitchType, SWITCH_NI2,,         "ATP2<cr>"   ;National ISDN 1, 2 SPIDs
HKR, ISDN\SwitchType, SWITCH_ATTPTP,,      "ATP4<cr>"   ;AT&T 5ESS Custom, Point-to-Point
HKR, ISDN\SwitchType, SWITCH_ATT1,,        "ATP5<cr>"   ;AT&T 5ESS Custom, Point-to-MultiPoint, 1 SPID
HKR, ISDN\SwitchType, SWITCH_ATT2,,        "ATP6<cr>"   ;AT&T 5ESS Custom, Point-to-MultiPoint, 2 SPIDs

HKR, Responses, "<cr><lf>Switch Type : Northern Telecom DMS<cr><lf>",                   1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : NI1(1 SPID)<cr><lf>",                            1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : NI1(2 SPID)<cr><lf>",                            1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : NI2<cr><lf>",                                    1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : NI3<cr><lf>",                                    1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : AT&T 5ESS point-to-point<cr><lf>",               1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : AT&T 5ESS point-to-multipoint(1 SPID)<cr><lf>",  1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Switch Type : AT&T 5ESS point-to-multipoint(2 SPID)<cr><lf>",  1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "SPID0 =",                                                              1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "SPID1 =",                                                              1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "Please use ATSPIDnn..n to input SPID!<cr><lf>",                        1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "Please Reset TA (Power On/Off) & Reenter SPID(s)",                     1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>WARNING: No Channel(SPID) Available<cr><lf>",                  1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>WARNING: Layer 1 Not Active<cr><lf>",                          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>Don't need SPID in AT&T P-t-P mode!<cr><lf>",                  1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>SPID correct!<cr><lf>",                                        1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>SPID Error!<cr><lf>",                                          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>SPID correct! Full Service.<cr><lf>",                          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>SPID not correct! Restricted Service.<cr><lf>",                1, 00, 00, 00,00,00,00, 00,00,00,00

HKR, ISDN, CompatibilityFlags,             1, 00,00,00,01
HKR, ISDN\SetSpid, 1,,                     "ATSPID0=%s<cr>"
HKR, ISDN\SetSpid, 2,,                     "ATSPID1=%s<cr>"
HKR, ISDN\DirectoryNo, 1,,                 "AT&ZI4=%s<cr>"  ; ISDN Data (MultiAuto)
HKR, ISDN\DirectoryNo, 2,,                 "AT&ZI7=%s<cr>"  ; POTS port #1
;HKR, ISDN\DirectoryNo, 3,,                "AT&ZI6=%s<cr>"    POTS port #2


[ISDN.DSS1]
HKR, ISDN\SwitchType, SWITCH_DSS1,,        "AT<cr>"
HKR, ISDN,CompatibilityFlags,1,            00,00,00,00
HKR, ISDN\SetMSN,1,,                       "AT&ZI4=%s<cr>"  ; ISDN Data (MultiAuto)
HKR, ISDN\SetMSN,2,,                       "AT&ZI7=%s<cr>"  ; POTS port #1
;HKR, ISDN\SetMSN,3,,                       "AT&ZI6=%s<cr>"   POTS port #2

[ISDN.JAPAN]
HKR, ISDN\SwitchType, SWITCH_INS64,,       "AT<cr>"
HKR, ISDN\SwitchType, SWITCH_DSS1,,        "AT<cr>"
HKR, Protocol\ISDN\V110_57DOT6K,1,,        "ATB19<cr>"
HKR, ISDN,CompatibilityFlags,1,            00,00,00,00
HKR, ISDN\SetMSN,1,,                       "AT&ZI4=%s<cr>"  ; ISDN Data (MultiAuto)
HKR, ISDN\SetMSN,2,,                       "AT&ZI7=%s<cr>"  ; POTS port #1
;HKR, ISDN\SetMSN,3,,                       "AT&ZI6=%s<cr>"   POTS port #2
