; NECX540.INF
; Setup information file for NEC MultiSync X540 Monitor
;
; Copyright 2004, NEC-Mitsubishi Electronics Display, Inc.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NMD%
CatalogFile=NX540.cat
DriverVer=02/25/2004,4.02.0025.0922

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC61E4

[DestinationDirs]
DefaultDestDir = 11
NEC-X540.CopyFiles = 23

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
NX540.icm=1

[Manufacturer]
%NMD%=NMD

[NMD]
%NEC-X540%=NEC-X540.Install, Monitor\NEC61E4

[NEC-X540.Install]
DelReg=DEL_CURRENT_REG
AddReg=NEC-X540.AddReg, 1280, DPMS
CopyFiles=NEC-X540.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1280]
HKR,,MaxResolution,,"1280,1024"

[DPMS]
HKR,,DPMS,,1

[NEC-X540.AddReg]
HKR,"MODES\1280,1024",Mode1,,"30.0-71.0,55.0-120.0,+,+"
HKR,,ICMProfile,0,"NX540.icm"

[NEC-X540.CopyFiles]
NX540.icm

[Strings]
NMD="NEC-Mitsubishi"
Disk1="NEC-Mitsubishi Monitor Installation Disk"
NEC-X540="NEC MultiSync X540"