; nl218ux.inf
; Setup information file for NEC MultiSync LCD2180UX Monitor
;
; Copyright 2005, NEC Display Solutions, Ltd.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NECDS%
CatalogFile=nl218ux.cat
DriverVer=10/18/2005,2.05.1018.2017

[ClassInstall32]
AddReg=ClassAddReg32

[ClassAddReg32]
HKR,,,,%MonitorClassName%
HKR,,Icon,,"-1"
HKR,,NoInstallClass,,1

[DestinationDirs]
LCD2180UX.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
nl218ux.icm=1

[Manufacturer]
%NECDS%=NECDS,ntamd64

[NECDS]
%LCD2180UX%=LCD2180UX.Install, Monitor\NEC662C

[NECDS.ntamd64]
%LCD2180UX%=LCD2180UX.Install.ntamd64, Monitor\NEC662C

[LCD2180UX.Install]
DelReg=DEL_CURRENT_REG
AddReg=LCD2180UX.AddReg, 1600, DPMS
CopyFiles=LCD2180UX.CopyFiles

[LCD2180UX.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=LCD2180UX.AddReg, 1600, DPMS
CopyFiles=LCD2180UX.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1600]
HKR,,MaxResolution,,"1600,1200"

[DPMS]
HKR,,DPMS,,1

[LCD2180UX.AddReg]
HKR,"MODES\1600,1200",Mode1,,"30.0-96.0,48.0-87.0,+,+"
HKR,,ICMProfile,0,"nl218ux.icm"

[LCD2180UX.CopyFiles]
nl218ux.icm

[Strings]
MonitorClassName="Monitor"
NECDS="NEC"
LCD2180UX="NEC MultiSync LCD2180UX"
Disk1="NEC Display Solutions Installation Disk"