; nl2335.inf
; Setup information file for NEC MultiSync LCD2335WXM Monitor
;
; Copyright 2005, NEC-Mitsubishi Electronics Display, Inc.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NMD%
CatalogFile=nl2335.cat
DriverVer=01/18/2005,1.05.0118.1024

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC667F
ExcludeFromSelect.nt=Monitor\NEC6680

[DestinationDirs]
LCD2335WXM.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
nl2335.icm=1

[Manufacturer]
%NMD%=NMD

[NMD]
%LCD2335WXM-A%=LCD2335WXM-A.Install, Monitor\NEC667F
%LCD2335WXM-D%=LCD2335WXM-D.Install, Monitor\NEC6680

[LCD2335WXM-A.Install]
DelReg=DEL_CURRENT_REG
AddReg=LCD2335WXM-A.AddReg, 1280, DPMS
CopyFiles=LCD2335WXM.CopyFiles

[LCD2335WXM-D.Install]
DelReg=DEL_CURRENT_REG
AddReg=LCD2335WXM-D.AddReg, 1280, DPMS
CopyFiles=LCD2335WXM.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1280]
HKR,,MaxResolution,,"1280,768"

[DPMS]
HKR,,DPMS,,1

[LCD2335WXM-A.AddReg]
HKR,"MODES\1280,768",Mode1,,"31.0-63.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"nl2335.icm"

[LCD2335WXM-D.AddReg]
HKR,"MODES\1280,768",Mode1,,"31.0-63.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"nl2335.icm"


[LCD2335WXM.CopyFiles]
nl2335.icm

[Strings]
NMD="NEC-Mitsubishi"
LCD2335WXM-A="NEC MultiSync LCD2335WXM(Analog)"
LCD2335WXM-D="NEC MultiSync LCD2335WXM(Digital)"
Disk1="NEC-Mitsubishi Monitor Installation Disk"