/************************************************************************/
/*									*/
/*	Install documentation for Plug & Play Hansol Mazellan Monitor	*/
/*									*/
/*      Windows Hansol Mazellan Monitor Installation Program  	 	*/						
/*									*/
/************************************************************************/  

/***********************  Contents  *************************************/
/*									*/
/*   1.Windows2000 Monitor Installation Procedure			*/
/*       1)Automatic Install Procedure					*/
/*       2)Manual Install Procedure					*/
/*									*/
/*   2.Windows98 Monitor Installation Procedure				*/
/*       1)Automatic Install Procedure					*/
/*       2)Manual Install Procedure					*/
/*									*/
/*   3.Windows95 Monitor Installation Procedure				*/
/*       1)Automatic Install Procedure					*/
/*       2)Manual Install Procedure					*/
/*									*/
/*   4.WindowsNT Monitor Installation Procedure				*/
/*									*/
/*   5.Linux Monitor Installation Procedure				*/
/*       1)Linux Install Procedure					*/
/*       2)Monitor Installation Tip					*/
/*									*/
/*   6.WindowsME Monitor Installation Procedure				*/
/*       1)Automatic Install Procedure					*/
/*       2)Manual Install Procedure					*/
/*									*/
/*   7.Windows xp Monitor Installation Procedure			*/
/*       1)Automatic Install Procedure					*/
/*									*/
/************************************************************************/



*** Warning: Before you install your monitor, please verify the correct monitor model name.
               If this is not selected correctly, the host pc can not display the monitor as best 
		refresh rate and display resolution.
		You can see the correct monitor name at front or back label of monitor. 

  *** Monitor Optimization : This is the funtion which gives the optimal display of monitor.
                             When you use the monitor, this may set the optiomal resolution and
                             refresh rate for helping eye to see more correctly.     
			     And this program operates on automatic install procedure.


1.Windows2000 Monitor Installation Procedure			

 1)Automatic Install Procedure					

    > Insert Installation Disk into your Computer.	
      
    > Run "install.exe".
      
    > Select your monitor model.

    > Press the "OK" button. 
     
    > If you meet the "Do you want to continue the installtion?", press the "Yes" button.

    > If you meet the "Monitor is installed in your system successfully", Press the "Yes" button.

    > From now on, the monitor optimization program is going to be started.
   
         "Now,Ready to start Monitor optimization.
          If you don't want to keep the new settings,
          Press 'Esc' or wait 12 seconds"
   
      If the above window appear, press "OK" button. At this time you may see the 
      blank display for a few seconds.
      And if you don't want to run the optimization program, press "Cancel" button.


    > If the display appear without any problem after optimization operated, press "Yes" on
      below window.

         "Monitor optimization is completed!!
          Return to previous window in 6 seconds
          Do you want to keep this setting?"   

      If you don't want the optimized display video mode, press "No" button.


    > From above, if you press "No", the below window will be displayed.
      This window helps you set the new video mode again.

          "Choose resolution and refresh rate"

      Press "OK" button, after setting the resolution and refresh rate.
      If you don't want to change the resolution and refresh rate, press "Cancel" button.	 


    > From above, if you press "OK" button, the below window will be displayed.

          "If you don't want to keep the new settings,
          Press 'Esc' or wait 12 seconds"

      If the above window appear, press "OK" button. At this time you may see the 
      blank display for a few seconds.
     

    > The below window will be displayed

          "Display size is changed !!
           Return to previous window in 6 seconds
           Do you want to keep this setting?"
   
      If the display appear without any problem , press "Yes" button on above window.
      And if you don't want the new display mode, press "No" button and try to proceed
      above procedure repeatedly until get the optimal video mode.   



 2)Manual Install Procedure					

    > Click Start, then Settings, then Control Panel.

    > Start the "Display" applet program. 

    > Select the "Settings" page and select the "Advanced Properties" button.

    > Select the "Monitor" page.

    > Press the "Properties" button.
     
    > Select the "Driver"  page.

    > Press the "Update Driver..." button.

    > Press the "Next" button.

    > Select the "Display a list of the known drivers for this device so that I can choose a 
                   specific driver" and press the "Next" button.
    
    > Press the "Have Disk..." button.

    > Specify the path to the INF file and press the "OK" button

          Example 1: Insert the disk in the A: floppy drive,
                     and enter A:\.

          Example 2: Type in the name of the directory where you copied
                     the INF file, either on your local hard drive or
                     on a network share.

          Example 3: If you're not sure exactly where the INF file is,
                     choose the "Browse..." button to find it.

    > Select the monitor model that corresponds to the one you connected to your 
      computer and press "Next" button.

    > Press the "Next" button.

    > Press the "Yes" button.

    > Windows2000 will copy the INF file and the ICM Profile to the proper
      directory on your system.

    > Press the "Finish" button.
      
    > Continue choosing "Close" button and "OK" button  until you close 
      the Display Properties dialog box.
      (You can get some other screen for warning message or others,then
       click the appreciate option for your monitor)


////////////////////////////////////////////////////////////////////////////////////////////////////

2.Windows98 Monitor Installation Procedure	 
  
 1)Automatic Install Procedure					
      
    > Insert Installation Disk into your Computer.	
      
    > Run "install.exe".
      
    > Select your monitor model.
     
    > On "Insert Disk" Screen, Type full path name for the Installation Disk
      to install monitor driver. and  Click "OK" Button.
      
    > Click "OK" Button for continuing install.

    > From now on, the monitor optimization program is going to be started.
   
         "Now,Ready to start Monitor optimization.
          If you don't want to keep the new settings,
          Press 'Esc' or wait 12 seconds"
   
      If the above window appear, press "OK" button. At this time you may see the 
      blank display for a few seconds.
      And if you don't want to run the optimization program, press "Cancel" button.


    > If the display appear without any problem after optimization operated, press "Yes" on
      below window.

         "Monitor optimization is completed!!
          Return to previous window in 6 seconds
          Do you want to keep this setting?"   

      If you don't want the optimized display video mode, press "No" button.


    > From above, if you press "No", the below window will be displayed.
      This window helps you set the new video mode again.

          "Choose resolution and refresh rate"

      Press "OK" button, after setting the resolution and refresh rate.
      If you don't want to change the resolution and refresh rate, press "Cancel" button.	 


    > From above, if you press "OK" button, the below window will be displayed.

          "If you don't want to keep the new settings,
          Press 'Esc' or wait 12 seconds"

      If the above window appear, press "OK" button. At this time you may see the 
      blank display for a few seconds.
     

    > The below window will be displayed

          "Display size is changed !!
           Return to previous window in 6 seconds
           Do you want to keep this setting?"
   
      If the display appear without any problem , press "Yes" button on above window.
      And if you don't want the new display mode, press "No" button and try to proceed
      above procedure repeatedly until get the optimal video mode.   




 2)Manual Install Procedure					

    > Click Start, then Settings, then Control Panel.

    > Start the "Display" applet program. 

    > Select the "Settings" page and select the "Advanced Properties" button.

    > Select the "Monitor" button.

    > Select the "Change" button in the "Monitor Type" area.
     
    > Click the "Have Disk" button.

    > Specify the path to the INF file and press the <ENTER> key:

          Example 1: Insert the disk in the A: floppy drive,
                     and enter A:\.

          Example 2: Type in the name of the directory where you copied
                     the INF file, either on your local hard drive or
                     on a network share.

          Example 3: If you're not sure exactly where the INF file is,
                     choose the "Browse..." button to find it.

    > The "Select Device" dialog box will appear. Choose "Show all devices"
      Select the monitor that corresponds to the one you connected to your 
      computer and click OK.

    > Windows 98 will copy the INF file and the ICM Profile to the proper
      directory on your system.
      
    > Continue choosing "Close" button and "O.K" button  until you close 
      the Display Properties dialog box.
      (You can get some other screen for warning message or others,then
       click the appreciate option for your monitor)


/////////////////////////////////////////////////////////////////////////////////

3.Windows95 Monitor Installation Procedure			

 1)Automatic Install Procedure					
      
    > Insert Installation Disk into your Computer.	
      
    > Run "install.exe".
      
    > Select your monitor model.
     
    > On "Insert Disk" Screen, Type full path name for the Installation Disk
      to install monitor driver. and  Click "OK" Button.
      
    > Click "OK" Button for continuing install.

    > On "Window needed to be restarted 
          Do you want to restart window right now?" Screen
      Click "OK" Button for completing installation.

    * Note : We recommend you to restart window right now for using the driver 
             setting correctly.

 2)Manual Install Procedure					
     
    > Click Start, then Settings, then Control Panel.

    > Start the "Display" applet program. 

    > Select the "Settings" page and select the "Change Display Type" button.
	
    * Note : If "Advanced Properties" appears on this "Settings" window,
	 	 use the instructions for Windows 98.

    > Select the "Change" button in the "Monitor Type" area.

    > Select the "Have Disk" button and press "OK".

    > Specify the path to the INF file and press the <ENTER> key:

          Example 1: Insert the disk in the A: floppy drive,
                     and enter A:\.

          Example 2: Type in the name of the directory where you copied
                     the INF file, either on your local hard drive or
                     on a network share.

          Example 3: If you're not sure exactly where the INF file is,
                     choose the "Browse..." button to find it.

    > The "Select Device" dialog box will appear. Choose "Show all devices"
      Select the monitor that corresponds to the one you connected to your 
      computer and click OK.
    
    > Continue choosing "Close" button until you close the Display 
	Properties dialog box.
	* Note : Reboot the system to use the new driver.


/////////////////////////////////////////////////////////////////////////////////

4.WindowsNT Monitor Installation Procedure
 
  <WindowNT  Display Monitor setting procedure>

   > Select Control panel by clicking first twice My Computer and 
     then twice the Control Panel. 

   > In Control panel click Display icon twice. 

   > Click "Settings". 

   > Click "Display Type". 

   > Click "Change", if You want to change the Display adapter type. 

   > In the Manufacturers box select the model that matches your hardware 
      (refer to the manufacturer specification if you need help). 
      If your graphics adapter vendor is not listed insert the disk and 
       click "Have Disk" or contact Your graphic card manufacturer. 

   > Click "OK" and follow instructions on the screen. 

   > After the Display Adapter has been installed properly click "Close" 
      to exit Display Type screen. 

   > In the Display properties screen Select wanted Desktop Area 
     and the amount of colors in the Color Palette box. For possible 
      alternatives refer to the monitor specification in the User's manual. 

   > Click "Refresh frequency" to change it. 
     For possible Refresh rates refer to the monitor specification in the 
     User's manual. 

   > Select e.g. 60Hz , 75Hz , 85 Hz. 

   > Click "TEST" to test the display. 

   > Click "OK" and the test screen appears. 

   > If You saw the test bitmap correctly press "Yes" , otherwise "No". 

   > If you have changed the adapter settings you have to restart the computer 
     before settings will take effect.                                    


/////////////////////////////////////////////////////////////////////////////////

5. Linux Monitor Installation Procedure

 1)Linux Install Procedure					

   In order to execute the X-window, you have to make the XF86Config file which is 
   the system setup file. Your monitor also can setup through this file.
   Also this file is generated by executing the XF86config.

   > After execute the xf86config, press "Enter" at first and second display.

   > At third display, you can see the display of installation of mouse

   > At this time you have to setup your mouse according to your mouse hardware

   > And next display is the installation of Keyboard.

   > You have to setup your keyboard according to your keyboard.

   > From now on , the monitor installation will come out.

   > At first, you have to setup the Horizontal frequency. Select the number which you want to setup.
     And also you can type the frequency directly.  See monitor user's manual.

   > And then you have to setup the Vertical frequency. following is the same as Horizontal frequency.

   > Type the name of monitor. This name is not related to X-window execution.

   > Now the monitor setup is completed

   > Complete the other hardware setup.

   > If you complete all hardware setup, save the configuration file.

   > Now execute the X-window.
     Even though you setup all above procedure, the X-Window can't run.
     If the X-window doesn't run properly, you will have to modify the x86config file as follows.

    < Linux Modification Items >

   >  Replace the "#" with the value of Bandwidth refer to user's manual

   >  Modify the other additional hardware modification.

   >  Finally, you have to select the video mode.

   >  Now run the X-Window.


 2)Monitor Installation Tip					

  < Explanation and Concept regarding the display monitor >

    The related document is located at dm/usr/X11R6/lib/X11/doc/Video Mode.doc and read the "readme.txt".

    >Horizontal Sync. Frequency (Unit Khz)
      This is the Dot Line per 1 seconds. And if you are setting the H-Frequency incorrectly, it will cause  problem 
      to the monitor hardware. you have to set the H-Frequency correctly.

    >Vertical Sync Frequency(Refresh Rate,  Unit Hz)
      This is the frame number per 1seconds. And if you are setting the V-Frequency incorrectly, it will cause flickering.
      If you work long time with this stituation, your eye will be tired. In order to reduce this problem,
      you have to increase the V-Frequency  up to 70Hz. 

    >Dot Clock (Bandwidth)
      This is indicate the speed of Video Signal.

    >ModeLine Data Detail
	ModeLine "640x400"   25.175    640 664 760 800 400 409 411 450 -hsync +vsync
	640x480 --> Resolution
        25.175  --> Dot Clock(MHz)

    >Using the monitor installation diskette
        - Open the Xf86Config file with Linux Editor.
        - Move to [Monitor] Section.
        - After you select the monitor model in your install diskette, copy the data of HorizSync and VertRefresh
          to XF86Config.
        - Disable the resolution using the "#" at ModeLine.
          And after you select the monitor model in your install diskette, copy the data of ModeLine to XF86Config.  


////////////////////////////////////////////////////////////////////////////////////////////////////

6.Windows Me(Millennium) Monitor Installation Procedure	 
  
 1)Automatic Install Procedure					
      
    > Insert Installation Disk into your Computer.	
      
    > Run "install.exe".
      
    > Select your monitor model.
     
    > On "Insert Disk" Screen, Type full path name for the Installation Disk
      to install monitor driver. and  Click "OK" Button.
      
    > Click "OK" Button for continuing install.

    > From now on, the monitor optimization program is going to be started.
   
         "Now,Ready to start Monitor optimization.
          If you don't want to keep the new settings,
          Press 'Esc' or wait 12 seconds"
   
      If the above window appear, press "OK" button. At this time you may see the 
      blank display for a few seconds.
      And if you don't want to run the optimization program, press "Cancel" button.


    > If the display appear without any problem after optimization operated, press "Yes" on
      below window.

         "Monitor optimization is completed!!
          Return to previous window in 6 seconds
          Do you want to keep this setting?"   

      If you don't want the optimized display video mode, press "No" button.


    > From above, if you press "No", the below window will be displayed.
      This window helps you set the new video mode again.

          "Choose resolution and refresh rate"

      Press "OK" button, after setting the resolution and refresh rate.
      If you don't want to change the resolution and refresh rate, press "Cancel" button.	 


    > From above, if you press "OK" button, the below window will be displayed.

          "If you don't want to keep the new settings,
          Press 'Esc' or wait 12 seconds"

      If the above window appear, press "OK" button. At this time you may see the 
      blank display for a few seconds.
     

    > The below window will be displayed

          "Display size is changed !!
           Return to previous window in 6 seconds
           Do you want to keep this setting?"
   
      If the display appear without any problem , press "Yes" button on above window.
      And if you don't want the new display mode, press "No" button and try to proceed
      above procedure repeatedly until get the optimal video mode.   



 2)Manual Install Procedure					

    > Click Start, then Settings, then Control Panel.

    > Start the "Display" applet program. 

    > Select the "Settings" page and select the "Advanced Properties" button.

    > Select the "Monitor" button.

    > Select the "Change" button.
     
    > Click the "Specify the location of the driver(Advanced)" radio button and press "Next" button.

    > Click the "Display a list of all the drivers in a specific location, so you can select the driver you want"
        radio button and press the "Next" button.

    > Press the "Have Disk..." button.

    > Click the "Show all hardware."

    > Select the model what you want to install and press the "Next" button.

    > Press the "Next" button.

    > Press the "Finish" button.

    > Windows ME will copy the INF file and the ICM Profile to the proper
      directory on your system.
      
    > Continue choosing "Close" button and "O.K" button  until you close 
      the Display Properties dialog box.
      (You can get some other screen for warning message or others,then
       click the appreciate option for your monitor)


////////////////////////////////////////////////////////////////////////////////////////////////////

7.Windows xp Monitor Installation Procedure	 
  
 1)Automatic Install Procedure					
      
    > Insert Installation Disk into your Computer.	
      
    > Run "Install.exe".
      
    > Select your monitor model.
     
    > On "Insert Disk" Screen, Type full path name for the Installation Disk
      to install monitor driver. and  Click "OK" Button.
      
    > Click "OK" Button for continuing install.

    > From now on, the monitor optimization program is going to be started.
   
         "Now,Ready to start Monitor optimization.
          If you don't want to keep the new settings,
          Press 'Esc' or wait 12 seconds"
   
      If the above window appear, press "OK" button. At this time you may see the 
      blank display for a few seconds.
      And if you don't want to run the optimization program, press "Cancel" button.


    > If the display appear without any problem after optimization operated, press "Yes" on
      below window.

         "Monitor optimization is completed!!
          Return to previous window in 6 seconds
          Do you want to keep this setting?"   

      If you don't want the optimized display video mode, press "No" button.


    > From above, if you press "No", the below window will be displayed.
      This window helps you set the new video mode again.

          "Choose resolution and refresh rate"

      Press "OK" button, after setting the resolution and refresh rate.
      If you don't want to change the resolution and refresh rate, press "Cancel" button.	 


    > From above, if you press "OK" button, the below window will be displayed.

          "If you don't want to keep the new settings,
          Press 'Esc' or wait 12 seconds"

      If the above window appear, press "OK" button. At this time you may see the 
      blank display for a few seconds.
     

    > The below window will be displayed

          "Display size is changed !!
           Return to previous window in 6 seconds
           Do you want to keep this setting?"
   
      If the display appear without any problem , press "Yes" button on above window.
      And if you don't want the new display mode, press "No" button and try to proceed
      above procedure repeatedly until get the optimal video mode.   





