;------------------------------------------------------------------------
;
;   Copyright and Disclaimer:
;
;       ---------------------------------------------------------------
;       This software is provided "as is" without warranty of any kind,
;       either expressed or implied, including but not limited to the
;       implied warranties of merchantability and/or fitness for a
;       particular purpose.
;
;       Copyright (c) 2005 Conexant Systems, Inc.
;       All Rights Reserved.
;       ---------------------------------------------------------------
;
;   Abstract:
;
;       This is the 32-bit CX23880 video capture driver inf file.
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Conexant"
DriverVer=03/16/2007,6.0.103.0
CatalogFile.ntx86=cxavsvid.cat

[Manufacturer]
"Conexant"=Conexant

[SourceDisksNames]
1="Conexant Cx23880 Drivers",,,""

[SourceDisksFiles]
cxavsvid.sys=1
cpnotify.ax=1

[Conexant]
;---------------------------------
; Philips 4-in-1 EVK
;---------------------------------
%CX23880.videoPhilips4In1%=CX23880.Philips4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_096614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_096614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_096614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_096614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_096614F1
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_096614F1

;---------------------------------
; E4 TVFM 880 PAL MK3
;---------------------------------
%CX23880.videoPhilips4In1%=CX23880.Philips4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_011314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_011314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_011314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_011314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_011314F1
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_011314F1

;---------------------------------
; 1394 PAL MK3
;---------------------------------
%CX23880.videoPhilips4In1%=CX23880.Philips4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_018314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_018314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_018314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_018314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_018314F1

;---------------------------------
; StreamAMachine PAL MK3
;---------------------------------
%CX23880.videoPhilips4In1%=CX23880.Philips4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_019814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_019814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_019814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_019814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_019814F1

;---------------------------------
; NTSC 1394 EVK, Philips 1236 MK3 tuner
;---------------------------------
%CX23880.videoPhilipsMK3%=CX23880.PhilipsMK3,PCI\VEN_14F1&DEV_8800&SUBSYS_008314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_008314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_008314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_008314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_008314F1

;---------------------------------
; E4 TVFM 880 NTSC MK3
;---------------------------------
%CX23880.videoPhilipsMK3%=CX23880.PhilipsMK3,PCI\VEN_14F1&DEV_8800&SUBSYS_001314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_001314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_001314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_001314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_001314F1
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_001314F1

;---------------------------------
; E4 TVFM 883 NTSC FI1236 MK3
;---------------------------------
%CX23880.videoPhilipsFIMK3%=CX23880.FI1236MK3,PCI\VEN_14F1&DEV_8800&SUBSYS_00F814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_00F814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_00F814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_00F814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_00F814F1

;---------------------------------
; Half-high NTSC 880 MK3
;---------------------------------
%CX23880.videoPhilipsMK3%=CX23880.PhilipsMK3,PCI\VEN_14F1&DEV_8800&SUBSYS_027614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_027614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_027614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_027614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_027614F1

;---------------------------------
; StreamAMachine NTSC MK3
;---------------------------------
%CX23880.videoPhilipsMK3%=CX23880.PhilipsMK3,PCI\VEN_14F1&DEV_8800&SUBSYS_009814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_009814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_009814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_009814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_009814F1

;---------------------------------------
; Stratford - DVB-T using Gromit OFDM demod with Alps Tuner
;---------------------------------------
%CX23880.videoAlpsDVBT%=CX23880.AlpsDVBT,PCI\VEN_14F1&DEV_8800&SUBSYS_008714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_008714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_008714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_008714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_008714F1

;---------------------------------------
; Goshawk - DVB-S using Conexant Rosie/Camaric QPSK tuner/demod combination with IR remote
;---------------------------------------
%CX23880.videoCnxtDVBS%=CX23880.CnxtDVBS,PCI\VEN_14F1&DEV_8800&SUBSYS_008414F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_008414F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_008414F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_008414F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_008414F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_008414F1

;---------------------------------------
; Stratford2 - DVB-T using Gromit OFDM demod with Thomson Tuner and IR remote
;---------------------------------------
%CX23880.videoThomsonDVBT%=CX23880.ThomsonDVBT,PCI\VEN_14F1&DEV_8800&SUBSYS_018714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_018714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_018714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_018714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_018714F1

;---------------------------------------
; KittyHawk2 - ATSC/NTSC/FM using 8-VSB demod with Thomson DTT7612 Tuner
; and IR remote
;---------------------------------------
%CX23880.videoThomsonATSCNTSC%=CX23880.Kittyhawk2,PCI\VEN_14F1&DEV_8800&SUBSYS_000614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_000614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_000614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_000614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_000614F1

;---------------------------------------
; Oxford, 882 - PAL/DVB-T using Gromit COFDM demod with Philips FDM1216ME tuner
; Video Driver enabled
; Audio Driver disabled
; TS Driver enabled
; VIP Port disabled
; Host Port disabled
;---------------------------------------
%CX23880.videoPhilipsPALDVBT%=CX23880.PhilipsPALDVBT,PCI\VEN_14F1&DEV_8800&SUBSYS_007114F1
%CX23880.null%=NullSection,                          PCI\VEN_14F1&DEV_8801&SUBSYS_007114F1
%CX23880.null%=NullSection,                          PCI\VEN_14F1&DEV_8802&SUBSYS_007114F1
%CX23880.null%=NullSection,                          PCI\VEN_14F1&DEV_8803&SUBSYS_007114F1
%CX23880.null%=NullSection,                          PCI\VEN_14F1&DEV_8804&SUBSYS_007114F1
%CX23880.null%=NullSection,                          PCI\VEN_14F1&DEV_8811&SUBSYS_007114F1

;---------------------------------
; E4 TVFM 880 PAL DKI with TCL2002MI tuner
;---------------------------------
%CX23880.videoTclPALDKI%=CX23880.TclPALDKI,PCI\VEN_14F1&DEV_8800&SUBSYS_084214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_084214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_084214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_084214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_084214F1
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_084214F1

[CX23880.Philips4In1]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,WDMAUDIO.Registration,BDA.Registration,bda.Installation.NT
AddReg=     CX880.AddReg,Philips4in1.AddReg,XBAR.AddReg,CX23880.Philips4In1.AddReg
CopyFiles=  CX880.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23880.PhilipsMK3]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,WDMAUDIO.Registration,BDA.Registration,bda.Installation.NT
AddReg=     CX880.AddReg,PhilipsMK3.AddReg,XBAR.AddReg
CopyFiles=  CX880.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23880.FI1236MK3]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,WDMAUDIO.Registration,BDA.Registration,bda.Installation.NT
AddReg=     CX880.AddReg,PhilipsFI1236MK3.AddReg,XBAR.AddReg
CopyFiles=  CX880.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23880.AlpsDVBT]
Include=    ks.inf, kscaptur.inf, ksfilter.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation,WDMAUDIO.Registration,BDA.Registration,bda.Installation.NT
AddReg=     CX880.AddReg,AlpsDVBT.AddReg,XBAR.AddReg,CXTS.AddReg
CopyFiles=  CX880.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23880.CnxtDVBS]
Include=    ks.inf, kscaptur.inf, ksfilter.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation,WDMAUDIO.Registration,BDA.Registration,bda.Installation.NT
AddReg=     CX880.AddReg,CnxtDVBS.AddReg,XBAR.AddReg,CXTS.AddReg
CopyFiles=  CX880.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23880.ThomsonDVBT]
Include=    ks.inf, kscaptur.inf, ksfilter.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation,WDMAUDIO.Registration,BDA.Registration,bda.Installation.NT
AddReg=     CX880.AddReg,ThomsonDVBT.AddReg,XBAR.AddReg,CXTS.AddReg
CopyFiles=  CX880.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23880.Kittyhawk2]
Include=    ks.inf, kscaptur.inf, ksfilter.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation,WDMAUDIO.Registration,BDA.Registration,bda.Installation.NT
AddReg=     CX880.AddReg,Kittyhawk2.AddReg,XBAR.AddReg,CXTS.AddReg
CopyFiles=  CX880.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23880.PhilipsPALDVBT]
Include=    ks.inf, kscaptur.inf, ksfilter.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation,WDMAUDIO.Registration,BDA.Registration,bda.Installation.NT
AddReg=     CX880.AddReg,PhilipsPALDVBT.AddReg,XBAR_Dual2.AddReg,CXTS.AddReg
CopyFiles=  CX880.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23880.TclPALDKI]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,WDMAUDIO.Registration,BDA.Registration,bda.Installation.NT
AddReg=     CX880.AddReg,TclPALDKI.AddReg,XBAR.AddReg,CX23880.TclPALDKI.AddReg
CopyFiles=  CX880.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[NullSection]

[NullSection.Services]
AddService = , 2  ; null service install

[DestinationDirs]
CX880.CopyDrivers=10,system32\drivers
DSFilters.CopyFiles=11

[CX880.CopyDrivers]
cxavsvid.sys

[DSFilters.CopyFiles]
cpnotify.ax

[DSFilters.RegDLL]
11,,cpnotify.ax,1

[CX880.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,cxavsvid.sys
HKR,,OkToHibernate,3,01
; Disable driver page out
HKR,,PageOutWhenUnopened,3,0
;HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKLM,%MediaCategories%\%GUID.PINNAME_ANALOG_AUDIO_IN%,Name,,%Pin.p2AnalogAudioIn%
HKLM,%MediaCategories%\%GUID.PINNAME_AUDIO_OUT%,Name,,%PinName.AnalogAudioOut%
;Wave in audio device registration
HKR,Drivers,SubClasses,,"wave"
HKR,Drivers\wave\wdmaud.drv, Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,%AudioFriendlyName%
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0xFE, 0x00, 0x00, 0x00
;setting timer value to 1500ms
HKR,"DriverData","XPSP2CracklingFixDelayTime", 0x00010001, 0x5dc

;
; Driver Configuration Registry Entries
;
[CX23880.Philips4In1.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00

[CX23880.TclPALDKI.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x20,0x00,0x00,0x00
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x56,0x00,0x00,0x00
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

;-------------------------------------------------------------------
; Crossbar AddReg sections
;
;---Crossbar registry values---
;
; Note: For each pin on the crossbar, specify the following:
; (1) Pin type 
;     0 - SVIDEO
;     1 - Tuner
;     2 - Composite
;     3 - 656
;     4 - audio tuner in
;     5 - audio line in
; (2) InputMux (optional) - input mux to use for the selected pin
; (3) RelatedPinIndex 
; (4) GPIOMask (optional) - Mask specifying which GPIO bits to set or clear
; (5) GPIOSettings (optional) - Settings for GPIO bits specified in the mask 

;-------------------------------------------------------------------

[XBAR.AddReg]
;Pin 0 - Tuner In
;HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x01,0x00,0x00,0x00
;HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x00,0x00,0x00,0x00
;HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00

;Pin 1 - Composite in
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 2 - S-Video in
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x02,0x00,0x00,0x00
;HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 3 - Tuner Audio
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 4 - Audio Line in
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x05,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

[XBAR_Dual2.AddReg]
;Pin 0 - Tuner In
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x05,0x00,0x00,0x00

;Pin 1 - Composite 1
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","GPIOMask",0x00010001, 0x83,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","GPIOSettings",0x00010001, 0x81,0x00,0x00,0x00

;Pin 2 - Composite 2
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","GPIOMask",0x00010001, 0x83,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","GPIOSettings",0x00010001, 0x03,0x00,0x00,0x00

;Pin 3 - S-Video 1
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","InputMux",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","GPIOMask",0x00010001, 0x83,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","GPIOSettings",0x00010001, 0x81,0x00,0x00,0x00

;Pin 4 - S-Video 2
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputMux",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","GPIOMask",0x00010001, 0x83,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","GPIOSettings",0x00010001, 0x03,0x00,0x00,0x00

;Pin 5 - Tuner Audio
HKR,"DriverData\XBarPin5","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBarPin5","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 6 - Audio Line in 1
HKR,"DriverData\XBarPin6","PinType",0x00010001, 0x05,0x00,0x00,0x00
HKR,"DriverData\XBarPin6","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin6","GPIOMask",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData\XBarPin6","GPIOSettings",0x00010001, 0x01,0x00,0x00,0x00

;Pin 7 - Audio Line in 2
HKR,"DriverData\XBarPin7","PinType",0x00010001, 0x05,0x00,0x00,0x00
HKR,"DriverData\XBarPin7","RelatedPinIndex",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin7","GPIOMask",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData\XBarPin7","GPIOSettings",0x00010001, 0x03,0x00,0x00,0x00

;Tuner input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x00,0x00,0x00,0x00

;-------------------------------------------------------------------
; Tuner AddReg sections
;-------------------------------------------------------------------

[PhilipsMK3.AddReg]
HKR,"DriverData","TunerType",0x00010001, 0x0B, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC0, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00

[Philips4in1.AddReg]
HKR,"DriverData","TunerType",0x00010001, 0x0A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC0, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00

[PhilipsFI1236MK3.AddReg]
HKR,"DriverData","TunerType",0x00010001, 0x0C, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC0, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00

[TclPALDKI.AddReg]
HKR,"DriverData","TunerType",0x00010001, 0x1E, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC0, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00


;-------------------------------------------------------------------
; AddReg sections for DVB-T DVB-S and ATSC
;-------------------------------------------------------------------

[AlpsDVBT.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x00,0x01,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; prevent audio tracking thread from running, card doesn't support
; any audio.  Audio is in mpeg packets.  Setting to I2S audio.
HKR,"DriverData","WWAudioPrimaryStandard",0x00010001, 0x0B,0x00,0x00,0x00
HKR,"DriverData","TunerModel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","UseFreqOffsetDVBT",0x00010001, 0x00, 0x00, 0x00, 0x00

; these registry keys for TS filter
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

[CnxtDVBS.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; prevent audio tracking thread from running, card doesn't support
; any audio.  Audio is in mpeg packets.  Setting to I2S audio.
HKR,"DriverData","WWAudioPrimaryStandard",0x00010001, 0x0B,0x00,0x00,0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

; these registry keys for TS filter
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

[ThomsonDVBT.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x00,0x01,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; prevent audio tracking thread from running, card doesn't support
; any audio.  Audio is in mpeg packets.  Setting to I2S audio.
HKR,"DriverData","WWAudioPrimaryStandard",0x00010001, 0x0B,0x00,0x00,0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","TunerModel",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","UseFreqOffsetDVBT",0x00010001, 0x00, 0x00, 0x00, 0x00

; these registry keys for TS filter
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

[Kittyhawk2.AddReg]
HKR,"DriverData","TunerType",0x00010001, 0x18, 0x00, 0x00, 0x00
HKR,"DriverData","DemodType",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00
HKR,"DriverData","TunerModel",0x00010001, 0x05,0x00,0x00,0x00

;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00

; these registry keys for TS filter
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x00,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

[PhilipsPALDVBT.AddReg]
HKR,"DriverData","TunerType",0x00010001, 0x17, 0x00, 0x00, 0x00
HKR,"DriverData","DemodType",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00
HKR,"DriverData","TunerModel",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData","UseFreqOffsetDVBT",0x00010001, 0x00, 0x00, 0x00, 0x00

HKR,"DriverData","VideoStandard",0x00010001, 0x00,0x01,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is Great Britain = 44
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x2C,0x00,0x00,0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x04,0x00,0x00,0x00

; these registry keys for TS filter
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

;-------------------------------------------------------------------
; AddReg sections for TS filter
;-------------------------------------------------------------------

[CXTS.AddReg]
HKLM,System\CurrentControlSet\Control\MediaCategories\%TSPinID%,Display,1, 00,00,00,00
HKLM,System\CurrentControlSet\Control\MediaCategories\%TSPinID%,Name,,%TSPinName%

;
; Interfaces installation
;

;
; Video
;
[CX23880.Philips4In1.Interfaces]
Needs=VID.Interfaces

[CX23880.PhilipsMK3.Interfaces]
Needs=VID.Interfaces

[CX23880.FI1236MK3.Interfaces]
Needs=VID.Interfaces

[CX23880.AlpsDVBT.Interfaces]
Needs=BDA.Interfaces

[CX23880.CnxtDVBS.Interfaces]
Needs=BDA.Interfaces

[CX23880.ThomsonDVBT.Interfaces]
Needs=BDA.Interfaces

[CX23880.Kittyhawk2.Interfaces]
Needs=VID.Interfaces

[CX23880.PhilipsPALDVBT.Interfaces]
Needs=VID.Interfaces

[CX23880.TclPALDKI.Interfaces]
Needs=VID.Interfaces

[VID.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%KsNameFilter%,VID_Interface,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%TVAudioReferenceGuid%,TvAudio_Interface,
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%XBARReferenceGUID%,CX88XBAR_Interface,
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},%TunerReferenceGuid%,CX88TUNE_Interface,
AddInterface={6994AD04-93EF-11D0-A3CC-00A0C9223196},%AudioReferenceGuid%,AUD_Interface,
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%BDATuneReferenceGuid%,BDATUNE_Interface,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSReferenceGuid%,TS_Interface

[BDA.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%KsNameFilter%,VID_Interface,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%TVAudioReferenceGuid%,TvAudio_Interface,
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%XBARReferenceGUID%,CX88XBAR_Interface,
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%BDATuneReferenceGuid%,BDATUNE_Interface,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSReferenceGuid%,TS_Interface

[VID_Interface]
AddReg=VID_Interface.AddReg

[VID_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%VIDFriendlyName%

[TvAudio_Interface]
AddReg=TvAudio_Interface.AddReg

[TvAudio_Interface.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%TVAudioFriendlyName%

[CX88XBAR_Interface]
AddReg=CX88XBAR_Interface.AddReg

[CX88XBAR_Interface.AddReg]
HKR,,CLSID,,{71F96460-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%XBARFriendlyName%

[CX88TUNE_Interface]
AddReg=CX88TUNE_Interface.AddReg

[CX88TUNE_Interface.AddReg]
HKR,,CLSID,,{266EEE40-6C63-11cf-8A03-00AA006ECB65}
HKR,,FriendlyName,,%TunerFriendlyName%

[AUD_Interface]
AddReg=AUD_Interface.AddReg

[AUD_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%AudioFriendlyName%

[BDATUNE_Interface]
AddReg=BDATUNE_Interface.AddReg

[BDATUNE_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%BDATuneFriendlyName%

[TS_Interface]
AddReg=TS_Interface.AddReg

[TS_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%TSFriendlyName%

;
; Services installation
;
[CX23880.Philips4In1.Services]
AddService = CX88VID,2,VID.ServiceInstall

[CX23880.PhilipsMK3.Services]
AddService = CX88VID,2,VID.ServiceInstall

[CX23880.FI1236MK3.Services]
AddService = CX88VID,2,VID.ServiceInstall

[CX23880.AlpsDVBT.Services]
AddService = CX88VID,2,VID.ServiceInstall

[CX23880.CnxtDVBS.Services]
AddService = CX88VDVBS,2,VID.ServiceInstall

[CX23880.ThomsonDVBT.Services]
AddService = CX88VID,2,VID.ServiceInstall

[CX23880.Kittyhawk2.Services]
AddService = CX88VID,2,VID.ServiceInstall

[CX23880.PhilipsPALDVBT.Services]
AddService = CX88VID,2,VID.ServiceInstall

[CX23880.TclPALDKI.Services]
AddService = CX88VID,2,VID.ServiceInstall

[VID.ServiceInstall]
DisplayName   = %CX23880.DeviceDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\cxavsvid.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
KsNameFilter                 = "{9B365890-165F-11D0-A195-0020AFD156E4}"
Proxy.CLSID                  = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
CX23880.DeviceDesc           = "Conexant 2388x AvStream Video Capture"
CX23880.videoPhilipsMK3      = "Conexant 2388x AVS Video Capture (Philips 1236MK3)"
CX23880.videoPhilipsFIMK3    = "Conexant 2388x AVS Video Capture (Philips FI1236MK3)"	
CX23880.videoPhilips4In1     = "Conexant 2388x AVS Video Capture (Philips 4-in-1)"
CX23880.videoAlpsDVBT        = "Conexant 2388x AVS Video Capture (Alps DVB-T)"
CX23880.videoCnxtDVBS        = "Conexant 2388x AVS Video Capture (Conexant DVB-S)"
CX23880.videoThomsonDVBT     = "Conexant 2388x AVS Video Capture (Thomson DVB-T)"
CX23880.videoThomsonATSCNTSC = "Conexant 2388x AVS Video Capture (Thomson ATSC/NTSC)"
CX23880.videoPhilipsPALDVBT  = "Conexant 2388x AVS Video Capture (Philips PAL/DVB-T)"
CX23880.videoTclPALDKI       = "Conexant 2388x AVS Video Capture (TCL2002MI PAL-D/K & I)"
VIDFriendlyName              = "Conexant 2388x Video Capture"
CX23880.null                 = "Conexant (unused device function)"
CX23881.null                 = "Conexant (unused device function)"
MediaCategories              = "SYSTEM\CurrentControlSet\Control\MediaCategories"
GUID.PINNAME_ANALOG_AUDIO_IN = "{04394D28-52A7-4c46-AED0-65D62CC64DA6}"
Pin.p2AnalogAudioIn          = "Analog Audio In"
GUID.PINNAME_AUDIO_OUT       = "{9DA02733-7910-40f2-95DD-0441676C9A9B}"
PinName.AnalogAudioOut       = "Audio Out"
TSPinID                      = "{5237C937-0A21-4f7e-B338-DE0D0793D03F}"
TSPinName                    = "TS Out"
AudioFriendlyName            = "Conexant 2388x Audio Capture"
AudioReferenceGuid           = "{AB766B70-AFB3-4461-A4DE-22E9C516B7FE}"
TVAudioFriendlyName          = "Conexant 2388x TvAudio"
TVAudioReferenceGuid         = "{991182D5-71A2-4b5c-9817-F551FBBC8232}"
XBARFriendlyName             = "Conexant 2388x Crossbar"
XBARReferenceGUID            = "{77F656DA-696D-407c-BA1C-50E4457C12E8}"
TunerFriendlyName            = "Conexant 2388x Tuner"
TunerReferenceGuid           = "{5618011C-A4DA-455b-A448-EC2AF3DCCB02}"
BDATuneFriendlyName          = "Conexant 2388x BDA Tuner/Demod"
BDATuneReferenceGuid         = "{91B0CC87-9905-4d65-A0D1-5861C6F22CBF}"
TSFriendlyName               = "Conexant 2388x AVStream TS Capture"
TSReferenceGuid              = "{5ea9c066-1dfe-41c5-a2de-bf766e83c98e}"
