;==============================================================================
; TerraTec Cinergy 200/250 USB (Video)
; Driver Install Script for for Windows 2000 and XP
; Copyright (c) 2003-04, TerraTec Electronic GmbH
;------------------------------------------------------------------------------
; Notes:
;  a) Driver filenames must be <= 8 characters (8.3 format) !
;  b) Win9x: On Windows 98/Me, section names should be no longer than 28 characters.
;  c) Win9x: [SourceDisksNames] must always come before [SourceDisksFiles]  !!!   
;  d) Win9x: Filenames must be in 8.3 format  !              
;  e) Win9x: Registry pathes must use single slashes
;  f) [xxx.KnownFiles] sections are used by Win9x only
;  g) [xxx.Services] sections are used by WinNT only
;  h) If we have OS specific DDInstall sections we must have 
;     OS specific [xxx.Interfaces] and [.HW] also!
;  The Cinergy 200 USB supports TWAIN but not WIA
;------------------------------------------------------------------------------
; History:
; 15-Sep-03 First driver version 
; 02-Oct-03 v.0.99.0922.0
; 17-Mar-04 v.1.0.0208.1000
; 13-Apr-03 v.1.1.0323.0
;           Simplified INF file layout
;           Support for new TT 2820 revisions
; 14-Apr-04 v.1.1.0413.0
; 14-May-04 v.1.1.0428.0
; 24-May-04 v.1.1.0521.0
; 08-Jul-04 v.1.1.0708
;==============================================================================
;------------------------------------------------------------------
; 
;   emVideo.inf -- This file contains installation information
;                  for eMPIA USB 2.0 Video Devices:  EM27xx
;                  and EM28xx.
;           
;
;   This installation is for Windows 2000 and XP.
;
;   Copyright (C) eMPIA Technology, Inc.  2002-2004
;
;------------------------------------------------------------------

[Version]
Signature   = "$CHICAGO$"
Class       = Media        
ClassGUID   = {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider    = %Vendor%
CatalogFile = TT003601.cat
DriverVer   = 07/08/2004, 1.1.0708.0

[ControlFlags]
ExcludeFromSelect = *

[SourceDisksNames]
1 = %DiskLabel%,emDevice.sys,,

[SourceDisksFiles]
emProp.ax      = 1
emVFW.dll      = 1
emYUV.dll      = 1
emUSD.dll      = 1
emScan.sys     = 1
emFilter.sys   = 1
emDevice.sys   = 1
emStream.sys   = 1
emTwain.ds     = 1

[DestinationDirs]
DefaultDestDir = 11
CAP.CopyDLL    = 11
CAP.CopyEXE    = 10
CAP.CopySYS    = 10,system32\drivers
; FMB NOTE: subkey USB2800 is valid for all EM chip types; don't modify!
CAP.CopyTwain  = 10,twain_32\USB2800

[Manufacturer]
%Vendor% = Models

[Models]
;FMB NOTE: 2801/2821 are the composite devices with audio & video

; Cinergy 200 USB (2800/PAL)
%USB2800.DeviceDesc% = USB2800,USB\VID_EB1A&PID_2800
; Cinergy 250 USB (2820/PAL/EEPROM)
%USB0036.DeviceDesc% = USB0036,USB\VID_0CCD&PID_0036&MI_00
; Cinergy 250 USB (2820/PAL+SECAM/EEPROM)
%USB0037.DeviceDesc% = USB0037,USB\VID_0CCD&PID_0037&MI_00

; no EEPROM	 (Prototypes)
%USB2801.DeviceDesc% = USB2800,USB\VID_EB1A&PID_2801&MI_00
%USB2820.DeviceDesc% = USB2800,USB\VID_EB1A&PID_2820
%USB2821.DeviceDesc% = USB2800,USB\VID_EB1A&PID_2821&MI_00



;=====================  U S B 2 8 0 0  ====================
[USB2800.NT]
Include       = ks.inf, kscaptur.inf, ksfilter.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT
AddReg        = CAP.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2	; 1 for scanners, 2 for cameras, 3 for video devices
DeviceSubType = 0	; vendor defined value (optional)
Capabilities  = 1	; 1 - device generates events
DeviceData    = STI.DeviceData
Events        = STI.Events
ICMProfiles   = "sRGB Color Space Profile.icm"

;------------ H W ------------
[USB2800.NT.HW]
AddReg = InstFilter.AddReg

;------ S E R V I C E S ------
[USB2800.NT.Services]
AddService = DCamUSBEMPIA,0x00000002,DriverInstall
AddService = ScanUSBEMPIA,0x00000000,UpperInstall
AddService = FiltUSBEMPIA,0x00000000,LowerInstall

;---- I N T E R F A C E S ----
[USB2800.NT.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,   CAP.2800.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,   CAP.2800.Interface
AddInterface = %KSCATEGORY_TVTUNER%,GLOBAL,TVTuner.PAL.Interface
AddInterface = %KSCATEGORY_TVAUDIO%,GLOBAL,    TVAudio.Interface
AddInterface = %KSCATEGORY_XBAR%,   GLOBAL,       Xbar.Interface

;---- Capture interface ----
[CAP.2800.Interface]
AddReg = CAP.2800.AddReg

[CAP.2800.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,ExtensionDLL,,"emVFW.dll"
; FMB NOTE: FriendlyName and DSName must be identical for TWAIN for work!!!
HKR,,FriendlyName,,%USB2800.DeviceDesc%
HKLM,%Twain.Key%,DSName,0,%USB2800.DeviceDesc%

; IAMVideoCompression installed as static interface on both output pins
HKR,PinFactory\0\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
HKR,PinFactory\1\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}

;=====================  USB0036   ====================
[USB0036.NT]
Include       = ks.inf, kscaptur.inf, ksfilter.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT
AddReg        = CAP.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1 
Events        = STI.Events
DeviceData    = STI.DeviceData
ICMProfiles   = "sRGB Color Space Profile.icm"

;------------ H W ------------
[USB0036.NT.HW]
AddReg = InstFilter.AddReg

;------ S E R V I C E S ------
[USB0036.NT.Services]
;Include    = sti.inf
;Needs      = STI.USBSection.Services
AddService = DCamUSBEMPIA,0x00000002,DriverInstall
AddService = ScanUSBEMPIA,0x00000000,UpperInstall
AddService = FiltUSBEMPIA,0x00000000,LowerInstall

;---- I N T E R F A C E S ----
[USB0036.NT.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,   CAP.0036.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,   CAP.0036.Interface
AddInterface = %KSCATEGORY_TVTUNER%,GLOBAL,TVTuner.PAL.Interface
AddInterface = %KSCATEGORY_TVAUDIO%,GLOBAL,    TVAudio.Interface
AddInterface = %KSCATEGORY_XBAR%,   GLOBAL,       Xbar.Interface

;---- Capture interface ----
[CAP.0036.Interface]
AddReg = CAP.0036.AddReg

[CAP.0036.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,ExtensionDLL,,"emVFW.dll"
; FMB NOTE: FriendlyName and DSName must be identical for TWAIN to work!!!
HKR,,FriendlyName,,%USB0036.DeviceDesc%
HKLM,%Twain.Key%,DSName,0,%USB0036.DeviceDesc%
; IAMVideoCompression installed as static interface on both output pins
HKR,PinFactory\0\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
HKR,PinFactory\1\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}

;=====================  USB0037   ====================
[USB0037.NT]
Include       = ks.inf, kscaptur.inf, ksfilter.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT
AddReg        = CAP.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1
Events        = STI.Events
DeviceData    = STI.DeviceData
ICMProfiles   = "sRGB Color Space Profile.icm"

;------------ H W ------------
[USB0037.NT.HW]
AddReg = InstFilter.AddReg

;------ S E R V I C E S ------
[USB0037.NT.Services]
;Include    = sti.inf
;Needs      = STI.USBSection.Services
AddService = DCamUSBEMPIA,0x00000002,DriverInstall
AddService = ScanUSBEMPIA,0x00000000,UpperInstall
AddService = FiltUSBEMPIA,0x00000000,LowerInstall

;---- I N T E R F A C E S ----
[USB0037.NT.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,         CAP.0037.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,         CAP.0037.Interface
AddInterface = %KSCATEGORY_TVTUNER%,GLOBAL,TVTuner.PAL_SECAM.Interface
AddInterface = %KSCATEGORY_TVAUDIO%,GLOBAL,          TVAudio.Interface
AddInterface = %KSCATEGORY_XBAR%,   GLOBAL,             Xbar.Interface

;---- Capture interface ----
[CAP.0037.Interface]
AddReg = CAP.0037.AddReg

[CAP.0037.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,ExtensionDLL,,"emVFW.dll"
; FMB NOTE: FriendlyName and DSName must be identical for TWAIN to work!!!
HKR,,FriendlyName,,%USB0037.DeviceDesc%
HKLM,%Twain.Key%,DSName,0,%USB0037.DeviceDesc%
; IAMVideoCompression installed as static interface on both output pins
HKR,PinFactory\0\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
HKR,PinFactory\1\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}


;=========================  COMMON SECTION (TT) ==============


;-------------------------  Services  ------------------------
[DriverInstall]
DisplayName   = %Driver.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\emDevice.sys

[UpperInstall]
DisplayName   = %USBscan.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\emScan.sys

[LowerInstall]
DisplayName   = %emLower.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\emFilter.sys

;-------------------------  Filters  ------------------------
[InstFilter.AddReg]
HKR,,"UpperFilters",0x00010000,"ScanUSBEMPIA"
HKR,,"LowerFilters",0x00010000,"FiltUSBEMPIA"

;-------------------------  TV Tuner interface  ------------------------
[TVTuner.PAL.Interface]
AddReg = TVTuner.PAL.AddReg

[TVTuner.PAL.AddReg]
HKR,,CLSID,,%ProxyTVTuner.CLSID%
HKR,,FriendlyName,,%TVTuner.PAL.Name%

[TVTuner.PAL_SECAM.Interface]
AddReg = TVTuner.PAL_SECAM.AddReg

[TVTuner.PAL_SECAM.AddReg]
HKR,,CLSID,,%ProxyTVTuner.CLSID%
HKR,,FriendlyName,,%TVTuner.PAL_SECAM.Name%


;-------------------------  TV Audio interface  ------------------------
[TVAudio.Interface]
AddReg = TVAudio.AddReg

[TVAudio.AddReg]
HKR,,CLSID,,%ProxyTVAudio.CLSID%
HKR,,FriendlyName,,%TVAudio.Name%

;-------------------------  Crossbar interface  ------------------------
[Xbar.Interface]
AddReg = Xbar.AddReg

[Xbar.AddReg]
HKR,,CLSID,,%ProxyXbar.CLSID%
HKR,,FriendlyName,,%Xbar.Name%


;---------------------  C O M M O N  ----------------------

[CAP.AddReg]
HKR,,HardwareConfig,1,1
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,emDevice.sys
HKR,,OkToHibernate,3,1
HKR,,DontSuspendIfStreamsAreRunning,3,1 
HKR,,PageOutWhenUnopened,3,0
HKR,,PowerDownWhenUnopened,3,0

; ICustomCameraProp
HKCR,CLSID\{BE0AB5D2-3B9A-4e42-A05E-4A178B566C7C},,,%CustomPlugIn%
HKCR,CLSID\{BE0AB5D2-3B9A-4e42-A05E-4A178B566C7C}\InprocServer32,,,emProp.ax
HKCR,CLSID\{BE0AB5D2-3B9A-4e42-A05E-4A178B566C7C}\InprocServer32,ThreadingModel,,Both
; This IID is aggregated for the filter given the CLSID of the property set
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{BE0AB5D2-3B9A-4e42-A05E-4A178B566C7C},,,%CustomPlugIn%
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{BE0AB5D2-3B9A-4e42-A05E-4A178B566C7C},IID,1,D2,B5,0A,BE, 9a,3b, 42,4e, 0xa0, 0x5e, 0x4a, 0x17, 0x8b, 0x56, 0x6c, 0x7c

; CustomCamera Property Page
HKCR,CLSID\{7B37EDC5-0108-49b9-9CBC-46E826B23F7B},,,%CustomPropPage%
HKCR,CLSID\{7B37EDC5-0108-49b9-9CBC-46E826B23F7B}\InprocServer32,,,emProp.ax
HKCR,CLSID\{7B37EDC5-0108-49b9-9CBC-46E826B23F7B}\InprocServer32,ThreadingModel,,Both

; Associate property set with property page
HKLM,System\CurrentControlSet\Control\MediaSets\{BE0AB5D2-3B9A-4e42-A05E-4A178B566C7C}\PropertyPages\{7B37EDC5-0108-49b9-9CBC-46E826B23F7B},,,%CustomPropPage%

; Still Image
HKR,,USDClass,,"{95220838-61E0-47c0-B996-8461662A1598}"
HKCR,CLSID\{95220838-61E0-47c0-B996-8461662A1598} ,,,%StillUSD%
HKCR,CLSID\{95220838-61E0-47c0-B996-8461662A1598}\InProcServer32,,,%11%\emUSD.dll
HKCR,CLSID\{95220838-61E0-47c0-B996-8461662A1598}\InProcServer32,ThreadingModel,,"Both"

; FMB NOTE this section  is only used for USB2710/11 Win9x
[CAP.Sensor.AddReg]
; Register ePCCAP as a push-model application
HKLM,%STIRegistration%,%StillAPP%,,"%10%\ePCCAP.exe /StiDevice:%%1 /StiEvent:%%2"




[CAP.CopyDLL]
emUSD.dll
emVFW.dll
emYUV.dll
emProp.ax

[CAP.CopySYS]
emDevice.sys
emStream.sys
emScan.sys
emFilter.sys

[CAP.CopyTwain]
emTwain.ds

[CAP.CopyEXE]

[CAP.UpdateIni]
system.ini,drivers32,,"VIDC.I420=emYUV.dll"
system.ini,drivers32,,"VIDC.YUY2=emYUV.dll"

[STI.Events]
; FMB NOTE: * = use registered application
; FNB TEST ""
NewPicture = "%NewPicture%",{AF715AB9-8475-46da-9417-7E0BC349654E},*
SnapButton = "%SnapButton%",{FA69D8B1-D989-47d2-A5D2-A6635246098F},*

[STI.DeviceData]
TwainDS=%USBscan.DeviceDesc%


;-------------------------  O E M  ------------------------

; For hardware designs without EEPROM:  All OEM configuration data 
; in this section are active.
;
; For hardware designs with EEPROM:  FixupOWC, Optimization and OemID
; are specified in this section. All other configuration data in this 
; section will have no effects and should be spedified in EEPROM.
;
; OemID is the vendor ID from EEPROM, but can be overridden here.
;
[OEM.AddReg]
HKR,settings\OEMSettings,Optimization,0x00010001,1          ; 1=ISO, 2=Bulk
HKR,settings\OEMSettings,FixUpOWC,0x00010001,12
HKR,settings\OEMSettings,EnablePAL640x576,0x00010001,0      ; For 2820/2840
HKR,settings\OEMSettings,OemID            ,0x00010001,0x0ccd; TerraTec USB Vendor ID
;;;HKR,settings\OEMSettings,PowerControl,0x00010001,0

; Board Configurations
HKR,settings\OEMSettings,Composite  ,0x00010001,1           ; Composite Input
HKR,settings\OEMSettings,SVideo     ,0x00010001,1           ; S-Video Input
HKR,settings\OEMSettings,SonyOnBoard,0x00010001,0           ; Sony Modules    

; Driver Configurations
HKR,settings\OEMSettings,StrictI2cAccess  ,0x00010001,0     ; 0=Normal, 1=Strict
HKR,settings\OEMSettings,VideoSwitchMode  ,0x00010001,1     ; 0=Freeze, 1=Blackout
HKR,settings\OEMSettings,EnableSquarePixel,0x00010001,1     ; 1=enabled
HKR,settings\OEMSettings,Enable704        ,0x00010001,0     ; 1=enabled
HKR,settings\OEMSettings,EnableUSB1CMOS640,0x00010001,1     ; 1=enabled
HKR,settings\OEMSettings,FixupDecoderStd  ,0x00010001,1     ; 1=enabled
HKR,settings\OEMSettings,GPIObyAP         ,0x00010001,0     ;
HKR,settings\OEMSettings,TVTuneByAP       ,0x00010001,0     ;

; OEM Devices Accessed from Applications Directly.
; FMB NOTE: NEC Remote Control Decoder (IIC address 0x60)
HKR,settings\OEMSettings,Oem0I2C ,0x00010001,0x60
HKR,settings\OEMSettings,Oem0Type,0x00010001,2
HKR,settings\OEMSettings,Oem1I2C ,0x00010001,0x60
HKR,settings\OEMSettings,Oem1Type,0x00010001,2
HKR,settings\OEMSettings,Oem2I2C ,0x00010001,0x60
HKR,settings\OEMSettings,Oem2Type,0x00010001,2
HKR,settings\OEMSettings,Oem3I2C ,0x00010001,0x60
HKR,settings\OEMSettings,Oem3Type,0x00010001,2

;------------------------------------------------------
; Tuner CFG & Overrides
;------------------------------------------------------
; FMB NOTE: The Tuner IDs are 
;   - 12 for TALN_M200T (Cinergy 200 USB) and 
;   - 15 for TALN-S200T
;; RP NOTE TunerIDBase must be set to 8 for Cinergy 200 USB (w/o EEPROM) to get tuner running 
HKR,settings\OEMSettings,TunerIDBase,0x00010001,8
;;;HKR,settings\OEMSettings,TunerID7   ,0x00010001,12        ; FMB NOTE: use this line or not?

; USB/Ext Audio Mux - 2820/2840 Only
;;;HKR,settings\OEMSettings,USBAudioMux,0x00010001,1
;;;HKR,settings\OEMSettings,ExtAudioMux,0x00010001,2


;------------------------------------------------------
; OEM Property Defaults:
;------------------------------------------------------
; This section provides property defaults for the WDM driver.
;
; If EEPROM is on board, some of these property defaults are provided
; by EEPROM. The remaining perperty defaults are specified here.
;
; A property default is only meaningful if the corresponding property
; is not yet defined in the system registry.
;
[OEM.Defaults.AddReg]

; Default Video ProcAmp for Sensor-only or Decoder-only devices.
; Brightness[0..255], Contrast[0..63], Hue[0..127], Saturation[0..63]
; Hue control for decoder only. No Hue control for Sensor


HKR,settings\PropDefaults,Brightness,0x00010001,128         ;
HKR,settings\PropDefaults,Contrast,0x00010001,32            ;
HKR,settings\PropDefaults,Hue,0x00010001,64                 ;
HKR,settings\PropDefaults,Saturation,0x00010001,32          ;
HKR,settings\PropDefaults,Sharpness,0x00010001,2            ;
HKR,settings\PropDefaults,Gamma,0x00010001,50               ;

HKR,settings\PropDefaults,Mirror,0x00010001,0               ; 0=OFF, 1=ON
HKR,settings\PropDefaults,Flip,0x00010001,0                 ; 0=OFF, 1=ON
HKR,settings\PropDefaults,AutoExposure,0x00010001,1         ; 0=OFF, 1=ON
HKR,settings\PropDefaults,AEMode,0x00010001,1               ; 0=Dark, 1=Normal
HKR,settings\PropDefaults,AE_Level,0x00010001,3             ; Target AE (0-6)        
HKR,settings\PropDefaults,Exposure,0x00010001,4             ;
HKR,settings\PropDefaults,LightTemperature,0x00010001,0     ;
HKR,settings\PropDefaults,LightFreq,0x00010001,1            ; 0=60Hz, 1=50Hz
HKR,settings\PropDefaults,AutoWhiteBalance,0x00010001,1     ; 0=OFF , 1=ON
HKR,settings\PropDefaults,AWB_R,0x00010001,32               ;
HKR,settings\PropDefaults,AWB_B,0x00010001,32               ;
HKR,settings\PropDefaults,WindowSize,0x00010001,0           ; 0=640x480, 1=320x240, 2=1280x960
HKR,settings\PropDefaults,MonitorType,0x00010001,0          ; 0=CRT,  1=LCD

HKR,settings\PropDefaults,VideoStandard,0x00010001,0x10     ; 1=NTSC, 0x10=PAL_B, 0x40000=SECAM_L
HKR,settings\PropDefaults,Deinterlace,0x00010001,1          ; 1=Weave, 2=Bob
HKR,settings\PropDefaults,VCRMask,0x00010001,2              ; # of lines masked out
HKR,settings\PropDefaults,MaskColor,0x00010001,1            ; 0=Gray, 1=Black



;--------------------- S T R I N G S -----------------------

[Strings]
;---------------
;Non-Localizable
;---------------  
ImageClassGUID     = "{6bdd1fc6-810f-11d0-bec7-08002be2092f}"
MediaClassGUID     = "{4d36e96c-e325-11ce-bfc1-08002be10318}"

KSCATEGORY_CAPTURE = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO   = "{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_TVTUNER = "{a799a800-a46d-11d0-a18c-00a02401dcd4}"
KSCATEGORY_TVAUDIO = "{a799a802-a46d-11d0-a18c-00a02401dcd4}"
KSCATEGORY_XBAR    = "{a799a801-a46d-11d0-a18c-00a02401dcd4}"

ProxyVCap.CLSID    = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
ProxyTVTuner.CLSID = "{266EEE40-6C63-11cf-8A03-00AA006ECB65}"
ProxyTVAudio.CLSID = "{71F96462-78F3-11d0-A18C-00A0C9118956}"
ProxyXbar.CLSID    = "{71F96460-78F3-11d0-A18C-00A0C9118956}"

Twain.Key          = "Software\USB2800\TwainDS"
CustomPlugIn       = "emProp Custom Interface"
CustomPropPage     = "emProp Custom Property Page"
StillUSD           = "USB Still Image USD"
STIRegistration    = "Software\Microsoft\Windows\CurrentVersion\StillImage\Registered Applications"

;---------------
;Localizable
;---------------
Vendor             = "TerraTec Electronic GmbH"
DiskLabel          = "TerraTec Driver Disk"

NewPicture         = "New Picture Requested"
SnapButton         = "Snapshot Button Pressed"

Driver.DeviceDesc  = "Cinergy 200/250 USB Video Capture"
USBscan.DeviceDesc = "Cinergy 200/250 USB Still Image"
emLower.DeviceDesc = "Cinergy 200/250 USB Lower Filter"

USB2800.DeviceDesc = "Cinergy 200 USB Video"
USB2801.DeviceDesc = "Cinergy 200 USB Video (2801)"
USB2820.DeviceDesc = "Cinergy 250 USB Video (2820)"
USB2821.DeviceDesc = "Cinergy 250 USB Video (2821)"
USB0036.DeviceDesc = "Cinergy 250 USB Video (PAL)"
USB0037.DeviceDesc = "Cinergy 250 USB Video (PAL/SECAM)"

TVTuner.PAL.Name        = "Cinergy 200/250 USB Tuner (PAL)"
TVTuner.PAL_SECAM.Name  = "Cinergy 200/250 USB Tuner (PAL/SECAM)"
TVAudio.Name            = "Cinergy 200/250 USB TVAudio"
Xbar.Name               = "Cinergy 200/250 USB Crossbar"
