;-------------------------------------------------------------------------------
;
; Motorola Android (Mot) USB Bulk device (motoandroid.inf)
;
; Copyright (c) 2009-2014 Motorola
;
;-------------------------------------------------------------------------------
[Version]
Signature="$WINDOWS NT$"
Class=USB
ClassGuid={F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}
Provider=%Motorola%
DriverVer= 11/08/2011, 1.2.9.0
CatalogFile=motoandroid.cat

; ================= Class section =====================

[ClassInstall32]
Addreg=AndroidUsbClassReg

[AndroidUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-5

[DestinationDirs]
DefaultDestDir = 12

; ================= Device section =====================

[Manufacturer]
%Motorola% = Motorola,NTamd64

; For Win2K
[Motorola]

; t qc
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2E16&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2E18&MI_00
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2E1A&MI_02

; g2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41C7&MI_02

; p qc
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_2DF1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DF3&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DF5&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DF7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DF9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DFB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DFD&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DFF&MI_05
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2E02&MI_02
; o4
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4311&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_433B&MI_02

; o4-1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4313&MI_03
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4314&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4315&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4317&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4319&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_431B&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_431D&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_431F&MI_06
; o4-2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4330&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4331&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4333&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4335&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4337&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4339&MI_02
; dq+
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DE6&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DE8&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DE9&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DEA&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DEB&MI_02

; h nV
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70AB&MI_04
; et
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7094&MI_09
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7096&MI_0B
; ev
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70B1&MI_07
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70B3&MI_09
; t o4
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_42F1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42F3&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42F5&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42F7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42F9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42FB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42FD&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4302&MI_09
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4304&MI_0B
; s o4
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_42D1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42D3&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42D5&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42D7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42D9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42DB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42DD&MI_02
; d nV
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_70C1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70C3&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70C5&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70C7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70C9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70CB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70CD&MI_02

; e
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_18D1&PID_708C
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_18D1&PID_70AC
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70A2&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70A9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70AF&MI_02

; o3
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C1&MI_01
; o,e
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7090&MI_01
; g
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41C3&MI_01
; ft
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41E5&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7092&MI_02

; g,o3 
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41E7&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41E9&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41EA&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41EC&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41ED&MI_03
; c
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DD3&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DD4&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DD5&MI_02
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_2DD9
; o/e,e
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7080&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7082&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7087&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7089&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_708B&MI_04
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_708C
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_70AC
; s
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4284&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4286&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4289&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_428B&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_428C&MI_01
; d2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42A2&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42A4&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42A7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42A9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42AA&MI_01
; dp
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42B2&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42B4&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42B7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42B9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42BA&MI_01
; v2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C2&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C4&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42CA&MI_01
;Calgary
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D7B&MI_03

; For loopback testing
%USB\VID_18D1&PID_DDDD.DeviceDescTest%=motandroidusb.Dev, USB\VID_18D1&PID_DDDD
; Android Sooner
%USB\VID_18D1&PID_D00D.DeviceDescRelease%=motandroidusb.Dev, USB\VID_18D1&PID_D00D
%USB\VID_18D1&PID_DEED&MI_01.DeviceDescRelease%=motandroidusb.Dev, USB\VID_18D1&PID_DEED&MI_01
%USB\VID_18D1&PID_DEED&MI_02.DeviceDescRelease%=motandroidusb.Dev, USB\VID_18D1&PID_DEED&MI_02
;Calgary
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D74&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D75&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D76&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D7B&MI_03

;Morrison
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_2D62
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D61&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D64&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D66&MI_00
;sholes umts
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_41D1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41D2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41DA&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41DB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41DC&MI_01
;Sholes CDMA
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41DB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41E2&MI_04
; test
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41EE&MI_09

;Morrison/Motus/Zepplin
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D68&MI_01


[Motorola.NTamd64]

; t qc
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2E16&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2E18&MI_00
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2E1A&MI_02

; g2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41C7&MI_02

; p qc
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_2DF1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DF3&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DF5&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DF7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DF9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DFB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DFD&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DFF&MI_05
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2E02&MI_02
; o4
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4311&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_433B&MI_02

; o4-1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4313&MI_03
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4314&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4315&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4317&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4319&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_431B&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_431D&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_431F&MI_06
; o4-2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4330&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4331&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4333&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4335&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4337&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4339&MI_02
; dq+
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DE6&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DE8&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DE9&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DEA&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DEB&MI_02

; h nV
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70AB&MI_04
; et
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7094&MI_09
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7096&MI_0B
; ev
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70B1&MI_07
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70B3&MI_09
; t o4
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_42F1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42F3&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42F5&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42F7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42F9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42FB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42FD&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4302&MI_09
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4304&MI_0B
; s o4
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_42D1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42D3&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42D5&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42D7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42D9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42DB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42DD&MI_02
; d nV
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_70C1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70C3&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70C5&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70C7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70C9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70CB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70CD&MI_02

; e
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_18D1&PID_708C
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_18D1&PID_70AC
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70A2&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70A9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_70AF&MI_02

; o3
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C1&MI_01
; o,e
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7090&MI_01
; g
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41C3&MI_01
; ft
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41E5&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7092&MI_02

; g,o3 
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41E7&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41E9&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41EA&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41EC&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41ED&MI_03
; c
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DD3&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DD4&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2DD5&MI_02
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_2DD9
; o/e,e
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7080&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7082&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7087&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_7089&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_708B&MI_04
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_708C
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_70AC
; s
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4284&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4286&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_4289&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_428B&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_428C&MI_01
; d2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42A2&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42A4&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42A7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42A9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42AA&MI_01
; dp
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42B2&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42B4&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42B7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42B9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42BA&MI_01
; v2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C2&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C4&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C7&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42C9&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_42CA&MI_01
;Calgary
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D7B&MI_03

; For loopback testing
%USB\VID_18D1&PID_DDDD.DeviceDescTest%=motandroidusb.Dev, USB\VID_18D1&PID_DDDD
; Android Sooner
%USB\VID_18D1&PID_D00D.DeviceDescRelease%=motandroidusb.Dev, USB\VID_18D1&PID_D00D
%USB\VID_18D1&PID_DEED&MI_01.DeviceDescRelease%=motandroidusb.Dev, USB\VID_18D1&PID_DEED&MI_01
%USB\VID_18D1&PID_DEED&MI_02.DeviceDescRelease%=motandroidusb.Dev, USB\VID_18D1&PID_DEED&MI_02
;Calgary
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D74&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D75&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D76&MI_02
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D7B&MI_03

;Morrison
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_2D62
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D61&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D64&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D66&MI_00
;sholes umts
%MotSingleInterface%    = motandroidusb.Dev, USB\VID_22B8&PID_41D1
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41D2
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41DA&MI_04
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41DB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41DC&MI_01
;Sholes CDMA
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41DB&MI_01
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41E2&MI_04
; test
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_41EE&MI_09
;Morrison/Motus/Zepplin
%MotCompositeInterface% = motandroidusb.Dev, USB\VID_22B8&PID_2D68&MI_01

[motandroidusb.Dev.NT]
CopyFiles=motandroidusb.Files.Ext

[motandroidusb.Dev.NT.Services]
Addservice = motandroidusb, 0x00000002, motandroidusb.AddService

[motandroidusb.AddService]
DisplayName    = %motandroidusb.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\motoandroid.sys
AddReg         = motandroidusb.AddReg
LoadOrderGroup = Base

[motandroidusb.AddReg]
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2
HKR, Parameters\Wdf, VerboseOn,       0x00010001, 1
HKR, Parameters\Wdf, VerifierOn,      0x00010001, 1
HKR, Parameters\Wdf, DbgBreakOnError, 0x00010001, 1

[motandroidusb.Files.Ext]
motoandroid.sys

[SourceDisksNames]
1=%Disk_Description%,,,

[SourceDisksFiles]
motoandroid.sys = 1

;-------------- WDF Coinstaller installation
[DestinationDirs]
CoInstaller_CopyFiles = 11

[motandroidusb.Dev.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
wdfcoinstaller01007.dll

[SourceDisksFiles]
wdfcoinstaller01007.dll=1 ; make sure the number matches with SourceDisksNames

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "wdfcoinstaller01007.dll,WdfCoInstaller"

[motandroidusb.Dev.NT.Wdf]
KmdfService = motandroidusb, motandroidusb_wdfsect

[motandroidusb_wdfsect]
KmdfLibraryVersion = 1.7

;---------------------------------------------------------------;

[Strings]
Motorola                = "Motorola"
Disk_Description        = "ADB Interface Installation Disk"
motandroidusb.SvcDesc      = "Mot ADB Interface Driver"
ClassName               = "ADB Interface"
USB\VID_18D1&PID_DDDD.DeviceDescTest="Android Sooner ADB Testing Interface"
USB\VID_18D1&PID_D00D.DeviceDescRelease="Android Sooner Single ADB Interface"
USB\VID_18D1&PID_DEED&MI_01.DeviceDescRelease="Android Sooner Composite ADB Interface"
USB\VID_18D1&PID_DEED&MI_02.DeviceDescRelease="Android Sooner Kernel Debug Interface"
MotSingleInterface		= "Mot Single ADB Interface"
MotCompositeInterface	= "Mot Composite ADB Interface"
