;-------------------------------------------------------------------------------
;
; Installation inf for Coolpad Android USB Bulk device
;
; Copyright (c) 2009-2014 YuLong
;
;-------------------------------------------------------------------------------
[Version]
Signature="$WINDOWS NT$"
Class=USB
ClassGuid={F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}
Provider=%YuLong%
DriverVer=04/18/2010,2.1.0.1
CatalogFile=cp_android_adb.cat

; ================= Class section =====================

[ClassInstall32]
Addreg=AndroidUsbClassReg

[AndroidUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1

[DestinationDirs]
DefaultDestDir = 12

; ================= Device section =====================

[Manufacturer]
%YuLong% = YuLong,NTx86,NTamd64

; For Win2K
[YuLong]
; Coolpad M1
%SingleAdbInterface%        = androidusb.Dev, USB\VID_18D1&PID_0001
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_18D1&PID_0002&MI_01
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6001
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&PID_6002&MI_01

;0:MSC/MTP,1:MSC/MTP,2:MODEM,4:ADB
;Coolpad N930
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6005&MI_04

%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6008&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6009&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600A&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600B&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600C&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600D&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600E&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600F&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6010&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6011&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6012&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6013&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6014&MI_04


;0:MSC/MTP,1:MSC/MTP,2:ADB,3:MODEM
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601A&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601B&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601C&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601D&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601E&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601F&MI_02


;Single ADB
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6020
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6021

;0:MSC/MTP,1:MODEM,3:ADB
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6025&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6026&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6027&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6028&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6029&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602A&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602B&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602C&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602D&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602E&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602F&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6030&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6031&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6032&MI_03


;0:MSC,1:ADB,2:MODEM
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603A&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603B&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603C&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603D&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603E&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603F&MI_01


;Single ADB
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6040
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6041


;0:MSC,1:MODEM,3:PUIA,4:NMEA,5:DIAGNOSE,6:ADB
;Coolpad D530
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6045&MI_06

%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6046&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6047&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6048&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6049&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604A&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604B&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604C&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604D&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604E&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604F&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6050&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6051&MI_06


;0:MSC/MTP,1:MSC/MTP,2:MODEM,4:PUIA,5:NMEA,6:DIAGNOSE,7:ADB
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6058&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6059&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605A&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605B&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605C&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605D&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605E&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605F&MI_07


;Single ADB
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_606B
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_606C
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_606D


;Coolpad Qualcomm Android
%SingleAdbInterface%        = androidusb.Dev, USB\VID_18D1&PID_D00D

;Coolpad 9060
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_0237
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_0235&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&PID_0236&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_0238&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_0239&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023A&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023B&MI_05
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023C&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023D&MI_03

;Coolpad Marvin Android
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&PID_0231&MI_03

; For XP and later
[YuLong.NTx86]
; Coolpad M1
%SingleAdbInterface%        = androidusb.Dev, USB\VID_18D1&PID_0001
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_18D1&PID_0002&MI_01
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6001
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&PID_6002&MI_01

;0:MSC/MTP,1:MSC/MTP,2:MODEM,4:ADB
;Coolpad N930
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6005&MI_04

%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6008&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6009&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600A&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600B&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600C&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600D&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600E&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600F&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6010&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6011&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6012&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6013&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6014&MI_04


;0:MSC/MTP,1:MSC/MTP,2:ADB,3:MODEM
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601A&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601B&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601C&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601D&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601E&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601F&MI_02


;Single ADB
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6020
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6021

;0:MSC/MTP,1:MODEM,3:ADB
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6025&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6026&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6027&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6028&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6029&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602A&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602B&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602C&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602D&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602E&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602F&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6030&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6031&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6032&MI_03


;0:MSC,1:ADB,2:MODEM
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603A&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603B&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603C&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603D&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603E&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603F&MI_01


;Single ADB
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6040
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6041


;0:MSC,1:MODEM,3:PUIA,4:NMEA,5:DIAGNOSE,6:ADB
;Coolpad D530
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6045&MI_06

%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6046&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6047&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6048&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6049&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604A&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604B&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604C&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604D&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604E&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604F&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6050&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6051&MI_06


;0:MSC/MTP,1:MSC/MTP,2:MODEM,4:PUIA,5:NMEA,6:DIAGNOSE,7:ADB
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6058&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6059&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605A&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605B&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605C&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605D&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605E&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605F&MI_07


;Single ADB
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_606B
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_606C
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_606D


;Coolpad Qualcomm Android
%SingleAdbInterface%        = androidusb.Dev, USB\VID_18D1&PID_D00D

;Coolpad 9060
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_0237
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_0235&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&PID_0236&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_0238&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_0239&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023A&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023B&MI_05
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023C&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023D&MI_03

;Coolpad Marvin Android
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&PID_0231&MI_03

[YuLong.NTamd64]
; Coolpad M1
%SingleAdbInterface%        = androidusb.Dev, USB\VID_18D1&PID_0001
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_18D1&PID_0002&MI_01
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6001
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&PID_6002&MI_01

;0:MSC/MTP,1:MSC/MTP,2:MODEM,4:ADB
;Coolpad N930
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6005&MI_04

%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6008&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6009&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600A&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600B&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600C&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600D&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600E&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_600F&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6010&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6011&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6012&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6013&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6014&MI_04


;0:MSC/MTP,1:MSC/MTP,2:ADB,3:MODEM
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601A&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601B&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601C&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601D&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601E&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_601F&MI_02


;Single ADB
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6020
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6021

;0:MSC/MTP,1:MODEM,3:ADB
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6025&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6026&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6027&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6028&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6029&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602A&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602B&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602C&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602D&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602E&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_602F&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6030&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6031&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6032&MI_03


;0:MSC,1:ADB,2:MODEM
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603A&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603B&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603C&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603D&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603E&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_603F&MI_01


;Single ADB
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6040
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_6041


;0:MSC,1:MODEM,3:PUIA,4:NMEA,5:DIAGNOSE,6:ADB
;Coolpad D530
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6045&MI_06

%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6046&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6047&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6048&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6049&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604A&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604B&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604C&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604D&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604E&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_604F&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6050&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6051&MI_06


;0:MSC/MTP,1:MSC/MTP,2:MODEM,4:PUIA,5:NMEA,6:DIAGNOSE,7:ADB
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6058&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_6059&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605A&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605B&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605C&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605D&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605E&MI_07
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_605F&MI_07


;Single ADB
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_606B
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_606C
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_606D


;Coolpad Qualcomm Android
%SingleAdbInterface%        = androidusb.Dev, USB\VID_18D1&PID_D00D

;Coolpad 9060
%SingleAdbInterface%        = androidusb.Dev, USB\VID_1EBF&PID_0237
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_0235&MI_01
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&PID_0236&MI_06
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_0238&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_0239&MI_03
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023A&MI_04
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023B&MI_05
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023C&MI_02
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&Pid_023D&MI_03

;Coolpad Marvin Android
%CompositeAdbInterface%     = androidusb.Dev, USB\VID_1EBF&PID_0231&MI_03

[androidusb.Dev.NT]
CopyFiles=androidusb.Files.Ext

[androidusb.Dev.NT.Services]
Addservice = androidusb, 0x00000002, androidusb.AddService

[androidusb.AddService]
DisplayName    = %androidusb.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\androidusb.sys
AddReg         = androidusb.AddReg
LoadOrderGroup = Base

[androidusb.AddReg]
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2
HKR, Parameters\Wdf, VerboseOn,       0x00010001, 1
HKR, Parameters\Wdf, VerifierOn,      0x00010001, 1
HKR, Parameters\Wdf, DbgBreakOnError, 0x00010001, 1

[androidusb.Files.Ext]
androidusb.sys

[SourceDisksNames]
1 = %Disk_Description%,,,\i386
2 = %Disk_Description%,,,\amd64

[SourceDisksFiles.x86]
WdfCoInstaller01007.dll = 1
androidusb.sys = 1

[SourceDisksFiles.amd64]
WdfCoInstaller01007.dll = 2
androidusb.sys = 2

;-------------- WDF Coinstaller installation
[DestinationDirs]
CoInstaller_CopyFiles = 11

[androidusb.Dev.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
wdfcoinstaller01007.dll


[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "wdfcoinstaller01007.dll,WdfCoInstaller"

[androidusb.Dev.NT.Wdf]
KmdfService = androidusb, androidusb_wdfsect

[androidusb_wdfsect]
KmdfLibraryVersion = 1.7


;---------------------------------------------------------------;

[Strings]
YuLong                = "YuLong"
Disk_Description        = "Coolpad ADB Interface Installation Disk"
androidusb.SvcDesc      = "Coolpad ADB Interface Driver"
ClassName               = "ADB Interface"

SingleAdbInterface="Coolpad Single ADB Interface"
CompositeAdbInterface="Coolpad Composite ADB Interface"
