;; Modded by Pieter @ www.laptopvideo2go.com v1.31

; /****************************************************************************
; * Copyright 2006 Atheros Communications Inc., all rights reserved.          *
; * INF file for Atheros reference designs                                    *
; ****************************************************************************/

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
LoutFiles   = layout.inf
CatalogFile = athrextx.cat
DriverVer   = 11/05/2010,9.2.0.105

[Manufacturer]
%ATHEROS%     = Atheros, NTamd64.6.1, NTamd64.6.0

[ControlFlags]
ExcludeFromSelect = *

[Atheros.NTamd64.6.1]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ATHER.DeviceDesc.0013%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_0013
%ATHER.DeviceDesc.0013%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_0014
%ATHER.DeviceDesc.0013%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_0015
%ATHER.DeviceDesc.0013%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_0016
%ATHER.DeviceDesc.0013%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_0017
%ATHER.DeviceDesc.0013%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_0018
%ATHER.DeviceDesc.0013%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_0019
%ATHER.DeviceDesc.001A%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_001A
%ATHER.DeviceDesc.001B%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_001B
%ATHER.DeviceDesc.001B%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_001C
%ATHER.DeviceDesc.001B%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_FF19
%ATHER.DeviceDesc.001D%  = ATHER_DEV_OS61_0013.ndi,    PCI\VEN_168C&DEV_001D
%ATHER.DeviceDesc.0023%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_0023
%ATHER.DeviceDesc.0023%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_0024
%ATHER.DeviceDesc.0023%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_FF1C
%ATHER.DeviceDesc.0023%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_FF1D
%ATHER.DeviceDesc.0029%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_0029
%ATHER.DeviceDesc.002A%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_002A
%ATHER.DeviceDesc.002B%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_002B
%ATHER.DeviceDesc.002C%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_002C
%ATHER.DeviceDesc.002D%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_002D
%ATHER.DeviceDesc.002E%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_002E
%ATHER.DeviceDesc.0030%  = ATHER_DEV_OS61_0023.ndi,    PCI\VEN_168C&DEV_0030
%ATHER.DeviceDesc.0032%  = ATHER_DEV_OS61_0032.ndi,    PCI\VEN_168C&DEV_0032

[Atheros.NTamd64.6.0]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0014
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0015
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0016
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0017
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0018
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0019
%ATHER.DeviceDesc.001A%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_001A
%ATHER.DeviceDesc.001B%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_001B
%ATHER.DeviceDesc.001B%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_001C
%ATHER.DeviceDesc.001B%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_FF19
%ATHER.DeviceDesc.001D%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_001D
%ATHER.DeviceDesc.0023%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_0023
%ATHER.DeviceDesc.0023%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_0024
%ATHER.DeviceDesc.0023%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_FF1C
%ATHER.DeviceDesc.0023%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_FF1D
%ATHER.DeviceDesc.0029%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_0029
%ATHER.DeviceDesc.002A%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_002A
%ATHER.DeviceDesc.002B%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_002B
%ATHER.DeviceDesc.002C%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_002C
%ATHER.DeviceDesc.002D%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_002D
%ATHER.DeviceDesc.002E%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_002E
%ATHER.DeviceDesc.0030%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_0030
%ATHER.DeviceDesc.0032%  = ATHER_DEV_0032.ndi,    PCI\VEN_168C&DEV_0032

; OS 6.1 Manufacturer section

[ATHER_DEV_OS61_0013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg,11n.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHER_DEV_OS61_0013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHER_DEV_OS61_0013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHER_DEV_OS61_0023.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg,11n.reg, 20-40mhz
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHER_DEV_OS61_0023.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHER_DEV_OS61_0023.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHER_DEV_OS61_0032.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg,11n.reg, 20-40mhz, 9485BTcoex.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHER_DEV_OS61_0032.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHER_DEV_OS61_0032.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

; OS 6.0 Manufacturer section

[ATHER_DEV_0013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg,11n.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHER_DEV_0013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHER_DEV_0023.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg,11n.reg, 20-40mhz
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHER_DEV_0023.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[ATHER_DEV_0032.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os60.reg,11n.reg, 20-40mhz, 9485BTcoex.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHER_DEV_0032.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog

[atheros_os61.reg]
HKR, Ndi,                           Service,    0, "athr"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet,vwifi"

HKR, Ndi\IHVExtensions, ExtensibilityDLL, 0, %%SystemRoot%%\system32\athihvs.dll
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID, 0, "{4A31B2F3-8714-4236-8B6F-5BA745A04AB7}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Atheros IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI, 0x00010001, 0x00037f

[atheros_os60.reg]
HKR, Ndi,                           Service,    0, "athr"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet"

HKR, Ndi\IHVExtensions, ExtensibilityDLL, 0, %%SystemRoot%%\system32\athihvs.dll
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID, 0, "{4A31B2F3-8714-4236-8B6F-5BA745A04AB7}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Atheros IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI, 0x00010001, 0x00037f

[atheros.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,halPcieClockReq
HKR,Ndi\params,MapRegisters,0x2000
HKR,,MapRegisters
HKR,Ndi\params,radioEnable,0x2000
HKR,Ndi\params,sleepMode,0x2000
HKR,,sleepMode
HKR,,gpioFunc0ActHi
HKR,,gpioFunc1ActHi
HKR,,gpioLedCustom
HKR,,gpioPinFunc0
HKR,,gpioPinFunc1
HKR,,transmitRateMax
HKR, Ndi\params\*TransmitBuffers
HKR,,*TransmitBuffers
HKR,,rxChainMask
HKR,,txChainMaskLegacy
HKR,,rxChainMaskLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR, Ndi\params\smpsDynamic
HKR,,d3forcel1disable.reg
HKR,,d3forcel1disablekite.reg
HKR,,d3forcel1disablekite1.reg
HKR,,wmeEnabled
HKR,,halPcieWaen
HKR,,halPcieDetach
HKR,,ampEnable
HKR,Ndi\IHVExtensions
HKR,,roamPolicy
HKR,,btCoexAntDivEnable

;;Customized Section

[11n.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "14"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  forceWake,                 	0x00002,  "1"

HKR,,                                   linkLEDFunc,                    0,        "35"
HKR, ,                                  swapDefaultLED,                 0x00002,  "1"
;-----------------------------------------------------------------------------
;;Customized Section

HKR, Ndi\params\GreenTx,                ParamDesc,                      0,        %GreenTx%
HKR, Ndi\params\GreenTx,                Base,                           0,        "10"
HKR, Ndi\params\GreenTx,                default,                        0,        "0"
HKR, Ndi\params\GreenTx,                type,                           0,        "enum"
HKR, Ndi\params\GreenTx\enum,           "0",                            0,        %GreenTxEnableOff%
HKR, Ndi\params\GreenTx\enum,           "1",                            0,        %GreenTxEnableOn%

HKR, ,                                  ampEnable,                      0x00002,  "1"
HKR, Ndi\params\ampEnable,              ParamDesc,                      0,        %bt30%
HKR, Ndi\params\ampEnable,              default,                        0,        "1"
HKR, Ndi\params\ampEnable,              type,                           0,        "enum"
HKR, Ndi\params\ampEnable\enum,         "1",                            0,        %bt30enable%
HKR, Ndi\params\ampEnable\enum,         "0",                            0,        %bt30disable%

HKR, NDI\params\htAdhocEnable,ParamDesc,,	%AdHoc11n%
HKR, NDI\params\htAdhocEnable,type,,		"enum"
HKR, NDI\params\htAdhocEnable,Default,,	        "0"
HKR, NDI\params\htAdhocEnable\enum,0,,	        %Disable%
HKR, NDI\params\htAdhocEnable\enum,1,,	        %Enable%

HKR, Ndi\params\smpsDynamic,            ParamDesc,                      0,  %smpsDynamic%
HKR, Ndi\params\smpsDynamic,            Base,                           0,  "10"
HKR, Ndi\params\smpsDynamic,            default,                        0,  "0"
HKR, Ndi\params\smpsDynamic,            type,                           0,  "enum"
HKR, Ndi\params\smpsDynamic\enum,       "1",                            0,  %Enable%
HKR, Ndi\params\smpsDynamic\enum,       "0",                            0,  %Disable%

HKR, Ndi\params\defaultIbssChannel,     ParamDesc,                      0,        %adhocchannel%
HKR, Ndi\params\defaultIbssChannel,     default,                        0,        "10"
HKR, Ndi\params\defaultIbssChannel,     min,                            0,        "1"
HKR, Ndi\params\defaultIbssChannel,     max,                            0,        "14"
HKR, Ndi\params\defaultIbssChannel,     step,                           0,        "1"
HKR, Ndi\params\defaultIbssChannel,     base,                           0,        "10"
HKR, Ndi\params\defaultIbssChannel,     type,                           0,        "int"

HKR, NDI\params\ignore11dBeacon,ParamDesc,,	%Mode11d%
HKR, NDI\params\ignore11dBeacon,type,,		"enum"
HKR, NDI\params\ignore11dBeacon,Default,,	"1"
HKR, NDI\params\ignore11dBeacon\enum,0,,		%Mode11dEnable%
HKR, NDI\params\ignore11dBeacon\enum,1,,		%Mode11dDisable%

HKR, Ndi\params\tpc,                    ParamDesc,                      0,  %tpc%
HKR, Ndi\params\tpc,                    Base,                           0,  "10"
HKR, Ndi\params\tpc,                    default,                        0,  "0"
HKR, Ndi\params\tpc,                    type,                           0,  "enum"
HKR, Ndi\params\tpc\enum,               "0",                            0,  %tpc100%
HKR, Ndi\params\tpc\enum,               "1",                            0,  %tpc50%
HKR, Ndi\params\tpc\enum,               "2",                            0,  %tpc25%
HKR, Ndi\params\tpc\enum,               "3",                            0,  %tpc12%
HKR, Ndi\params\tpc\enum,               "4",                            0,  %tpcLowest%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

;Following Entry made to Enable/Disable rate Auto Rate control.
HKR, NDI\params\rateCtrlEnable,ParamDesc,,	%RateCtrl%
HKR, NDI\params\rateCtrlEnable,type,,		"enum"
HKR, NDI\params\rateCtrlEnable,Default,,		"1"
HKR, NDI\params\rateCtrlEnable\enum,0,,		%RateCtrlDisable%
HKR, NDI\params\rateCtrlEnable\enum,1,,		%RateCtrlEnable%

;Following Entry made to 11d mode switch 
HKR, NDI\params\ignore11dBeacon,ParamDesc,,	%Mode11d%
HKR, NDI\params\ignore11dBeacon,type,,		"enum"
HKR, NDI\params\ignore11dBeacon,Default,,	"1"
HKR, NDI\params\ignore11dBeacon\enum,0,,		%Mode11dEnable%
HKR, NDI\params\ignore11dBeacon\enum,1,,		%Mode11dDisable%

HKR, Ndi\params\rssiThrHigh,            ParamDesc,                      0,        %rssiThrHigh%
HKR, Ndi\params\rssiThrHigh,            Base,                           0,        "10"
HKR, Ndi\params\rssiThrHigh,            default,                        0,        "40"
HKR, Ndi\params\rssiThrHigh,            type,                           0,        "enum"
HKR, Ndi\params\rssiThrHigh\enum,       "40",                           0,        %rssiThrHighNormal%
HKR, Ndi\params\rssiThrHigh\enum,       "32",                           0,        %rssiThrHighMin%

HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh%

HKR, CustomParams\Configurations,       NicType,                        0x10003,  1

HKR, Ndi\params\bkScanEnable,           ParamDesc,                      0,        %bkScanEnable%
HKR, Ndi\params\bkScanEnable,           Base,                           0,        "10"
HKR, Ndi\params\bkScanEnable,           default,                        0,        "1"
HKR, Ndi\params\bkScanEnable,           type,                           0,        "enum"
HKR, Ndi\params\bkScanEnable\enum,      "1",                            0,        %bkScanEnableOn%
HKR, Ndi\params\bkScanEnable\enum,      "0",                            0,        %bkScanEnableOff%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssi11A%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

HKR, Ndi\params\roamRssiBOnly,          ParamDesc,                      0,        %roamRssi11BOnly%
HKR, Ndi\params\roamRssiBOnly,          default,                        0,        "8"
HKR, Ndi\params\roamRssiBOnly,          min,                            0,        "0"
HKR, Ndi\params\roamRssiBOnly,          max,                            0,        "95"
HKR, Ndi\params\roamRssiBOnly,          step,                           0,        "1"
HKR, Ndi\params\roamRssiBOnly,          base,                           0,        "10"
HKR, Ndi\params\roamRssiBOnly,          type,                           0,        "int"

HKR, Ndi\params\roamRssiB,              ParamDesc,                      0,        %roamRssi11B%
HKR, Ndi\params\roamRssiB,              default,                        0,        "24"
HKR, Ndi\params\roamRssiB,              min,                            0,        "0"
HKR, Ndi\params\roamRssiB,              max,                            0,        "95"
HKR, Ndi\params\roamRssiB,              step,                           0,        "1"
HKR, Ndi\params\roamRssiB,              base,                           0,        "10"
HKR, Ndi\params\roamRssiB,              type,                           0,        "int"

HKR, Ndi\params\roamRateA,              ParamDesc,                      0,        %roamRateA%
HKR, Ndi\params\roamRateA,              Base,                           0,        "10"
HKR, Ndi\params\roamRateA,              default,                        0,        "24000"
HKR, Ndi\params\roamRateA,              type,                           0,        "enum"
HKR, Ndi\params\roamRateA\enum,         "6000",                         0,        %roamRateA6M%
HKR, Ndi\params\roamRateA\enum,         "9000",                         0,        %roamRateA9M%
HKR, Ndi\params\roamRateA\enum,         "12000",                        0,        %roamRateA12M%
HKR, Ndi\params\roamRateA\enum,         "18000",                        0,        %roamRateA18M%
HKR, Ndi\params\roamRateA\enum,         "24000",                        0,        %roamRateA24M%
HKR, Ndi\params\roamRateA\enum,         "36000",                        0,        %roamRateA36M%
HKR, Ndi\params\roamRateA\enum,         "48000",                        0,        %roamRateA48M%
HKR, Ndi\params\roamRateA\enum,         "54000",                        0,        %roamRateA54M%

HKR, Ndi\params\roamRateBOnly,          ParamDesc,                      0,        %roamRateBOnly%
HKR, Ndi\params\roamRateBOnly,          Base,                           0,        "10"
HKR, Ndi\params\roamRateBOnly,          default,                        0,        "5000"
HKR, Ndi\params\roamRateBOnly,          type,                           0,        "enum"
HKR, Ndi\params\roamRateBOnly\enum,     "1000",                         0,        %roamRateBOnly1M%
HKR, Ndi\params\roamRateBOnly\enum,     "2000",                         0,        %roamRateBOnly2M%
HKR, Ndi\params\roamRateBOnly\enum,     "5000",                         0,        %roamRateBOnly5M%
HKR, Ndi\params\roamRateBOnly\enum,     "11000",                        0,        %roamRateBOnly11M%

HKR, Ndi\params\roamRateB,              ParamDesc,                      0,        %roamRateB%
HKR, Ndi\params\roamRateB,              Base,                           0,        "10"
HKR, Ndi\params\roamRateB,              default,                        0,        "9000"
HKR, Ndi\params\roamRateB,              type,                           0,        "enum"
HKR, Ndi\params\roamRateB\enum,         "1000",                         0,        %roamRateB1M%
HKR, Ndi\params\roamRateB\enum,         "2000",                         0,        %roamRateB2M%
HKR, Ndi\params\roamRateB\enum,         "5000",                         0,        %roamRateB5M%
HKR, Ndi\params\roamRateB\enum,         "6000",                         0,        %roamRateB6M%
HKR, Ndi\params\roamRateB\enum,         "9000",                         0,        %roamRateB9M%
HKR, Ndi\params\roamRateB\enum,         "11000",                        0,        %roamRateB11M%

HKR, Ndi\params\pcieAspm,               ParamDesc,                      0,        %pcieAspm%
HKR, Ndi\params\pcieAspm,               Base,                           0,        "10"
HKR, Ndi\params\pcieAspm,               default,                        0,        "0"
HKR, Ndi\params\pcieAspm,               type,                           0,        "enum"
HKR, Ndi\params\pcieAspm\enum,          "0",                            0,        %pcieAspmOff%
HKR, Ndi\params\pcieAspm\enum,          "1",                            0,        %pcieAspmL0sOn%
HKR, Ndi\params\pcieAspm\enum,          "2",                            0,        %pcieAspmL1On%
HKR, Ndi\params\pcieAspm\enum,          "3",                            0,        %pcieAspmL0sandL1On%

HKR, Ndi\params\antennaSwitch,          ParamDesc,                      0,        %antennaSwitch%
HKR, Ndi\params\antennaSwitch,          Base,                           0,        "10"
HKR, Ndi\params\antennaSwitch,          default,                        0,        "0"
HKR, Ndi\params\antennaSwitch,          type,                           0,        "enum"
HKR, Ndi\params\antennaSwitch\enum,     "1",                            0,        %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum,     "2",                            0,        %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum,     "0",                            0,        %antennaSwitchAuto%

HKR, ,                                  rxChainSelect,                 	0x00002,  "7"
HKR, ,                                  txChainSelectLegacy,            0x00002,  "7"
HKR, ,                                  rxChainSelectLegacy,           	0x00002,  "7"
HKR, ,                                  forceBias,           	        0x00002,  "2"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

HKR, Ndi\params\uapsdEnabledBE,            ParamDesc,                      0,  %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBE,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBE,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBE\enum,       "1",                            0,  %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum,       "0",                            0,  %uapsdEnabledBEOff%

HKR, Ndi\params\uapsdEnabledBK,            ParamDesc,                      0,  %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBK,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBK,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBK\enum,       "1",                            0,  %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum,       "0",                            0,  %uapsdEnabledBKOff%

HKR, Ndi\params\uapsdEnabledVI,            ParamDesc,                      0,  %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVI,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVI,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVI\enum,       "1",                            0,  %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum,       "0",                            0,  %uapsdEnabledVIOff%

HKR, Ndi\params\uapsdEnabledVO,            ParamDesc,                      0,  %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVO,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVO,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVO\enum,       "1",                            0,  %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum,       "0",                            0,  %uapsdEnabledVOOff%

HKR, Ndi\params\psPollEnable,            ParamDesc,                      0,  %psPoll%
HKR, Ndi\params\psPollEnable,            Base,                           0,  "10"
HKR, Ndi\params\psPollEnable,            default,                        0,  "0"
HKR, Ndi\params\psPollEnable,            type,                           0,  "enum"
HKR, Ndi\params\psPollEnable\enum,       "1",                            0,  %psPollEnable%
HKR, Ndi\params\psPollEnable\enum,       "0",                            0,  %psPollDisable%

HKR, Ndi\params\*ReceiveBuffers,        ParamDesc,                      0,        "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,        default,                        0,        "256"
HKR, Ndi\params\*ReceiveBuffers,        min,                            0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        max,                            0,        "00000256"
HKR, Ndi\params\*ReceiveBuffers,        step,                           0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        Base,                           0,        "10"
HKR, Ndi\params\*ReceiveBuffers,        type,                           0,        "int"

HKR, Ndi\params\*TransmitBuffers,       ParamDesc,                      0,        "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,       default,                        0,        "512"
HKR, Ndi\params\*TransmitBuffers,       min,                            0,        "1"
HKR, Ndi\params\*TransmitBuffers,       max,                            0,        "00000512"
HKR, Ndi\params\*TransmitBuffers,       step,                           0,        "1"
HKR, Ndi\params\*TransmitBuffers,       Base,                           0,        "10"
HKR, Ndi\params\*TransmitBuffers,       type,                           0,        "int"

[20-40mhz]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "130573"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"

HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "3",                            0,        %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum,       "28",                           0,        %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum,       "31",                           0,        %wModeLegacy11abg%

HKR, Ndi\params\wModeSelect\enum,       "2052",                         0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "4099",                         0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "2076",                         0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "6175",                         0,        %wModeSelect11abgn%

HKR, Ndi\params\wModeSelect\enum,       "26628",                        0,        %wModeSelect11bonly40%
HKR, Ndi\params\wModeSelect\enum,       "103937",                       0,        %wModeSelect11na40%
HKR, Ndi\params\wModeSelect\enum,       "26636",                        0,        %wModeSelect11nbg40%
HKR, Ndi\params\wModeSelect\enum,       "130573",                       0,        %wModeSelect11abgn40%

[9485BTcoex.reg]
HKR, ,                                  wlanActiveGpioSelect,                   0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,                     0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,                   0x00002,  "8"
HKR, ,                                  btCoexEnable,                           0x00002,  "4"
HKR, ,                                  btCoexAgent,                            0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,                       0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                        0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,                     0x00002,  "0"

[MSI.reg]
;HKR, "Interrupt Management", 0x00000010
;HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
;HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
;HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 4

;;End of Customized Section

[atheros.Service]
DisplayName     = %ATHR.Service.DispName%
ServiceType     = 1         ;SERVICE_KERNEL_DRIVER
StartType       = 3         ;SERVICE_DEMAND_START
ErrorControl    = 1         ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\athrx.sys
LoadOrderGroup  = NDIS

[atheros.EventLog]
AddReg = atheros.AddEventLog.reg

[atheros.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


[atheros.CopyFiles]
athrx.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%,athrx.sys,,

[SourceDisksFiles]
athrx.sys = 1,,

[DestinationDirs]
atheros.CopyFiles            = 12
DefaultDestDirs              = 11

[Strings]
;Non-Localizable strings
11DModeSwitch		     = "11d Mode Switch"
2GOnly	                     = "2Ghz Only"
5GOnly	                     = "5Ghz Only"
802_11d                      = "802.11d"
radioEnable                 = "Radio On/Off"
radioEnableOff              = "Off"
radioEnableOn               = "On"
ATHR.Service.DispName        = "Atheros Extensible Wireless LAN device driver"
AdHoc11n                     = "AdHoc 11n"
AdhocBand_DEF_STR_A          = "1"                       ; (A)
AdhocBand_DEF_STR_AB         = "1"                       ; (A)
AdhocBand_DEF_STR_AG         = "0"                       ; (B)
AdhocBand_DEF_STR_G          = "0"                       ; (B)
Atheros                      = "Atheros Communications Inc."
Atheros                      = "Atheros"
Auto			     = "Auto"
Disable                      = "Disable"
DiskDescription              = "Atheros Sample Driver Disk 1"
Enable			     = "Enable"
Gigabyte                     = "Gigabyte Technology Corp."
MSFT                         = "Microsoft"
MapRegisters                 = "Map Registers"
Maximum                      = "Maximum"
Mode11d                      = "11d Mode Switch"
Mode11dDisable               = "Disable"
Mode11dEnable                = "Enable"
NetBand_DEF_STR_A            = "3"                       ; (A/T) 
NetBand_DEF_STR_AB           = "7"                       ; (A/T/B)   
NetBand_DEF_STR_AG           = "15"                      ; (A/T/B/G)
NetBand_DEF_STR_G            = "12"                      ; (B/G)     
NetworkAddress               = "Network Address"
Normal                       = "Normal"
Off			     = "Off"
PowerSaveMode		     = "Power Save Mode"
RateCtrl                     = "Auto Transmit Rate"
RateCtrlDisable              = "Disable"
RateCtrlEnable               = "Enable"
ReceiveBuffers               = "Receive Buffers"
TransmitBuffers              = "Transmit Buffers"
TxRate11a                    = "11a Transmit Rates"
TxRate11a12M                 = "12 Mbps"
TxRate11a18M                 = "18 Mbps"
TxRate11a24M                 = "24 Mbps"
TxRate11a36M                 = "36 Mbps"
TxRate11a48M                 = "48 Mbps"
TxRate11a54M                 = "54 Mbps"
TxRate11a6M                  = "6 Mbps"
TxRate11a9M                  = "9 Mbps"
TxRate11b                    = "11b Transmit Rates"
TxRate11b11M                 = "11 Mbps"
TxRate11b1M                  = "1 Mbps"
TxRate11b2M                  = "2 Mbps"
TxRate11b5M                  = "5.5 Mbps"
TxRate11g                    = "11g Transmit Rates"
TxRate11g11M                 = "11 Mbps"
TxRate11g12M                 = "12 Mbps"
TxRate11g18M                 = "18 Mbps"
TxRate11g1M                  = "1 Mbps"
TxRate11g24M                 = "24 Mbps"
TxRate11g2M                  = "2 Mbps"
TxRate11g36M                 = "36 Mbps"
TxRate11g48M                 = "48 Mbps"
TxRate11g54M                 = "54 Mbps"
TxRate11g5M                  = "5.5 Mbps"
TxRate11g6M                  = "6 Mbps"
TxRate11g9M                  = "9 Mbps"
WirelessMode                 = "Wireless Mode Selection"
WirelessMode11bgOnly         = "802.11b/g"
WirelessMode2GHzOnly         = "2.4 GHz Only"
WirelessMode5GHzOnly         = "5 GHz Only"
WirelessModeAuto             = "Auto"
adhocchannel                 = "Adhoc Channel Select"
adhocchannel                 = "Adhoc channel Selection"
antennaSwitch                = "AntennaSwitch"
antennaSwitchA               = "Antenna A"
antennaSwitchAuto            = "Auto"
antennaSwitchB               = "Antenna B"
authAuto                     = "Auto"
authOpen                     = "Open"
authShared                   = "Shared"
authTypeUseOnly              = "802.11 Authentication Type"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOff              = "Off"
bkScanEnableOn               = "On"
ccx5FeatureEnable            = "MFP"
ccx5FeatureEnableMfpDisable  = "Disable"
ccx5FeatureEnableMfpEnable   = "Enable"
pcieAspm                     = "pcieAspm"
pcieAspmL0sOn                = "L0s On,  L1 Off"
pcieAspmL0sandL1On           = "L0s On,  L1 On"
pcieAspmL1On                 = "L0s Off, L1 On"
pcieAspmOff                  = "L0s Off, L1 Off"
psPoll                       = "Power Save Legacy Algorithm"
psPollDisable                = "PS non Poll"
psPollEnable                 = "PS Poll"
radioEnable                  = "Radio On/Off"
radioEnableOff               = "Off"
radioEnableOn                = "On"
roamPolicy                   = "Roaming Policy"
roamPolicyHigh               = "High"
roamPolicyLow                = "Low"
roamPolicyNormal             = "Normal"
roamPolicyVeryHigh           = "Very High"
roamPolicyVeryLow            = "Very Low"
roamRateA                    = "roamRateA"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateB                    = "roamRateB"
roamRateB11M                 = "11Mbps"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly11M             = "11Mbps"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRssiA                    = "Roam Time Threshold (db)"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighMin               = "Min"
rssiThrHighNormal            = "Normal"
scanTime                     = "Roam Time (sec)"
scanTimeValid                = "Scan Valid Interval"
scanTimeValidcust            = "Roam Time (sec)"
scanTimeValidcust10          = "10"
scanTimeValidcust120         = "120"
scanTimeValidcust20          = "20"
scanTimeValidcust30          = "30"
scanTimeValidcust45          = "45"
scanTimeValidcust5           = "5"
scanTimeValidcust60          = "60"
shortPreamble                = "802.11b Preamble"
shortPreambleDisable         = "Long only"
shortPreambleEnable          = "Long and Short"
shortPreamble_DEFAULT        = "1"
sleepMode                    = "Power Save Mode"
sleepModeMax                 = "Maximum"
sleepModeNormal              = "Normal"
sleepModeOff                 = "Off"
sleepMode_DEFAULT            = "2"  
smpsDynamic                  = "Dynamic MIMO Power Save"
tpc                          = "Transmit Power"
tpc100                       = "100%"
tpc12                        = "12.5%"
tpc25                        = "25%"
tpc50                        = "50%"
tpcLowest                    = "Lowest"
uapsdEnabledBE               = "Power Save Policy (Best Effort)"
uapsdEnabledBEOff            = "Legacy Power Save"
uapsdEnabledBEOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBK               = "Power Save Policy (Background)"
uapsdEnabledBKOff            = "Legacy Power Save"
uapsdEnabledBKOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVI               = "Power Save Policy (Voice)"
uapsdEnabledVIOff            = "Legacy Power Save"
uapsdEnabledVIOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVO               = "Power Save Policy (Video)"
uapsdEnabledVOOff            = "Legacy Power Save"
uapsdEnabledVOOn             = "WMM Power Save (UAPSD)"
wModeLegacy11a               = "11a only"
wModeLegacy11a               = "legacy 11a only"
wModeLegacy11abg             = "11abg"
wModeLegacy11abg             = "legacy 11abg"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11bg              = "legacy 11g and 11b"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bonly           = "legacy 11b only"
wModeSelect                  = "Wireless Mode"
wModeSelect11abgn            = "11abgn"
wModeSelect11abgn20          = "11abgn (20Mhz)"
wModeSelect11abgn40          = "11abgn (40Mhz)"
wModeSelect11bonly           = "11b only"
wModeSelect11bonly20         = "11b only (20Mhz)"
wModeSelect11bonly40         = "11b only (40Mhz)"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11na              = "11na"
wModeSelect11na20            = "11na (20Mhz)"
wModeSelect11na40            = "11na (40Mhz)"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11nbg             = "11ngb"
wModeSelect11nbg20           = "11nbg (20Mhz"
wModeSelect11nbg40           = "11nbg (40Mhz)"
bt30                         = "802.11 Bluetooth High Speed"
bt30enable                   = "Enable"
bt30disable                  = "Disable"
GreenTx                      = "Green Tx"
GreenTxEnableOn              = "On"
GreenTxEnableOff             = "Off"

Atheros_Disk                 = "Atheros Driver Disk 1"
ATHER.Service.DispName       = "Atheros Wireless Network Adapter Service"
ATHER.DeviceDesc.0013        = "Atheros AR5001X+/AR5002G/AR5002X/AR5004G/AR5005GS Wireless Network Adapter"
ATHER.DeviceDesc.001A        = "Atheros AR5005G Wireless Network Adapter"
ATHER.DeviceDesc.001B        = "Atheros AR5006X/AR5006XS/AR5006GS/AR5006G Wireless Network Adapter"
ATHER.DeviceDesc.001C        = "Atheros AR5006EXS/AR5006EX/AR5006EGS/AR5006EG/AR5007EG Wireless Network Adapter"
ATHER.DeviceDesc.001D        = "Atheros AR5007G Wireless Network Adapter"
ATHER.DeviceDesc.0023        = "Atheros AR5008 Wireless Network Adapter"
ATHER.DeviceDesc.0024        = "Atheros AR5008X Wireless Network Adapter"
ATHER.DeviceDesc.0029        = "Atheros AR922X Wireless Network Adapter"
ATHER.DeviceDesc.002A        = "Atheros AR9280/AR9281/AR9283/AR5009/AR5B91/AR5BH92/AR5B93 Wireless Network Adapter"
ATHER.DeviceDesc.002B        = "Atheros AR9285 Wireless Network Adapter"
ATHER.DeviceDesc.002C        = "Atheros AR2427 Wireless Network Adapter"
ATHER.DeviceDesc.002D        = "Atheros AR9227 Wireless Network Adapter"
ATHER.DeviceDesc.002E        = "Atheros AR9287 Wireless Network Adapter"
ATHER.DeviceDesc.0030        = "Atheros AR938x Wireless Network Adapter"
ATHER.DeviceDesc.0032        = "Atheros AR9485 Wireless Network Adapter"
