+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
+      R5U870 Video Device Driver for MC501CB  Ver 6.1005.301.0             +
+	            	    RC Version                                      +
+                         December.15.2006            	                    +
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

The drivers in this driver release are compatible with 
the following R5U870 Video Device Drivers:

Model Number                                Supported Controller                                           
------------                                ------------
R5U870                                      UVC Filter driver            
				                        
   [1]  Directory structure
   [2]  Supported Environments
   [3]  Release note
   [4]  Known critical problem
   [5]  Installation
   [6]  Uninstallation


[1] Directory structure
------------------------------------------------------------------------------------------------

  \++--PID1841_UVC_Ver.6.1005.301.0_061215_32_64bit\+
	 +--R5U870FL.inf      ( R5U870FL***.sys R5U870FU***.sys INF File   (12/15/2006,Ver.6.1005.301.0) )
	 +--DPInst32.exe      ( Installer for 32 bit provided by Microsoft   (11/17/2005) )
	 +--DPInst64.exe      ( Installer for 64 bit provided by Microsoft   (11/17/2005) )
	 +--Install.bat       ( Batch file for installation   (08/08/2006) )
	 +--r5u870flx86.cat   ( Signed Catalog   (12/15/2006) )
	 +--r5u870flamd64.cat ( Signed Catalog   (12/15/2006) )
         +--R5U870flx86.sys   ( Lower Filter Driver(32bit)   (12/15/2006,Ver.6.1005.301.0) )
         +--R5U870fux86.sys   ( Upper Filter Driver(32bit)   (12/15/2006,Ver.6.1005.301.0) )
         +--R5U870flamd64.sys ( Lower Filter Driver(64bit)   (12/15/2006,Ver.6.1005.301.0) )
         +--R5U870fuamd64.sys ( Upper Filter Driver(64bit)   (12/15/2006,Ver.6.1005.301.0) )


[2] Supported Environments 
------------------------------------------------------------------------------------------------

    WindowsXP Professional/Home edition(SP1/SP2)
    WindowsVista

[3] Release note
------------------------------------------------------------------------------------------------

    Version : 6.1005.301.000
    Date    : 2006.12.15
      - Update Inf file(RC Version)

      [Fixed problem from the previously released version]
	    *The problem that the BSOD occurs after the additional of the scanner and the camera is solved.

    Version : 6.1003.301.000
    Date    : 2006.11.6
      - Update Inf file(RC Version)

      [Fixed problem from the previously released version]
	    *The problem that the installation doesn't finish correctly after the uninstallation of the driver is solved.

    Version : 6.1002.301.000
    Date    : 2006.10.24
      - Update Inf file(RC Version)

      [Functional change from the previously released driver]
	    *The setting of Sharpness was improved.

    Version : 6.1000.301.000
    Date    : 2006.10.20
      - First Released Version(RC Version)


[4] Known critical problem
------------------------------------------------------------------------------------------------
1.  Since these RC drivers have not been digitally signed yet, 
    you may see pop-ups when you install warning you that the driver you 
    are installing has not passed Windows Logo testing. You may get two 
    or more of these message boxes. 
    Pressing "Continue Anyway" on all of the boxes will allow the RC drivers 
    to install correctly.

[5] Installation
------------------------------------------------------------------------------------------------
1.  Insert the module.

2.  And then you can see the "Found New Hardware Wizard".

3.  Select the following option: "No,not this time".
    Click the "Next" button.

4.  Select the following option: "Install from a list or
    specific location (Advanced)". Click the "Next" button.

5.  Select the following option: "Don't search.  I will choose the driver to  
    install".  Click the "Next" button. 

6.  Select "Imaging device". Click the "Next" button.

7.  Click the "Have Disk..." button and then the "Browse"
    button.

8.  Enter the directory where you unzipped the file you downloaded,
    Highlight the "R5U870FL.inf" file. Click the "Open" button. 

9.  Click the "Next" button. 

10. The operating system will install the driver.
    Click the "Finish" button when done.

11. Shutdown the PC, and then power on the PC.

12. The installation is complete.

[Installer]
    Double-click the file "Install.bat" to install the drivers.(SilentMode)

[6] Uninstallation
------------------------------------------------------------------------------------------------
1.  Click "Start", then right click "My Computer" icon, and then click "Properties".

2.  Click "Hardware" Tab and select "Device Manager".

3.  Right click "RY5U870 VGA-CAM F01 UVC", and then click "Uninstall"

4.  Click "OK", and the operating system will uninstall the driver.

 
---------------------------  END  --------------------------------------------------------------
