;------------------------------------------------------------------------
;
;   Copyright and Disclaimer:
;
;       ---------------------------------------------------------------
;       This software is provided "as is" without warranty of any kind,
;       either expressed or implied, including but not limited to the
;       implied warranties of merchantability and/or fitness for a
;       particular purpose.
;
;       Copyright (c) 1999-2000 Conexant Systems, Inc.
;       All Rights Reserved.
;       ---------------------------------------------------------------
;
;
;   Abstract:
;
;       This is the video capture driver inf file.
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
;Provider="Conexant"
Provider="Compro"
DriverVer=07/11/2005,4.2.3.2
CatalogFile.ntx86=cx88vid.cat

[Manufacturer]
;"Conexant"=Conexant
"Compro"=Compro

[SourceDisksNames]
;1="Conexant Cx23880 Drivers",,,""
1="Compro VideoMate X series Drivers",,,""

[SourceDisksFiles]
cx88vid.sys=1
cxtvrate.dll=1

[Compro]
;[Conexant]
;---------------------------------
; NTSC EVK
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; CX23880 Version
%CX23880.videoNTSC%=CX23880.PhilipsNTSC,PCI\VEN_14F1&DEV_8800&SUBSYS_006614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_006614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_006614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_006614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_006614F1

; CX23881 Version
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_006614F1

;---------------------------------
; PAL-B/G EVK
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; CX23880 Version
%CX23880.videoPALBG%=CX23880.PhilipsPALBG,PCI\VEN_14F1&DEV_8800&SUBSYS_016614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_016614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_016614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_016614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_016614F1

; CX23881 Version
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_016614F1

;---------------------------------
; PAL-I EVK
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; CX23880
%CX23880.videoPALI%=CX23880.PhilipsPALI,PCI\VEN_14F1&DEV_8800&SUBSYS_026614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_026614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_026614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_026614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_026614F1

; CX23881
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_026614F1

;---------------------------------
; PAL DKI with XuGuang JS-2S/126 tuner
;---------------------------------
; PAL Video Driver enabled
; Audio Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------
%CX23880.videoPalDKI%=CX23880.PALDKI,PCI\VEN_14F1&DEV_8800&SUBSYS_061314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_061314F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_061314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_061314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_061314F1

;---------------------------------
; PAL DKI with TCL2002 MI-3 tuner
;---------------------------------
; PAL Video Driver enabled
; Audio Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------
%CX23880.videoTCLPALDKI%=CX23880.TCLPALDKI,PCI\VEN_14F1&DEV_8800&SUBSYS_084214F1
%CX23880.null%=NullSection,                PCI\VEN_14F1&DEV_8801&SUBSYS_084214F1
%CX23880.null%=NullSection,                PCI\VEN_14F1&DEV_8802&SUBSYS_084214F1
%CX23880.null%=NullSection,                PCI\VEN_14F1&DEV_8803&SUBSYS_084214F1
%CX23880.null%=NullSection,                PCI\VEN_14F1&DEV_8804&SUBSYS_084214F1

;---------------------------------
; NTSC EVK JAPAN
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; CX23880 Version
%CX23880.videoJAPAN%=CX23880.PhilipsNTSCJ,PCI\VEN_14F1&DEV_8800&SUBSYS_036614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_036614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_036614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_036614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_036614F1

; CX23881 Version
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_036614F1

;---------------------------------
; Temic 4-in-1 EVK
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; CX23880 Version
%CX23880.videoTemic4In1%=CX23880.Temic4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_046614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_046614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_046614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_046614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_046614F1

; CX23881 Version
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_046614F1

;---------------------------------
; Philips 4-in-1 EVK
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; CX23880 Version
%CX23880.videoPhilips4In1%=CX23880.Philips4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_096614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_096614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_096614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_096614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_096614F1

; CX23881 Version
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_096614F1

;---------------------------------
; Philips 4-in-1 Half-high EVK
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; CX23880 Version
%CX23880.video4IN1half%=CX23880.PhilipsH4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_017614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_017614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_017614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_017614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_017614F1

; CX23881 Version
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_017614F1

;---------------------------------
; NTSC Half-high EVK
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; CX23880 Version
%CX23880.videoNTSC%=CX23880.PhilipsHNTSC,PCI\VEN_14F1&DEV_8800&SUBSYS_007614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_007614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_007614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_007614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_007614F1

;---------------------------------
; NTSC 1394 EVK, Philips 1236 MK3 tuner
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
; CX23880 Version
;---------------------------------
;%CX23880.videoPhilipsMK3%=CX23880.PhilipsMK3,PCI\VEN_14F1&DEV_8800&SUBSYS_008314F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_008314F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_008314F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_008314F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_008314F1

;---------------------------------
; ATSC EVK
;---------------------------------
; Video Driver enabled
; Audio Driver disabled
; TS Driver enabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; CX23880 Version
%CX23880.video%=CX23880.PhilipsATSC,PCI\VEN_14F1&DEV_8800&SUBSYS_006814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_006814F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_006814F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_006814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_006814F1

;---------------------------------
; VWEB WIN3 EVK
;---------------------------------
; Video Driver enabled, no tuner
; Audio Driver enabled
; TS Driver enabled
; VIP Port disabled
; Host Port enabled
;---------------------------------

; CX23880 Version
%CX23880.video%=CX23880.NoTuner,    PCI\VEN_14F1&DEV_8800&SUBSYS_00F014F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8801&SUBSYS_00F014F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_00F014F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_00F014F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8804&SUBSYS_00F014F1

;---------------------------------
; VWEB WIN5 EVK
;---------------------------------
; Video Driver enabled, Temic 4136 NTSC tuner
; Audio Driver enabled
; TS Driver enabled
; VIP Port disabled
; Host Port enabled
;---------------------------------

; CX23880 Version
%CX23880.videoTemic4136%=CX23880.Temic4136,PCI\VEN_14F1&DEV_8800&SUBSYS_00F114F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8801&SUBSYS_00F114F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_00F114F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_00F114F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8804&SUBSYS_00F114F1

;---------------------------------
; Conexant BlackBird EVK
;---------------------------------
; NTSC Video Driver enabled
; Audio Driver disabled
; Encoder Driver enabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; Conexant CX23880 Version
%CX23880.videoBlackbird%=CX23880.Blackbird,PCI\VEN_14F1&DEV_8800&SUBSYS_004214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_004214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_004214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_004214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_004214F1

; Conexant PAL tuner version
%CX23880.videoBlackbirdPal%=CX23880.BB_PAL,PCI\VEN_14F1&DEV_8800&SUBSYS_014214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_014214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_014214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_014214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_014214F1

;---------------------------------
; Conexant Blackbird EVK with Philips FM1286 MK3 tuner
;---------------------------------
; NTSC Video Driver enabled
; Audio Driver disabled
; Encoder Driver enabled
; VIP Port disabled
; Host Port (remote control) disabled
;---------------------------------
%CX23880.videoBlackbirdNTSCMJ%=CX23880.BB_NTSCMJ,PCI\VEN_14F1&DEV_8800&SUBSYS_124214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_124214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_124214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_124214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_124214F1

;---------------------------------
; Conexant Blackbird EVK with TCL2002 MI-3 tuner
;---------------------------------
%CX23880.videoBlackbirdTCLPalDKI%=CX23880.BB_TCLPALDKI,PCI\VEN_14F1&DEV_8800&SUBSYS_104214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_104214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_104214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_104214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_104214F1

;---------------------------------
; Conexant BlackBird EVK with XuGuang JS-2S/126 tuner
;---------------------------------
; PAL Video Driver enabled
; Audio Driver disabled
; Encoder Driver enabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; Conexant PAL tuner version
%CX23880.videoBlackbirdPalDKI%=CX23880.BB_PALDKI,PCI\VEN_14F1&DEV_8800&SUBSYS_094214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_094214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_094214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_094214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_094214F1

;---------------------------------
;Conexant Blackbird with remote control
;---------------------------------
;Function 4 (host) is HID IR remote.
;---------------------------------

; Conexant CX23880 Version
%CX23880.videoBlackbirdIR%=CX23880.BB_IR,PCI\VEN_14F1&DEV_8800&SUBSYS_024214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_024214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_024214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_024214F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_024214F1

; Conexant PAL tuner version
%CX23880.videoBlackbirdIR_Pal%=CX23880.BB_IR_PAL,PCI\VEN_14F1&DEV_8800&SUBSYS_034214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_034214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_034214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_034214F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_034214F1

; Conexant NTSC-J Version
%CX23880.videoBlackbirdJ%=CX23880.BlackbirdJ,PCI\VEN_14F1&DEV_8800&SUBSYS_044214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_044214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_044214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_044214F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_044214F1

;---------------------------------------
; Conexant BlackBird with dual input
;---------------------------------------

; Dual input NTSC version
%CX23880.videoBlackbirdDualNTSC%=CX23880.BB_DUAL1_NTSC,PCI\VEN_14F1&DEV_8800&SUBSYS_054214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_054214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_054214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_054214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_054214F1

; Dual input PAL-B/G version
%CX23880.videoBlackbirdDualPALBG%=CX23880.BB_DUAL1_PALBG,PCI\VEN_14F1&DEV_8800&SUBSYS_064214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_064214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_064214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_064214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_064214F1

; Dual input NTSC-J version
%CX23880.videoBlackbirdDualNTSCJ%=CX23880.BB_DUAL1_NTSCJ,PCI\VEN_14F1&DEV_8800&SUBSYS_074214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_074214F1
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_074214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_074214F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_074214F1

;---------------------------------
; BlackBird EVK
;---------------------------------
; NTSC Video Driver enabled
; Audio Driver disabled
; Encoder Driver enabled
; VIP Port disabled
; Host Port disabled
;---------------------------------

; dual input NTSC version
%CX23880.videoBlackbirdDualNTSC%=CX23880.BB_DUAL_NTSC,PCI\VEN_14F1&DEV_8800&SUBSYS_48231043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_48231043
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_48231043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_48231043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_48231043

; dual input PAL-B/G version
%CX23880.videoBlackbirdDualPALBG%=CX23880.BB_DUAL_PALBG,PCI\VEN_14F1&DEV_8800&SUBSYS_48241043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_48241043
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_48241043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_48241043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_48241043

; dual input PAL-D/K version
%CX23880.videoBlackbirdDualPALDK%=CX23880.BB_DUAL_PALDK,PCI\VEN_14F1&DEV_8800&SUBSYS_48251043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_48251043
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_48251043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_48251043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_48251043

; dual input SECAM version
%CX23880.videoBlackbirdDualSECAM%=CX23880.BB_DUAL_SECAM,PCI\VEN_14F1&DEV_8800&SUBSYS_48261043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_48261043
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_48261043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_48261043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_48261043

; dual input PAL-I version
%CX23880.videoBlackbirdDualPALI%=CX23880.BB_DUAL_PALI,PCI\VEN_14F1&DEV_8800&SUBSYS_48271043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_48271043
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_48271043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_48271043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_48271043

; dual input NTSC-J version
%CX23880.videoBlackbirdDualNTSCJ%=CX23880.BB_DUAL_NTSCJ,PCI\VEN_14F1&DEV_8800&SUBSYS_48281043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_48281043
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_48281043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_48281043
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_48281043

;---------------------------------
; PVR1 EVK
;---------------------------------
; Video Driver enabled, Temic 4136 NTSC tuner, PVR1 crossbar
; Audio Driver .inf enabled
; TS Driver enabled
; VIP Port disabled
; Host Port enabled
;---------------------------------

; CX23880 Version
%CX23880.videoPVR1%=CX23880.PVR1,PCI\VEN_14F1&DEV_8800&SUBSYS_81961033
;CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_81961033
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_81961033
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_81961033
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8804&SUBSYS_81961033

; CX23881 Version
;%CX23881.null%=NullSection,        PCI\VEN_14F1&DEV_8811&SUBSYS_81961033

; Include swapped SSVID

; CX23880 Version
%CX23880.videoPVR1%=CX23880.PVR1,PCI\VEN_14F1&DEV_8800&SUBSYS_10338196
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8801&SUBSYS_10338196
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8802&SUBSYS_10338196
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_10338196
;%CX23880.null%=NullSection,        PCI\VEN_14F1&DEV_8804&SUBSYS_10338196

; CX23881 Version
;%CX23881.null%=NullSection,        PCI\VEN_14F1&DEV_8811&SUBSYS_10338196

; 883 NTSC EVK
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled

; CX23883 Version
%CX23880.video883%=CX23880.883_NTSC,PCI\VEN_14F1&DEV_8800&SUBSYS_017914F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_017914F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_017914F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_017914F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_017914F1

; 882 Half-high Philips 4-In-1 EVK
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
; CX23882 Version
%CX23880.video882%=CX23880.882_4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_017814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_017814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_017814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_017814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_017814F1

; 881 Half-high Philips 4-In-1 EVK
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
; CX23881 Version
%CX23880.video881%=CX23880.881_4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_017714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_017714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_017714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_017714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_017714F1

; E4 TVFM 880 NTSC MK3
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
%CX23880.videoPhilipsMK3%=CX23880.PhilipsMK3,PCI\VEN_14F1&DEV_8800&SUBSYS_001314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_001314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_001314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_001314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_001314F1

; CX23881 Version
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_001314F1

; E4 TVFM 883 NTSC FI1236 MK3
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
%CX23880.videoPhilipsMK3%=CX23880.FI1236MK3,PCI\VEN_14F1&DEV_8800&SUBSYS_00F814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_00F814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_00F814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_00F814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_00F814F1

; E4 TVFM 880 PAL MK3
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
%CX23880.videoPhilips4In1%=CX23880.Philips4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_011314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_011314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_011314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_011314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_011314F1

; CX23881 Version
%CX23881.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_011314F1

; Half-high NTSC 880 MK3
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
%CX23880.videoPhilipsMK3half%=CX23880.PhilipsMK3,PCI\VEN_14F1&DEV_8800&SUBSYS_027614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_027614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_027614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_027614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_027614F1

; Half-high PAL 880 MK3
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
%CX23880.video4IN1half%=CX23880.PhilipsH4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_037614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_037614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_037614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_037614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_037614F1

; 1394 PAL MK3
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
%CX23880.videoPhilips4In1%=CX23880.Philips4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_018314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_018314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_018314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_018314F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_018314F1

; StreamAMachine NTSC MK3
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
%CX23880.videoPhilipsMK3%=CX23880.PhilipsMK3,PCI\VEN_14F1&DEV_8800&SUBSYS_009814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_009814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_009814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_009814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_009814F1

; StreamAMachine PAL MK3
; Video Driver enabled
; Audio Driver disabled
; TS Driver disabled
; VIP Port disabled
; Host Port disabled
%CX23880.videoPhilips4In1%=CX23880.Philips4In1,PCI\VEN_14F1&DEV_8800&SUBSYS_019814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_019814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_019814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_019814F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_019814F1

; Stratford - DVB-T using Gromit OFDM demod with Alps Tuner
; Video Driver enable
; Audio Driver disabled
; TS Driver enabled
; VIP Port disabled
; Host Port diabled
%CX23880.video%=CX23880.AlpsDVBT,PCI\VEN_14F1&DEV_8800&SUBSYS_008714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_008714F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_008714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_008714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_008714F1

; Goshawk - DVB-S using Conexant Rosie/Camaric QPSK tuner/demod combination with IR remote
; Video Driver enable
; Audio Driver disabled
; TS Driver enabled
; VIP Port disabled
; Host Port enabled for IR
%CX23880.video%=CX23880.CnxtDVBS,PCI\VEN_14F1&DEV_8800&SUBSYS_008414F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_008414F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_008414F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_008414F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_008414F1

; Stratford2 - DVB-T using Gromit OFDM demod with Thomson Tuner and IR remote
; Video Driver enable
; Audio Driver disabled
; TS Driver enabled
; VIP Port disabled
; Host Port enabled for IR
%CX23880.video%=CX23880.ThomsonDVBT,PCI\VEN_14F1&DEV_8800&SUBSYS_018714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8811&SUBSYS_018714F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_018714F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_018714F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_018714F1

; KittyHawk - ATSC/NTSC/FM using 8-VSB demod with Thomson DTT7612 Tuner
; and IR remote
;
; Video Driver enable
; Audio Driver disabled
; TS Driver enabled
; VIP Port disabled
; Host Port disabled
%CX23880.video%=CX23880.Kittyhawk2,PCI\VEN_14F1&DEV_8800&SUBSYS_000614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801&SUBSYS_000614F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802&SUBSYS_000614F1
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803&SUBSYS_000614F1
;%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804&SUBSYS_000614F1

;
; Compro VideoMate X series
%CX23880.videoCompro%=CX23880.Compro,PCI\VEN_14F1&DEV_8800
%CX23880.videoCompro%=CX23880.Compro,PCI\VEN_14F1&DEV_8800&SUBSYS_E000185B
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8801
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8802
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8803
%CX23880.null%=NullSection,         PCI\VEN_14F1&DEV_8804

[NullSection]

[NullSection.Services]
AddService = , 2  ; null service install

[DestinationDirs]
CX23880.CopyDrivers=10,system32\drivers
CX23880.CopyFilters=11

[CX23880.CopyDrivers]
cx88vid.sys

[CX23880.CopyFilters]
cxtvrate.dll

[CX23880.PhilipsNTSC]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PhilipsNTSC.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.883_NTSC]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,883_NTSC.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.882_4In1]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,882_4In1.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.881_4In1]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,881_4In1.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.PhilipsNTSCJ]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PhilipsNTSCJ.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.PhilipsPALI]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PhilipsPALI.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.PALDKI]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PALDKI.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.TCLPALDKI]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,TCLPALDKI.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.PhilipsPALBG]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PhilipsPALBG.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.Philips4In1]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Philips4In1.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.PhilipsH4In1]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PhilipsH4In1.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.PhilipsHNTSC]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PhilipsHNTSC.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.PhilipsMK3]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PhilipsMK3.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.FI1236MK3]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,FI1236MK3.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.Temic4In1]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Temic4In1.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.Temic4136]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Temic4136.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.PVR1]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PVR1.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.PhilipsATSC]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,PhilipsATSC.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.AlpsDVBT]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,AlpsDVBT.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.CnxtDVBS]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,CnxtDVBS.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.ThomsonDVBT]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,ThomsonDVBT.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.Blackbird]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,Blackbird.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_PAL]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_PAL.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters

[CX23880.BB_PALDKI]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_PALDKI.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters

[CX23880.BB_NTSCMJ]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_NTSCMJ.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters

[CX23880.BB_TCLPALDKI]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_TCLPALDKI.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters

[CX23880.BB_IR]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_IR.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_IR_PAL]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_IR_PAL.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters

[CX23880.BlackbirdJ]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BlackbirdJ.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters

[CX23880.BB_DUAL1_NTSC]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL1_NTSC.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL1_PALBG]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL1_PALBG.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL1_NTSCJ]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL1_NTSCJ.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL2_NTSC]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL2_NTSC.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL2_PALBG]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL2_PALBG.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL_NTSC]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL_NTSC.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL_PALBG]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL_PALBG.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL_PALDK]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL_PALDK.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL_SECAM]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL_SECAM.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL_PALI]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL_PALI.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.BB_DUAL_NTSCJ]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Blackbird_Common.AddReg,BB_DUAL_NTSCJ.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters
RegisterDlls=TvRating.RegDLL    ; enable TvRating DLL for this device

[CX23880.Kittyhawk2]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Kittyhawk2.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.NoTuner]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,NoTuner.AddReg
CopyFiles=  CX23880.CopyDrivers

[CX23880.Compro]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Compro.AddReg
CopyFiles=  CX23880.CopyDrivers

[TvRating.RegDLL]
11,,cxtvrate.dll,1

[CX23880.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,cx88vid.sys
HKR,,OkToHibernate,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKR,"DriverData","XBarInPin0",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData","XBarInPin1",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","XBarInPin2",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","XBarInPin3",0x00010001, 0x00,0x10,0x00,0x00
HKR,"DriverData","XTal0",0x00010001, 0x1c, 0x00, 0x00, 0x00
HKR,"DriverData","XTal1",0x00010001, 0x23, 0x00, 0x00, 0x00
HKR,"DriverData","BobMode",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","VolumeLevelNegdB",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseExternalVPRES",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseI2SAsClock",0x00010001, 0x00, 0x00, 0x00, 0x00
HKLM,%MediaCategories%\%GUID.PINNAME_656_OUT%,Name,,%PinName.656_OUT%
HKLM,%MediaCategories%\%GUID.PINNAME_I2S_OUT%,Name,,%PinName.I2S_OUT%
HKLM,%MediaCategories%\%GUID.PINNAME_ANALOG_AUDIO_IN%,Name,,%Pin.p2AnalogAudioIn%

HKLM,%MediaInterfaces%\{0A7AF963-6805-4f99-B284-29B680975542},,,"Copy Protect Notification Filter"
HKLM,%MediaInterfaces%\{0A7AF963-6805-4f99-B284-29B680975542},IID,1,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00


[PhilipsNTSC.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips"

[883_NTSC.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[882_4In1.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[881_4In1.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[PhilipsNTSCJ.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x00,0x00,0x00,0x00
; Country code is Japan = 81
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[PhilipsPALI.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x00,0x01,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is Great Britain = 44
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x2C,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philipspali"

[PhilipsPALBG.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philipspalbg"

[TCLPALDKI.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x20,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is China = 86
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x56,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.tcl2002mi3"

[Philips4In1.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[PhilipsH4In1.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
; Use Mux'd AM audio output, GPIO pin 0 audio output control, GPIO pin 1 audio input control
HKR,"DriverData","AMAudioSelection",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData","AMAudioMuxInput",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","AMAudioMuxGPIOOutputSrcPin",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData","AMAudioMuxGPIOInputSrcPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[PhilipsHNTSC.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips"

[PhilipsMK3.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[FI1236MK3.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.FI1236MK3"

[Temic4In1.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.temic4in1"

[Temic4136.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.temic4136"

[PVR1.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","VDelayOdd525",  0x00010001, 0x1a, 0x00, 0x00, 0x00
HKR,"DriverData","VDelayEven525", 0x00010001, 0x1a, 0x00, 0x00, 0x00
HKR,"DriverData","VActiveOdd525",  0x00010001, 0xe7, 0x01, 0x00, 0x00
HKR,"DriverData","VActiveEven525", 0x00010001, 0xe7, 0x01, 0x00, 0x00
HKR,"DriverData","Out656VDelayOdd525", 0x00010001, 0x0c, 0x00, 0x00, 0x00
HKR,"DriverData","Out656VDelayEven525", 0x00010001, 0x0c, 0x00, 0x00, 0x00
HKR,"DriverData","PinMuxIO", 0x00010001, 0x88, 0x00, 0x00, 0x00
HKR,"DriverData","VBOSControl", 0x00010001, 0x00, 0x4A, 0x0A, 0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x00,0x00,0x00,0x00
; Country code is Japan = 81
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
; Override audio standard to I2S DAC passthrough
HKR,"DriverData","WWAudioPrimaryStandard",0x00010001, 0x0B,0x00,0x00,0x00
; Set the default I2S passthrough frequency to 48000 Hz (0xBB80)
HKR,"DriverData","WWI2SPTFrequency"      ,0x00010001, 0x80,0xBB,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.pvr1"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.temic4136"

[PhilipsATSC.AddReg]
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsFullMonty",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DemodInSerialMode",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips1236d"

[AlpsDVBT.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x00,0x01,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; prevent audio tracking thread from running, card doesn't support
; any audio.  Audio is in mpeg packets.  Setting to I2S audio.
HKR,"DriverData","WWAudioPrimaryStandard",0x00010001, 0x0B,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxbdatune.VEN_14F1.alpsdvbt"

[CnxtDVBS.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; prevent audio tracking thread from running, card doesn't support
; any audio.  Audio is in mpeg packets.  Setting to I2S audio.
HKR,"DriverData","WWAudioPrimaryStandard",0x00010001, 0x0B,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxbdatune.VEN_14F1.cnxtdvbs"

[ThomsonDVBT.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x00,0x01,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; prevent audio tracking thread from running, card doesn't support
; any audio.  Audio is in mpeg packets.  Setting to I2S audio.
HKR,"DriverData","WWAudioPrimaryStandard",0x00010001, 0x0B,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxbdatune.VEN_14F1.thomsondvbt"

[PALDKI.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x20,0x00,0x00,0x00
; Country code is China = 86; PAL-D
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x56,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.XuGuang126"

[Blackbird_Common.AddReg]
HKR,"DriverData","VDelayOdd525",  0x00010001, 0x1C, 0x00, 0x00, 0x00
HKR,"DriverData","VDelayEven525", 0x00010001, 0x1C, 0x00, 0x00, 0x00
HKR,"DriverData","VActiveOdd525",  0x00010001, 0xe0, 0x01, 0x00, 0x00
HKR,"DriverData","VActiveEven525", 0x00010001, 0xe0, 0x01, 0x00, 0x00
HKR,"DriverData","Out656VDelayOdd525",  0x00010001, 0x26, 0x00, 0x00, 0x00
HKR,"DriverData","Out656VDelayEven525", 0x00010001, 0x26, 0x00, 0x00, 0x00

HKR,"DriverData","VDelayOdd625",  0x00010001, 0x26, 0x00, 0x00, 0x00
HKR,"DriverData","VDelayEven625", 0x00010001, 0x26, 0x00, 0x00, 0x00
HKR,"DriverData","VActiveOdd625",  0x00010001, 0x40, 0x02, 0x00, 0x00
HKR,"DriverData","VActiveEven625", 0x00010001, 0x40, 0x02, 0x00, 0x00
HKR,"DriverData","Out656VDelayOdd625",  0x00010001, 0x26, 0x00, 0x00, 0x00
HKR,"DriverData","Out656VDelayEven625", 0x00010001, 0x26, 0x00, 0x00, 0x00

HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00

;Enable I2S out to encoder
HKR,"DriverData","WWAudioEnableI2SOut",0x00010001, 0x01,0x00,0x00,0x00

; Disable Macrovision Obfuscation
HKR,"DriverData","EncoderMVDRM",0x00010001, 0x00,0x00,0x00,0x00

;I2S output format is Sony (1) 
HKR,"DriverData","WWAudioI2SOutFormat",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","WWAudioI2SFrequency",0x00010001, 0x80,0xBB,0x00,0x00
HKR,"DriverData","WWAudioMuteDACs"    ,0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00

[Blackbird.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","WhiteCrushMAJSEL",  0x00010001, 0x01, 0x00, 0x00, 0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[BB_PAL.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[BB_PALDKI.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x20,0x00,0x00,0x00
; Country code is China = 86; PAL-D
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x56,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.XuGuang126"

[BB_NTSCMJ.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","WhiteCrushMAJSEL",  0x00010001, 0x01, 0x00, 0x00, 0x00
; Country code is Japan = 81
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.FM1286MK3"

[BB_TCLPALDKI.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x20,0x00,0x00,0x00
; Country code is China = 86; PAL-D
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x56,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.TCL2002mi3"

[BB_IR.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","WhiteCrushMAJSEL",  0x00010001, 0x01, 0x00, 0x00, 0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[BB_IR_PAL.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[BlackbirdJ.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[BB_DUAL_NTSC.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","WhiteCrushMAJSEL",  0x00010001, 0x01, 0x00, 0x00, 0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[BB_DUAL_PALBG.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[BB_DUAL_PALDK.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x20,0x00,0x00,0x00
; Country code is China = 86
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x56,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[BB_DUAL_SECAM.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x00,0x00,0x04,0x00
; Country code is France = 33
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x21,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[BB_DUAL_PALI.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x00,0x01,0x00,0x00
; Country code is Great Britain = 44
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x2C,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[BB_DUAL_NTSCJ.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
; Country code is Japan = 81
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[BB_DUAL1_NTSCJ.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x02,0x00,0x00,0x00
; Country code is Japan = 81
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x51,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x02,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL_1"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[BB_DUAL1_PALBG.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x02,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL_1"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[BB_DUAL1_NTSC.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","WhiteCrushMAJSEL",  0x00010001, 0x01, 0x00, 0x00, 0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x02,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL_1"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[BB_DUAL2_NTSC.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","WhiteCrushMAJSEL",  0x00010001, 0x01, 0x00, 0x00, 0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL_2"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.PhilipsMK3"

[BB_DUAL2_PALBG.AddReg]
HKR,"DriverData","4in1Tuner",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00
; Country code is Germany = 49
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BlackbirdType",0x00010001, 0x01,0x00,0x00,0x00

HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.BB_DUAL_2"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.philips4in1"

[Kittyhawk2.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","UseCompositeOnSVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.thomson761x"
HKR,"ENUM\Device3",pnpid,,"cxbdatune.VEN_14F1.kittyhawk2"

[NoTuner.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","Pll27",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"

[Compro.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
; we disable color killer
HKR,"DriverData","ColorKillEnable",0x00010001, 0x00,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
; we disable auto blue
HKR,"DriverData","DisableAutoBlueScreen",0x00010001, 0x01, 0x00, 0x00, 0x00
; we enable white crush AGC
HKR,"DriverData","WCENEnable",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","ChromaSubcarrierFast",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"ENUM\Device1",pnpid,,"cx88xbar.VEN_14F1.cnxt"
HKR,"ENUM\Device2",pnpid,,"cxtune.VEN_14F1.Compro"

[VideoCapture]
AddReg=VideoCapture.AddReg

[VideoTvAudio]
AddReg=VideoTvAudio.AddReg

[VideoCapture.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%CX23880.friendly%

[VideoTvAudio.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%CX23880.friendly2%

[VideoCaptureCompro]
AddReg=VideoCaptureCompro.AddReg

[VideoTvAudioCompro]
AddReg=VideoTvAudioCompro.AddReg

[VideoCaptureCompro.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%CX23880.friendlyCompro%

[VideoTvAudioCompro.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%CX23880.friendly2Compro%

[CX23880.PhilipsNTSC.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PhilipsNTSC.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.883_NTSC.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.883_NTSC.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.882_4In1.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.882_4In1.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.881_4In1.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.881_4In1.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.PhilipsNTSCJ.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PhilipsNTSCJ.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.PhilipsPALBG.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PhilipsPALBG.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.PhilipsPALI.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PhilipsPALI.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.Philips4In1.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Philips4In1.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.PhilipsH4In1.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PhilipsH4In1.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.PhilipsHNTSC.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PhilipsHNTSC.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.PhilipsMK3.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PhilipsMK3.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.FI1236MK3.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.FI1236MK3.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.Temic4In1.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Temic4In1.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.Temic4136.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Temic4136.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.PVR1.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PVR1.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.PhilipsATSC.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PhilipsATSC.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.AlpsDVBT.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.AlpsDVBT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.CnxtDVBS.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.CnxtDVBS.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.ThomsonDVBT.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.ThomsonDVBT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PALDKI.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.PALDKI.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.TCLPALDKI.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.TCLPALDKI.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.Blackbird.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Blackbird.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_PAL.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_PAL.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_PALDKI.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_PALDKI.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_NTSCMJ.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_NTSCMJ.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_TCLPALDKI.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_TCLPALDKI.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_IR.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_IR.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_IR_PAL.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_IR_PAL.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL1_NTSC.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL1_NTSC.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL1_PALBG.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL1_PALBG.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL1_NTSCJ.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL1_NTSCJ.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL2_NTSC.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL2_NTSC.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL2_PALBG.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL2_PALBG.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL_NTSC.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL_NTSC.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL_PALBG.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL_PALBG.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL_PALDK.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL_PALDK.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL_SECAM.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL_SECAM.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL_PALI.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL_PALI.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BB_DUAL_NTSCJ.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BB_DUAL_NTSCJ.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.BlackbirdJ.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.BlackbirdJ.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.Kittyhawk2.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.Kittyhawk2.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.NoTuner.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.NoTuner.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Compro.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCaptureCompro,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudioCompro,

[CX23880.Compro.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.ServiceInstall]
DisplayName   = %CX23880.video%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_AUTO_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\system32\drivers\cx88vid.sys

[Strings]
CX23880.video                       = "Conexant 23880 Video Capture"
CX23880.videoNTSC                   = "Conexant 23880 Video Capture (NTSC)"
CX23880.videoBlackbird   	        = "Conexant 23880 Video Capture (Blackbird)"
CX23880.videoBlackbirdNTSCMJ        = "Conexant 23880 Video Capture (Blackbird NTSC System M)"
CX23880.videoBlackbirdPAL 	        = "Conexant 23880 Video Capture (Blackbird PAL)"
CX23880.videoBlackbirdPALDKI        = "Conexant 23880 Video Capture (Blackbird PAL-D/K & I)"
CX23880.videoBlackbirdTCLPALDKI  	= "Conexant 23880 Video Capture (Blackbird TCL2002MI-3 PAL-D/K & I)"
CX23880.videoBlackbirdIR 	        = "Conexant 23880 Video Capture (Blackbird with remote)"
CX23880.videoBlackbirdDualNTSC 		= "Conexant 23880 Video Capture (Blackbird NTSC Dual-Input)"
CX23880.videoBlackbirdDualPALBG 	= "Conexant 23880 Video Capture (Blackbird PAL-B/G Dual-Input)"
CX23880.videoBlackbirdDualPALDK 	= "Conexant 23880 Video Capture (Blackbird PAL-D/K Dual-Input)"
CX23880.videoBlackbirdDualSECAM 	= "Conexant 23880 Video Capture (Blackbird SECAM Dual-Input)"
CX23880.videoBlackbirdDualPALI 		= "Conexant 23880 Video Capture (Blackbird PAL-I Dual-Input)"
CX23880.videoBlackbirdDualNTSCJ 	= "Conexant 23880 Video Capture (Blackbird NTSC-J Dual-Input)"
CX23880.videoBlackbirdIR_PAL 	    = "Conexant 23880 Video Capture (Blackbird PAL with Remote)"
CX23880.videoBlackbirdJ  	= "Conexant 23880 Video Capture (Blackbird NTSC-J)"
CX23880.videoPALBG          = "Conexant 23880 Video Capture (PAL-B/G)"
CX23880.videoPALI           = "Conexant 23880 Video Capture (PAL-I)"
CX23880.videoPALDKI  		= "Conexant 23880 Video Capture (PAL-D/K & I)"
CX23880.videoTCLPALDKI  	= "Conexant 23880 Video Capture (TCL2002MI-3 PAL-D/K & I)"
CX23880.videoJAPAN          = "Conexant 23880 Video Capture (Japan)"
CX23880.videoTemic4IN1      = "Conexant 23880 Video Capture (Temic 4-in-1)"
CX23880.videoPhilips4IN1    = "Conexant 23880 Video Capture (Philips 4-in-1)"
CX23880.video4IN1half       = "Conexant 23880 Video Capture (4-in-1 Half)"
CX23880.videoPhilipsMK3     = "Conexant 23880 Video Capture (Philips 1236 MK3)"
CX23880.videoPhilipsMK3half = "Conexant 23880 Video Capture (Philips MK3 Half)"
CX23880.videoTemic4136      = "Conexant 23880 Video Capture (Temic 4136)"
CX23880.videoPVR1           = "Conexant 23880 Video Capture (PVR1)"
CX23881.video               = "Conexant 23881 Video Capture"
CX23881.videoNTSC           = "Conexant 23881 Video Capture (NTSC)"
CX23881.videoPALBG          = "Conexant 23881 Video Capture (PAL-B/G)"
CX23881.videoPALI           = "Conexant 23881 Video Capture (PAL-I)"
CX23881.videoJAPAN          = "Conexant 23881 Video Capture (Japan)"
CX23881.videoTemic4IN1      = "Conexant 23881 Video Capture (Temic 4-in-1)"
CX23881.videoPhilips4IN1    = "Conexant 23881 Video Capture (Philips 4-in-1)"
CX23881.videoTemic4136      = "Conexant 23881 Video Capture (Temic 4136)"
CX23881.videoPVR1           = "Conexant 23881 Video Capture (PVR1)"
CX23880.video883            = "Conexant 23883 Video Capture (NTSC)"
CX23880.video882            = "Conexant 23882 Video Capture (4-in-1 Half)"
CX23880.video881            = "Conexant 23881 Video Capture (4-in-1 Half)"
;CX23880.null                = "Conexant (unused device function)"
CX23880.null                = "Compro VideoMate X series device"
;CX23881.null                = "Conexant (unused device function)"
CX23881.null                = "Compro VideoMate X series device"
CX23880.friendly            = "Conexant 2388x Video Capture"
CX23880.friendly2           = "Conexant 2388x TvAudio"
CX23880.friendlyCompro      = "VideoMate X series Video Capture"
CX23880.friendly2Compro     = "VideoMate X series TvAudio"
CX23880.videoCompro         = "Compro VideoMate X series Video Capture"
;RunOnce                    = "SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce"
SERVICE_KERNEL_DRIVER       = 1
SERVICE_AUTO_START          = 2
SERVICE_ERROR_NORMAL        = 1

MediaCategories		 	    = "SYSTEM\CurrentControlSet\Control\MediaCategories"
MediaInterfaces          =    "System\CurrentControlSet\Control\MediaInterfaces"
GUID.PINNAME_656_OUT     	= "{E2EEB283-EB84-4910-BABE-037FFBB03249}"
GUID.PINNAME_I2S_OUT     	= "{71A59578-46D2-4368-BEAF-062B0447565D}"
GUID.PINNAME_ANALOG_AUDIO_IN    = "{04394D28-52A7-4c46-AED0-65D62CC64DA6}"
PinName.656_OUT          	= "656"
PinName.I2S_OUT          	= "I2S"
Pin.p2AnalogAudioIn         = "Analog Audio In"


