;   88x Analog Stream driver Tuner Install Information File For Win2000, WinXP, MCE
;
;       
;
;   Copyright (c) 2004-2006 DVB-DTV Technology Inc.
;   All Rights Reserved.
;
;

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Twinhan"
DriverVer=04/29/2006,1.0.1.9
CatalogFile=88XAStream.cat

[Manufacturer]
"Twinhan"=Twinhan

[SourceDisksNames]
1="DVB-DTV PCI Analog Stream Driver",,,""

[SourceDisksFiles]
88xAStream.sys=1

[Twinhan]
; motorola(mc801) tuner & tda9887(all standard)
%CX23880.videoMoto%=CX23880.Motorola,PCI\VEN_14F1&DEV_8800&SUBSYS_00231822


[DestinationDirs]
CX23880.CopyDrivers=10,system32\drivers
CX23880.CopyFilters=11

[CX23880.CopyDrivers]
88xAStream.sys

[CX23880.CopyFilters]
; none for now


[CX23880.Motorola]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,Motorola.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters

[CX23880.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,88xAStream.sys
HKR,,OkToHibernate,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKR,"DriverData","XBarInPin0",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData","XBarInPin1",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","XBarInPin2",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","XBarInPin3",0x00010001, 0x00,0x10,0x00,0x00
HKR,"DriverData","XTal0",0x00010001, 0x1c, 0x00, 0x00, 0x00
HKR,"DriverData","XTal1",0x00010001, 0x23, 0x00, 0x00, 0x00
HKR,"DriverData","BobMode",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","VolumeLevelNegdB",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseExternalVPRES",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseI2SAsClock",0x00010001, 0x00, 0x00, 0x00, 0x00


[Motorola.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00
;HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.Motorola"
HKR,"ENUM\Device1",pnpid,,"THBDATUNE.VEN_14F1.MT352FMD1216"
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_14F1.Motorola"

[VideoCapture]
AddReg=VideoCapture.AddReg

;[VideoTvAudio]
;AddReg=VideoTvAudio.AddReg

[VideoCapture.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%CX23880.friendly%

[VideoTvAudio.AddReg]
;HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
;HKR,,FriendlyName,,%CX23880.friendly2%

[CX23880.Motorola.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
;AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.Motorola.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.ServiceInstall]
DisplayName   = %CX23880.video%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_AUTO_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\system32\drivers\88xAStream.sys

[Strings]
CX23880.video               = "DTV-DVB 88X Analog Video Capture"
CX23880.friendly            = "DTV-DVB 88X Analog Video Capture"
CX23880.friendly2           = "DT_DVB 88X TvAudio"
CX23880.videoMoto	    = "DTV-DVB 88X Analog Video"
;RunOnce                    = "SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce"
SERVICE_KERNEL_DRIVER       = 1
SERVICE_AUTO_START          = 2
SERVICE_ERROR_NORMAL        = 1


