;*******************************************************************************************
;
;FILE:
;
;    WUSB54G.inf
;
;DESCRIPTION:
;   Linksys Wireless-G USB Network Adapter
;   Linksys Wireless-G Portable USB Adapter 
;
;
;*******************************************************************************************

[Version]
 DriverVer = 01/12/2004, 1.0.8.0
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
 CatalogFile         = WUSB54G.cat

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %WUSB54G%      = USB20_PID2234,        USB\VID_1915&PID_2234
 %WUSB54GP%     = USB20_PID2235,        USB\VID_1915&PID_2235
 %WUSB54G%      = USB20_G,              USB\VID_5041&PID_2234
 %WUSB54GP%     = USB20_GP,             USB\VID_5041&PID_2235
  
[USB20_PID2234]
 AddReg         = USB20_PID2234.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = USB_DRIVER.copy 

[USB20_PID2234.NT]
 AddReg         = USB20_PID2234.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = USB_DRIVER.copy.NT 
 BusType        = 15
 Characteristics= 0x84

[USB20_PID2235]
 AddReg         = USB20_PID2235.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = USB_DRIVER.copy 

[USB20_PID2235.NT]
 AddReg         = USB20_PID2235.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = USB_DRIVER.copy.NT 
 BusType        = 15
 Characteristics= 0x84

[USB20_G]
 AddReg         = USB20_G.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = USB_DRIVER.copy 

[USB20_G.NT]
 AddReg         = USB20_G.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = USB_DRIVER.copy.NT 
 BusType        = 15
 Characteristics= 0x84

[USB20_GP]
 AddReg         = USB20_GP.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = USB_DRIVER.copy 

[USB20_GP.NT]
 AddReg         = USB20_GP.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = USB_DRIVER.copy.NT 
 BusType        = 15
 Characteristics= 0x84

[USB20_PID2234.NT.Services]
 AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog

[USB20_PID2235.NT.Services]
 AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog

[USB20_G.NT.Services]
 AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog

[USB20_GP.NT.Services]
 AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog

[USB20_PID2234.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_1915&PID_2234"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%WUSB54G%

[USB20_PID2235.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_1915&PID_2235"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%WUSB54GP%

[USB20_G.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_5041&PID_2234"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%WUSB54G%

[USB20_GP.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_5041&PID_2235"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%WUSB54GP%
;###############################################################################

[PRISM_DRIVER_A02.Service]
 DisplayName    = %WUSB54GSRV%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\WUSB20XP.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_A02.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM_A02"
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"0"

[COMMON_NDIS.reg]
 HKR,                   ,DeviceVxDs             ,0      ,"WUSB209x.sys"
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
; HKR,NDI                ,NdiInstaller           ,0      ,"USBCoI9x.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"WUSB209x"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.NT]
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,,RTSThresh,0,2432
 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,step,0,1
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,,FragThresh,0,2346
 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2
 HKR,NDI\params\FragThresh,optional,0,1

 HKR,,ShortRetryLimit,0,7
 HKR,NDI\params\ShortRetryLimit,default,0,7
 HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
 HKR,NDI\params\ShortRetryLimit,type,,int
 HKR,NDI\params\ShortRetryLimit,min,0,1
 HKR,NDI\params\ShortRetryLimit,max,0,255
 HKR,NDI\params\ShortRetryLimit,step,0,1
 HKR,NDI\params\ShortRetryLimit,optional,0,1

 HKR,,LongRetryLimit,0,4
 HKR,NDI\params\LongRetryLimit,default,0,4
 HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
 HKR,NDI\params\LongRetryLimit,type,0,int
 HKR,NDI\params\LongRetryLimit,min,0,1
 HKR,NDI\params\LongRetryLimit,max,0,255
 HKR,NDI\params\LongRetryLimit,step,0,1
 HKR,NDI\params\LongRetryLimit,optional,0,1

 HKR,,ConfigProfile,0,256
 HKR,NDI\params\ConfigProfile,default,0,256
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,,enum
 HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 ;HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
 HKR,NDI\params\ConfigProfile,optional,0,1

 HKR,,NitroMode,0,"1"
 ;HKR,NDI\params\NitroMode,default,0,1
 ;HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 ;HKR,NDI\params\NitroMode,type,,enum
 ;HKR,NDI\params\NitroMode,flag,1,30,00,00,00
 ;HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 ;HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
 ;HKR,NDI\params\NitroMode,optional,0,1

 HKR,,PSMode,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1

;###############################################################################

[DestinationDirs]
 DefaultDestDir       = 11 
 USB_DRIVER.copy      = 11 
 USB_DRIVER.copy.NT   = 12 

[USB_DRIVER.copy]
 WUSB209x.sys

[USB_DRIVER.copy.NT]
 WUSB20XP.sys

[SourceDisksNames]
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]
 WUSB209x.sys           = 1

[SourceDisksFiles.X86]
 WUSB20XP.sys           = 1

;###############################################################################

[Strings]
 VER_VENDOR_STR          = "The Cisco-Linksys, LLC."
 VER_VENDOR_NAME_STR     = "The Cisco-Linksys, LLC."
 WUSB54G                 = "Linksys Wireless-G USB Network Adapter"
 WUSB54GP                = "Linksys Wireless-G Portable USB Adapter"
 
 WUSB54GSRV              = "802.11a/g USB Driver"
 INSTALL_DISK_STR        = "Linksys Wireless-G USB Network Adapter Install Disk"

 ON_STR                  = "On"
 OFF_STR                 = "Off"
 RTSTHRESH_STR           = "RTS Threshold"
 FRAGTHRESH_STR          = "Fragmentation Threshold"
 AUTHENT_TYPE_STR        = "Authentication Algorithm"
 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic"
 POWER_SAVE_MAX_STR      = "Maximum"
 SHORT_RETRY_STR         = "Short Retry Limit"
 LONG_RETRY_STR          = "Long Retry Limit"
 CONFIG_PROFILE          = "Configuration Profile"
 CONFIG_PROF_B_ONLY      = "B only"
 CONFIG_PROF_MIXED       = "Mixed"
 CONFIG_PROF_MIXED_LONG  = "Mixed Long"
 CONFIG_PROF_G_ONLY      = "G only"
 CONFIG_PROF_TEST        = "Test"
 CONFIG_PROF_B_WIFI      = "B WiFi"
 CONFIG_PROF_MIXED_SHORT = "Mixed Short"
 CONFIG_PROF_WIFI_SPEC   = "WiFi Spec"
 NITRO_MODE              = "Nitro Mode"