;------------------------------------------------------------------------
;
;   Copyright and Disclaimer:
;
;       This software is provided "as is" without warranty of any kind,
;       either expressed or implied, including but not limited to the
;       implied warranties of merchantability and/or fitness for a
;       particular purpose.
;
;       Copyright (C) AVerMedia
;       All Rights Reserved.
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="AVerMedia TECHNOLOGIES, Inc."
DriverVer=06/02/2009,1.12.0.87
CatalogFile.ntx86=A885VCap.cat

[Manufacturer]
"AVerMedia TECHNOLOGIES, Inc."=Models,NT.6

[SourceDisksNames]
1="AVerMedia CX23885 Drivers",,,""

[SourceDisksFiles]
A885VCap.sys=1
cx416enc.rom=1
merlinAVC.rom=1
cpnotify.ax=1
;encprxypage.ax=1
cxtvrate.dll=1

[Models]

;-----------------------------------------------
; Sonora Zarlink353/Xceive EVK/416 MPEG2 Encoder
;-----------------------------------------------
;%CX23885.Sonora%=CX23885.Sonora,PCI\VEN_14F1&DEV_8852&SUBSYS_003714F1

;-----------------------------------------------
; XC3028 + Afa9013
;-----------------------------------------------
%CX23885.A577%=CX23885.A577,       PCI\VEN_14F1&DEV_8852&SUBSYS_C0391461          ;PCI-e     XCeive+FM+AFa9013
%CX23885.A306%=CX23885.A306,       PCI\VEN_14F1&DEV_8852&SUBSYS_C1391461          ;mini card XCeive+FM+AFa9013
%CX23885.HC81%=CX23885.HC81,       PCI\VEN_14F1&DEV_8852&SUBSYS_C2391461          ;PCI-e     XCeive+FM+AFa9013
%CX23885.A303%=CX23885.A303,       PCI\VEN_14F1&DEV_8852&SUBSYS_C3391461          ;mini card XCeive+AFa9013+NEC61151 (A303-A)
%CX23885.M787%=CX23885.M787,       PCI\VEN_14F1&DEV_8852&SUBSYS_C4391461          ;PCI-e     XCeive+FM+AFa9013 (DELL)
%CX23885.M787ENC%=CX23885.M787ENC, PCI\VEN_14F1&DEV_8852&SUBSYS_C5391461          ;PCI-e     XCeive+FM+AFa9013+23417
%CX23885.A303%=CX23885.A303,       PCI\VEN_14F1&DEV_8852&SUBSYS_C6391461          ;mini card XCeive+AFa9013+NEC61151 (A303-B)
%CX23885.M787%=CX23885.M787_HP,    PCI\VEN_14F1&DEV_8852&SUBSYS_C8391461          ;PCI-e     XCeive+FM+AFa9013 (HP)
%CX23888.A307%=CX23885.A307,       PCI\VEN_14F1&DEV_8852&SUBSYS_C9391461          ;mini card XCeive+FM+LG3303
%CX23885.M787%=CX23885.M787_FU,    PCI\VEN_14F1&DEV_8852&SUBSYS_CA391461          ;PCI-e     XCeive+FM+AFa9013 (Fujitsu)
%CX23885.A303%=CX23885.A303_C,     PCI\VEN_14F1&DEV_8852&SUBSYS_CB391461

%CX23885.M787%=CX23885.M787_C,           PCI\VEN_14F1&DEV_8852&SUBSYS_CC391461    ;PCI-e     XCeive+CE6353, D
%CX23885.M787%=CX23885.M787_ATSC,        PCI\VEN_14F1&DEV_8852&SUBSYS_CD391461    ;PCI-e     XCeive+LGD3304, D
;%CX23885.M787%=CX23885.M787ENC_ATSC,     PCI\VEN_14F1&DEV_8852&SUBSYS_CE391461    ;PCI-e     XCeive+LGD3304+CX23417, D
%CX23885.M787%=CX23885.M787ENC_C,        PCI\VEN_14F1&DEV_8852&SUBSYS_CF391461    ;PCI-e     XCeive+CE6353+CX23417, D
%CX23885.M787HP%=CX23885.M787_C_HP,      PCI\VEN_14F1&DEV_8852&SUBSYS_D0391461    ;PCI-e     XCeive+CE6353 (HP)
%CX23885.HC81%=CX23885.HC81_B,           PCI\VEN_14F1&DEV_8852&SUBSYS_D2391461    ;PCI-e     XCeive_L+FM+Afa9013
%CX23885.M787FU%=CX23885.M787_C_FU,      PCI\VEN_14F1&DEV_8852&SUBSYS_D5391461    ;PCI-e     XCeive+FM+CE6353 (FU)

%CX23885.A577A%=CX23885.A577A,           PCI\VEN_14F1&DEV_8852&SUBSYS_D6391461    ;PCI-e     XCeive+FM
%CX23885.M787GTW%=CX23885.M787_C_GTW,    PCI\VEN_14F1&DEV_8852&SUBSYS_D8391461    ;PCI-e     XCeive+CE6353 (GTW)
%CX23885.HC81R%=CX23885.HC81_C,          PCI\VEN_14F1&DEV_8852&SUBSYS_D9391461    ;PCI-e     XCeive_L+FM+Afa9013

%CX23885.M787%=CX23885.M787R_HYBRID,     PCI\VEN_14F1&DEV_8852&SUBSYS_DA391461    ;PCI-e     XCeive+MT353+FM+Remote, Retail
%CX23885.M787A%=CX23885.M787R_ANAOLG,    PCI\VEN_14F1&DEV_8852&SUBSYS_DB391461    ;PCI-e     XCeive+FM+Remote, Retail
%CX23885.M787D%=CX23885.M787R_DVBT,      PCI\VEN_14F1&DEV_8852&SUBSYS_DC391461    ;PCI-e     XCeive+MT353+Remote, Retail
%CX23885.M787A%=CX23885.M787_ANAOLG_HP,  PCI\VEN_14F1&DEV_8852&SUBSYS_DD391461    ;PCI-e     XCeive+FM+Remote, (HP)

%CX23888.A307_B%=CX23885.A307_B,         PCI\VEN_14F1&DEV_8852&SUBSYS_E3391461    ;PCI-e mini card, XCeive+FM


;%CX23885.A306%=CX23885.A306,       PCI\VEN_14F1&DEV_8852

[Models.NT.6]

%CX23885.A577%=CX23885.A577_Vista,       PCI\VEN_14F1&DEV_8852&SUBSYS_C0391461    ;PCI-e     XCeive+FM+AFa9013
%CX23885.A306%=CX23885.A306,       	     PCI\VEN_14F1&DEV_8852&SUBSYS_C1391461    ;mini card XCeive+FM+AFa9013
%CX23885.HC81%=CX23885.HC81,       	     PCI\VEN_14F1&DEV_8852&SUBSYS_C2391461    ;PCI-e     XCeive+FM+AFa9013
%CX23885.A303%=CX23885.A303,       	     PCI\VEN_14F1&DEV_8852&SUBSYS_C3391461    ;mini card XCeive+AFa9013+NEC61151 (A303-A)
%CX23885.M787%=CX23885.M787,       	     PCI\VEN_14F1&DEV_8852&SUBSYS_C4391461    ;PCI-e     XCeive+FM+AFa9013 (DELL)
%CX23885.M787ENC%=CX23885.M787ENC, 	     PCI\VEN_14F1&DEV_8852&SUBSYS_C5391461    ;PCI-e     XCeive+FM+AFa9013+23417
%CX23885.A303%=CX23885.A303,       	     PCI\VEN_14F1&DEV_8852&SUBSYS_C6391461    ;mini card XCeive+AFa9013+NEC61151 (A303-B)
%CX23885.M787%=CX23885.M787_HP,    	     PCI\VEN_14F1&DEV_8852&SUBSYS_C8391461    ;PCI-e     XCeive+FM+AFa9013 (HP)
%CX23888.A307%=CX23885.A307,        	 PCI\VEN_14F1&DEV_8852&SUBSYS_C9391461    ;mini card XCeive+FM+LG3303
%CX23885.M787%=CX23885.M787_FU,     	 PCI\VEN_14F1&DEV_8852&SUBSYS_CA391461    ;PCI-e     XCeive+FM+AFa9013 (Fujitsu)
%CX23885.A303%=CX23885.A303_C,      	 PCI\VEN_14F1&DEV_8852&SUBSYS_CB391461

%CX23885.M787%=CX23885.M787_C,           PCI\VEN_14F1&DEV_8852&SUBSYS_CC391461    ;PCI-e     XCeive+CE6353, D
%CX23885.M787%=CX23885.M787_ATSC,        PCI\VEN_14F1&DEV_8852&SUBSYS_CD391461    ;PCI-e     XCeive+LGD3304, D
;%CX23885.M787%=CX23885.M787ENC_ATSC,    PCI\VEN_14F1&DEV_8852&SUBSYS_CE391461    ;PCI-e     XCeive+LGD3304+CX23417, D
%CX23885.M787%=CX23885.M787ENC_C,        PCI\VEN_14F1&DEV_8852&SUBSYS_CF391461    ;PCI-e     XCeive+CE6353+CX23417, D
%CX23885.M787HP%=CX23885.M787_C_HP,      PCI\VEN_14F1&DEV_8852&SUBSYS_D0391461    ;PCI-e     XCeive+CE6353 (HP)
%CX23885.HC81%=CX23885.HC81_B,           PCI\VEN_14F1&DEV_8852&SUBSYS_D2391461    ;PCI-e     XCeive_L+FM+Afa9013
%CX23885.M787FU%=CX23885.M787_C_FU,      PCI\VEN_14F1&DEV_8852&SUBSYS_D5391461    ;PCI-e     XCeive+FM+CE6353 (FU)

%CX23885.A577A%=CX23885.A577A,           PCI\VEN_14F1&DEV_8852&SUBSYS_D6391461    ;PCI-e     XCeive+FM
%CX23885.M787GTW%=CX23885.M787_C_GTW,    PCI\VEN_14F1&DEV_8852&SUBSYS_D8391461    ;PCI-e     XCeive+CE6353 (GTW)
%CX23885.HC81R%=CX23885.HC81_C,          PCI\VEN_14F1&DEV_8852&SUBSYS_D9391461    ;PCI-e     XCeive_L+FM+Afa9013

%CX23885.M787%=CX23885.M787R_HYBRID,     PCI\VEN_14F1&DEV_8852&SUBSYS_DA391461    ;PCI-e     XCeive+MT353+FM+Remote, Retail
%CX23885.M787A%=CX23885.M787R_ANAOLG,    PCI\VEN_14F1&DEV_8852&SUBSYS_DB391461    ;PCI-e     XCeive+FM+Remote, Retail
%CX23885.M787D%=CX23885.M787R_DVBT,      PCI\VEN_14F1&DEV_8852&SUBSYS_DC391461    ;PCI-e     XCeive+MT353+Remote, Retail
%CX23885.M787A%=CX23885.M787_ANAOLG_HP,  PCI\VEN_14F1&DEV_8852&SUBSYS_DD391461    ;PCI-e     XCeive+FM+Remote, (HP)

%CX23888.A307_B%=CX23885.A307_B,         PCI\VEN_14F1&DEV_8852&SUBSYS_E3391461    ;PCI-e mini card, XCeive+FM

;-----------------------------------------------------------------------------------------
; Model Sonora
;-----------------------------------------------------------------------------------------
[CX23885.Sonora]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,Sonora.AddReg,SonoraXBAR.AddReg,CX23885.Xceive.AddReg,Xceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.Sonora.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,Sonora.AddReg,SonoraXBAR.AddReg,CX23885.Xceive.AddReg,Xceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.Sonora.Interfaces]
Needs=VID.Interfaces

[CX23885.Sonora.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.Sonora.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.Sonora.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[Sonora.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0xFE, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","comp_select_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x00, 0x00, 0x00, 0x00

;BoardType Sonora353 = 0x03
HKR,"DriverData","BoardType",0x00010001, 0x03, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model A577
;-----------------------------------------------------------------------------------------
[CX23885.A577]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A577.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.A577.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A577.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.A577.Interfaces]
Needs=VID.Interfaces

[CX23885.A577.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.A577.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.A577.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[A577.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
;HKR,"ENUM\CIR",pnpid,,"AVerIR"
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00

; 0:NEC standard, 1:RC6A standard
HKR,"DriverData","IRStandard",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","MCEREMOTE",0x00010001, 0x00, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","comp_select_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType A577= 0x0D
HKR,"DriverData","BoardType",0x00010001, 0x0D, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model A577 Vista
;-----------------------------------------------------------------------------------------
[CX23885.A577_Vista]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A577_Vista.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.A577_Vista.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A577_Vista.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.A577_Vista.Interfaces]
Needs=VID.Interfaces

[CX23885.A577_Vista.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.A577_Vista.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.A577_Vista.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[A577_Vista.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"ENUM\CIR",pnpid,,"AVerIR"
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00

; 0:NEC standard, 1:RC6A standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","MCEREMOTE",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","comp_select_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType A577= 0x0D
HKR,"DriverData","BoardType",0x00010001, 0x0D, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model A577A
;-----------------------------------------------------------------------------------------
[CX23885.A577A]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A577A.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.A577A.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A577A.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.A577A.Interfaces]
Needs=VID.Interfaces

[CX23885.A577A.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.A577A.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.A577A.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[A577A.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","comp_select_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType A577A= 0x1C
HKR,"DriverData","BoardType",0x00010001, 0x1C, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model A306
;-----------------------------------------------------------------------------------------
[CX23885.A306]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A306.AddReg,AVerXBAR_11.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.A306.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A306.AddReg,AVerXBAR_11.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.A306.Interfaces]
Needs=VID.Interfaces

[CX23885.A306.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.A306.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.A306.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[A306.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x3A, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit",  0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",  0x00010001, 0x03, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",  0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit", 0x00010001, 0x01, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType A306= 0x0C
HKR,"DriverData","BoardType",0x00010001, 0x0C, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x01, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00
 
;ASPM
HKR,"DriverData","ASPM",0x00010001, 0x00, 0x00, 0x00, 0x00		;Enable L0s
HKR,"DriverData","ASPMForced",0x00010001, 0x00, 0x00, 0x00, 0x00	;Not forced.

;-----------------------------------------------------------------------------------------
; Model HC81
;-----------------------------------------------------------------------------------------
[CX23885.HC81]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg, HC81.AddReg, AVerXBAR_B.AddReg, CX23885.Xceive.AddReg, AVerXceive.AddReg, CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.HC81.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg, HC81.AddReg, AVerXBAR_B.AddReg, CX23885.Xceive.AddReg, AVerXceive.AddReg, CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.HC81.Interfaces]
Needs=VID.Interfaces

[CX23885.HC81.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.HC81.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.HC81.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[HC81.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit",  0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",  0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",  0x00010001, 0x01, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType HC81= 0x10
HKR,"DriverData","BoardType",0x00010001, 0x10, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model HC81_B
;-----------------------------------------------------------------------------------------
[CX23885.HC81_B]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg, HC81_B.AddReg, AVerXBAR_B.AddReg, CX23885.Xceive.AddReg, AVerXceiveL.AddReg, CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.HC81_B.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg, HC81_B.AddReg, AVerXBAR_B.AddReg, CX23885.Xceive.AddReg, AVerXceiveL.AddReg, CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.HC81_B.Interfaces]
Needs=VID.Interfaces

[CX23885.HC81_B.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.HC81_B.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.HC81_B.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[HC81_B.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x03, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit",  0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",  0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",  0x00010001, 0x01, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType HC81_B= 0x1B
HKR,"DriverData","BoardType",0x00010001, 0x1b, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model HC81_C
;-----------------------------------------------------------------------------------------
[CX23885.HC81_C]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg, HC81_C.AddReg, AVerXBAR_B.AddReg, CX23885.Xceive.AddReg, AVerXceiveL.AddReg, CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.HC81_C.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg, HC81_C.AddReg, AVerXBAR_B.AddReg, CX23885.Xceive.AddReg, AVerXceiveL.AddReg, CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.HC81_C.Interfaces]
Needs=VID.Interfaces

[CX23885.HC81_C.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.HC81_C.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.HC81_C.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[HC81_C.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x03, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit",  0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",  0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",  0x00010001, 0x01, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x00, 0x00, 0x00, 0x00

;BoardType HC81_C= 0x1E
HKR,"DriverData","BoardType",0x00010001, 0x1e, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model A303
;-----------------------------------------------------------------------------------------
[CX23885.A303]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A303.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.A303.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A303.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.A303.Interfaces]
Needs=VID.Interfaces

[CX23885.A303.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.A303.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.A303.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[A303.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x03, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x00, 0x00, 0x00, 0x00

;BoardType A303= 0x0F
HKR,"DriverData","BoardType",0x00010001, 0x0F, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model A303-C
;-----------------------------------------------------------------------------------------
[CX23885.A303_C]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A303_C.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.A303_C.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A303_C.AddReg,AVerXBAR_B.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.A303_C.Interfaces]
Needs=VID.Interfaces

[CX23885.A303_C.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.A303_C.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.A303_C.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[A303_C.AddReg]
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",            0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",         0x00010001, 0x00,0x00,0x00,0x00

HKR,"DriverData","TunerModel",           0x00010001, 0x03, 0x00, 0x00, 0x00
HKR,"DriverData","Enable_BDA",           0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type", 0x00010001, 0x04, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",      0x00010001, 0x00, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x03, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0x01, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x00, 0x00, 0x00, 0x00

;BoardType A303_C = 0x13
HKR,"DriverData","BoardType",0x00010001, 0x13, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model M787
;-----------------------------------------------------------------------------------------
[CX23885.M787]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787.Interfaces]
Needs=VID.Interfaces

[CX23885.M787.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
;HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"DriverData","comp_select_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00


; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787= 0x11
HKR,"DriverData","BoardType",0x00010001, 0x11, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x00, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00


;-----------------------------------------------------------------------------------------
; Model M787_HP
;-----------------------------------------------------------------------------------------
[CX23885.M787_HP]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_HP.AddReg,AVerXBAR_D.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787_HP.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_HP.AddReg,AVerXBAR_D.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787_HP.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_HP.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_HP.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787_HP.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787_HP.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
;HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"DriverData","comp_select_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00


; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787= 0x11
HKR,"DriverData","BoardType",0x00010001, 0x11, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x00, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00


;-----------------------------------------------------------------------------------------
; Model M787_FU
;-----------------------------------------------------------------------------------------
[CX23885.M787_FU]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_FU.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787_FU.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_FU.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787_FU.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_FU.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_FU.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787_FU.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787_FU.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x38, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
;HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"DriverData","comp_select_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787= 0x11
HKR,"DriverData","BoardType",0x00010001, 0x11, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x01, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model M787ENC
;-----------------------------------------------------------------------------------------
[CX23885.M787ENC]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787ENC.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787ENC.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787ENC.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787ENC.Interfaces]
Needs=VID.Interfaces

[CX23885.M787ENC.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787ENC.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787ENC.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787ENC.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x3A, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
;HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x00, 0x00, 0x00, 0x00
;HKR,"DriverData","comp_select_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00


; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787ENC= 0x12
HKR,"DriverData","BoardType",0x00010001, 0x12, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00


;-----------------------------------------------------------------------------------------
; Model M787_C
;-----------------------------------------------------------------------------------------
[CX23885.M787_C]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_C.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787_C.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_C.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787_C.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_C.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_C.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787_C.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787_C.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x06, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",0x00010001, 0x03, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787_C= 0x15
HKR,"DriverData","BoardType",0x00010001, 0x15, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x00, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model M787_ATSC
;-----------------------------------------------------------------------------------------
[CX23885.M787_ATSC]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_ATSC.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787_ATSC.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_ATSC.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787_ATSC.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_ATSC.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_ATSC.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787_ATSC.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787_ATSC.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR, "DriverData", "Enable_BDA",           0x00010001, 0x01, 0x00, 0x00, 0x00
HKR, "DriverData", "BDA_Demod_Tuner_type", 0x00010001, 0x07, 0x00, 0x00, 0x00
HKR, "DriverData", "TunerI2CAddress",      0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR, "DriverData", "TunerI2CBus",          0x00010001, 0x02, 0x00, 0x00, 0x00
HKR, "DriverData", "DemodI2CAddress",      0x00010001, 0x1D, 0x00, 0x00, 0x00
HKR, "DriverData", "DemodI2CBus",          0x00010001, 0x01, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x01, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787_ATSC= 0x1D
HKR,"DriverData","BoardType",0x00010001, 0x1D, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x00, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00


;-----------------------------------------------------------------------------------------
; Model M787_C_HP
;-----------------------------------------------------------------------------------------
[CX23885.M787_C_HP]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_C_HP.AddReg,AVerXBAR_D.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787_C_HP.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_C_HP.AddReg,AVerXBAR_D.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787_C_HP.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_C_HP.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_C_HP.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787_C_HP.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787_C_HP.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x06, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",0x00010001, 0x03, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787_C= 0x15
HKR,"DriverData","BoardType",0x00010001, 0x15, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x00, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model M787ENC_C
;-----------------------------------------------------------------------------------------
[CX23885.M787ENC_C]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787ENC_C.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787ENC_C.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787ENC_C.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787ENC_C.Interfaces]
Needs=VID.Interfaces

[CX23885.M787ENC_C.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787ENC_C.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787ENC_C.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787ENC_C.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x06, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",0x00010001, 0x70, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787ENC_C= 0x16
HKR,"DriverData","BoardType",0x00010001, 0x16, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x00, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model M787_C_FU
;-----------------------------------------------------------------------------------------
[CX23885.M787_C_FU]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_C_FU.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787_C_FU.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_C_FU.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787_C_FU.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_C_FU.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_C_FU.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787_C_FU.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787_C_FU.AddReg]

;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x06, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

;HKR,"DriverData","MCEREMOTE",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",0x00010001, 0x03, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787_C= 0x15
HKR,"DriverData","BoardType",0x00010001, 0x15, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x01, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00


;-----------------------------------------------------------------------------------------
; Model M787_C_GTW
;-----------------------------------------------------------------------------------------
[CX23885.M787_C_GTW]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_C_GTW.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787_C_GTW.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_C_GTW.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787_C_GTW.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_C_GTW.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_C_GTW.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787_C_GTW.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787_C_GTW.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x06, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",0x00010001, 0x03, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787_C= 0x15
HKR,"DriverData","BoardType",0x00010001, 0x15, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x00, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00


;-----------------------------------------------------------------------------------------
; Model M787R_HYBRID
;-----------------------------------------------------------------------------------------
[CX23885.M787R_HYBRID]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787R_HYBRID.AddReg,AVerXBAR_F.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787R_HYBRID.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787R_HYBRID.AddReg,AVerXBAR_F.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787R_HYBRID.Interfaces]
Needs=VID.Interfaces

[CX23885.M787R_HYBRID.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787R_HYBRID.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787R_HYBRID.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787R_HYBRID.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x06, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",0x00010001, 0x03, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787_C= 0x15
HKR,"DriverData","BoardType",0x00010001, 0x15, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x01, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model M787R_ANAOLG
;-----------------------------------------------------------------------------------------
[CX23885.M787R_ANAOLG]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787R_ANAOLG.AddReg,AVerXBAR_F.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787R_ANAOLG.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787R_ANAOLG.AddReg,AVerXBAR_F.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787R_ANAOLG.Interfaces]
Needs=VID.Interfaces

[CX23885.M787R_ANAOLG.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787R_ANAOLG.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787R_ANAOLG.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787R_ANAOLG.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x06, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787R_ANALOG = 0x1F
HKR,"DriverData","BoardType",0x00010001, 0x1F, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x01, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model M787R_DVBT
;-----------------------------------------------------------------------------------------
[CX23885.M787R_DVBT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787R_DVBT.AddReg,AVerXBAR_10.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787R_DVBT.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787R_DVBT.AddReg,AVerXBAR_10.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787R_DVBT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787R_DVBT.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787R_DVBT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787R_DVBT.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787R_DVBT.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x06, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit",0x00010001, 0x03, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787R_DVBT = 0x20
HKR,"DriverData","BoardType",0x00010001, 0x20, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x01, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model M787_ANAOLG_HP
;-----------------------------------------------------------------------------------------
[CX23885.M787_ANAOLG_HP]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_ANAOLG_HP.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.M787_ANAOLG_HP.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,M787_ANAOLG_HP.AddReg,AVerXBAR_C.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.M787_ANAOLG_HP.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_ANAOLG_HP.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.M787_ANAOLG_HP.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.M787_ANAOLG_HP.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[M787_ANAOLG_HP.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x06, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType M787R_ANALOG = 0x1F
HKR,"DriverData","BoardType",0x00010001, 0x1F, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x00, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;Use 25MHz Crystal
HKR,"DriverData","Use25MHz",0x00010001, 0x00, 0x00, 0x00, 0x00

;-----------------------------------------------------------------------------------------
; Model A307
;-----------------------------------------------------------------------------------------
[CX23885.A307]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A307.AddReg,AVerXBAR_E.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.A307.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A307.AddReg,AVerXBAR_E.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.A307.Interfaces]
Needs=VID.Interfaces

[CX23885.A307.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.A307.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.A307.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[A307.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x05, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1C, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit",       0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_powersaving_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit",       0x00010001, 0x03, 0x00, 0x00, 0x00
HKR,"DriverData","demod_powersaving_gpio_bit", 0x00010001, 0x01, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x01, 0x00, 0x00, 0x00

;BoardType A307= 0x14
HKR,"DriverData","BoardType",0x00010001, 0x14, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x01, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;ASPM
HKR,"DriverData","ASPM",0x00010001, 0x00, 0x00, 0x00, 0x00		;Enable L0s
HKR,"DriverData","ASPMForced",0x00010001, 0x00, 0x00, 0x00, 0x00	;Not forced.


;-----------------------------------------------------------------------------------------
; Model A307_B
;-----------------------------------------------------------------------------------------
[CX23885.A307_B]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A307_B.AddReg,AVerXBAR_E.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.A307_B.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,A307_B.AddReg,AVerXBAR_E.AddReg,CX23885.Xceive.AddReg,AVerXceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX23885.A307_B.Interfaces]
Needs=VID.Interfaces

[CX23885.A307_B.NT.Interfaces]
Needs=VID.Interfaces

[CX23885.A307_B.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[CX23885.A307_B.NT.Services]
AddService = CXSONORA,2,VID.ServiceInstall

[A307_B.AddReg]
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0x04, 0x00, 0x00, 0x00

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit",       0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_powersaving_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
;HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;BoardType A307_B = 0x21
HKR,"DriverData","BoardType",0x00010001, 0x21, 0x00, 0x00, 0x00

;SupportFM
HKR,"DriverData","SupportFM",0x00010001, 0x01, 0x00, 0x00, 0x00

;Init_I2C_Check, 0: don't chack,so driver will register all needed filters.
HKR,"DriverData","Init_I2C_Check",0x00010001, 0x01, 0x00, 0x00, 0x00

;ASPM
HKR,"DriverData","ASPM",0x00010001, 0x00, 0x00, 0x00, 0x00		;Enable L0s
HKR,"DriverData","ASPMForced",0x00010001, 0x00, 0x00, 0x00, 0x00	;Not forced.

;-----------------------------------------------------------------------------------------
[DestinationDirs]
CX885.CopyDrivers=10,system32\drivers
DSFilters.CopyFiles=11

[CX885.CopyDrivers]
A885VCap.sys
cx416enc.rom
; Merlin Rev. C audio firmware
merlinAVC.rom

[DSFilters.CopyFiles]
cpnotify.ax
;encprxypage.ax
cxtvrate.dll

[DSFilters.RegDLL]
11,,cpnotify.ax,1
;11,,encprxypage.ax,1
11,,cxtvrate.dll,1

[CX885.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,A885VCap.sys
HKR,,OkToHibernate,3,01
; Disable driver page out
HKR,,PageOutWhenUnopened,3,0
;HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKLM,%MediaCategories%\%GUID.PINNAME_ANALOG_AUDIO_IN%,Name,,%Pin.p2AnalogAudioIn%
HKLM,%MediaCategories%\%GUID.PINNAME_AUDIO_OUT%,Name,,%PinName.AnalogAudioOut%

;
;Register the name of the 656 and MPEG pins
;
HKLM,%MediaCategories%\%GUID.PINNAME_656_OUT%,Name,,%PinName.656_OUT%
HKLM,%MediaCategories%\%GUID.PINNAME_656_IN%,Name,,%PinName.656_IN%
HKLM,%MediaCategories%\%GUID.PINNAME_MPEG_OUT%,Name,,%PinName.MpegOut%

;
;Add the property pages
;
;HKCR,CLSID\%GUID.General_Properties%\InprocServer32,,,encprxypage.ax
;HKCR,CLSID\%GUID.General_Properties%\InprocServer32,ThreadingModel,,Both
;HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.General_Properties%,,,

;HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,,,encprxypage.ax
;HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,ThreadingModel,,Both
;HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Video_Properties%,,,

;HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,,,encprxypage.ax
;HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,ThreadingModel,,Both
;HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Audio_Properties%,,,

;HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,,,encprxypage.ax
;HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,ThreadingModel,,Both
;HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.MPEG_Properties%,,,

;HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,,,encprxypage.ax
;HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,ThreadingModel,,Both
;HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Diagnostic_Properties%,,,

;HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,,,encprxypage.ax
;HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,ThreadingModel,,Both
;HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Noise_Properties%,,,

;Register the encoder and multiplexer classes with Direct X
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,CLSID,,%GUID.Encoder%
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,FriendlyName,,%Category_Encoders%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,CLSID,,%GUID.Multiplexer%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,FriendlyName,,%Category_Multiplexers%

;Register the names of the encoder and multiplexer nodes
HKLM,%MediaCategories%\%GUID.Encoder%,Name,,%Node.Encoder%
HKLM,%MediaCategories%\%GUID.Encoder%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%GUID.Multiplexer%,Name,,%Node.Multiplexer%
HKLM,%MediaCategories%\%GUID.Multiplexer%,Display,1,00,00,00,00

HKLM,%MediaInterfaces%\{0A7AF963-6805-4f99-B284-29B680975542},,,"Copy Protect Notification Filter"
HKLM,%MediaInterfaces%\{0A7AF963-6805-4f99-B284-29B680975542},IID,1,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

;Wave in audio device registration
HKR,Drivers,SubClasses,,"wave"
HKR,Drivers\wave\wdmaud.drv, Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,%AudioFriendlyName%

;Add the property pages
;HKCR,CLSID\%GUID.General_Properties%\InprocServer32,,,cxcorona.ax
;HKCR,CLSID\%GUID.General_Properties%\InprocServer32,ThreadingModel,,Both
;HKLM,%MediaSets%\%GUID.CORONA_VERSION_PROPERTIES%\PropertyPages\%GUID.General_Properties%,,,


[CX23885.Xceive.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00


;-------------------------------------------------------------------
; Crossbar AddReg sections
;
;---Crossbar registry values---
;
; Note: For each pin on the crossbar, specify the following:
; (1) Pin type 
;     0 - TunerIn
;     1 - Composite 1
;     2 - SVideo 1
;     3 - Component
;     4 - Composite 2
;     5 - SVideo 2
;     6 - Audio from Tuner
;     7 - Audio from Line In
;     8 - Audio from Line In 2
; (2) InputMux (optional) - input mux to use for the selected pin
;     in 0xAA, 0xBB, 0xCC, 0x00 format
;     where AA is the input mux for Composite/S-Video Luma/Component Luma
;           BB is the input mux for Tuner Audio/S-Video Chroma/Component YPr
;           CC is the input mux for Component YPb
; (3) InputChannel (optional, but required if InputMux present) - Input channel 
;     to use for mux in 0xAA, 0xBB, 0xCC, 0xDD format
;     where AA is the input channel for Composite/S-Video Luma/Component Luma
;           BB is the input channel for Tuner Audio/S-Video Chroma/Component YPr
;           CC is the input channel for Component YPb 
;           DD = 1 if dual ADC2 mode required, zero if single mode
; (4) RelatedPinIndex 
;
;-------------------------------------------------------------------

[SonoraXBAR.AddReg]

;Pin 0 - Tuner In
; Input MUX       : VIN2 for video, VIN5 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin6 
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x02,0x05,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00

;Pin 1 - Composite 1 (Rear)
; Input Mux       : VIN1 for Composite
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 2 - S-Video 1 (Rear)
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Lume, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 3 - Component 1 (Rear)
; Input Mux       : VIN8 for Luma, VIN6 for YPb, VIN7 for YPr
; Input Channel   : Ch1 for  Lume, Ch2  for YPb, Ch3  for YPr, Dual ADC
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","InputMux",0x00010001, 0x08,0x06,0x07,0x00
HKR,"DriverData\XBarPin3","InputChannel",0x00010001, 0x01,0x02,0x03,0x01
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 4 - Composite 2 (Front) 
; Input Mux       : VIN1 for Composite - same as Composite1 - switched with GPIO0 MUX
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 2 - Pin8
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x08,0x00,0x00,0x00

;Pin 5 - S-Video 2 (Front)
; Input Mux       : VIN3 for Luma, VIN4 for Chroma
; Input Channel   : Ch1 for  Luma, Ch2  for Chroma
; Related PinIndex: Audio Line In 2 - Pin8
HKR,"DriverData\XBarPin5","PinType",0x00010001, 0x05,0x00,0x00,0x00
HKR,"DriverData\XBarPin5","InputMux",0x00010001, 0x03,0x04,0x00,0x00
HKR,"DriverData\XBarPin5","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin5","RelatedPinIndex",0x00010001, 0x08,0x00,0x00,0x00

;Pin 6 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin6","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin6","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 7 - Audio Line In 1 (Rear)
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBarPin7","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin7","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Pin 8 - Audio Line In 2 (Front)
; Related PinIndex: Composite 2 - Pin4
HKR,"DriverData\XBarPin8","PinType",0x00010001, 0x08,0x00,0x00,0x00
HKR,"DriverData\XBarPin8","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

;---------------------------------------------------------------------------------
; AVerXBAR_A.AddReg ,single external input for A306
;---------------------------------------------------------------------------------

[AVerXBAR_A.AddReg]

;Pin 0 - Tuner In
; Input MUX       : VIN2 for video, VIN5 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin3 
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x02,0x05,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00

;Pin 1 - Composite 1 
; Input Mux       : VIN1 for Composite
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 1 - Pin4
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 2 - S-Video 1 
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Lume, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin4
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 3 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 4 - Audio Line In 1 
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

;---------------------------------------------------------------------------------
; AVerXBAR_B.AddReg ,single external input for A577
;---------------------------------------------------------------------------------

[AVerXBAR_B.AddReg]

;Pin 0 - Tuner In
; Input MUX       : VIN2 for video, VIN5 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin3 
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x02,0x05,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00

;Pin 1 - Composite 1 
; Input Mux       : VIN1 for Composite
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 1 - Pin4
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 2 - S-Video 1 
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Lume, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin4
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 3 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 4 - Audio Line In 1 
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x08,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00


;---------------------------------------------------------------------------------
; AVerXBAR_C.AddReg ,Dual external input for M787
;---------------------------------------------------------------------------------

[AVerXBAR_C.AddReg]

;Pin 0 - Tuner In
; Input MUX       : VIN3 for video, VIN4 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin5 
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x03,0x04,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x05,0x00,0x00,0x00

;Pin 1 - Composite 1 (Rear)
; Input Mux       : VIN1 for Composite
; Input Channel   : Ch2 for Composite
; Related PinIndex: Audio Line In 1 - Pin6
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00

;Pin 2 - S-Video 1 (Rear)
; Input Mux       : VIN6 for Luma, VIN5 for Chroma
; Input Channel   : Ch1 for  Lume, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin6
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x06,0x05,0x00,0x00
HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00

;Pin 3 - Composite 2 (Front) 
; Input Mux       : VIN2 for Composite 
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 2 - Pin7
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","InputMux",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 4 - S-Video 2 (Front)
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Luma, Ch2  for Chroma
; Related PinIndex: Audio Line In 2 - Pin7
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x05,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBarPin4","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 5 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin5","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin5","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 6 - Audio Line In 1 (Rear)
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBarPin6","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin6","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Pin 7 - Audio Line In 2 (Front)
; Related PinIndex: Composite 2 - Pin3
HKR,"DriverData\XBarPin7","PinType",0x00010001, 0x08,0x00,0x00,0x00
HKR,"DriverData\XBarPin7","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00

;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00


;---------------------------------------------------------------------------------
; AVerXBAR_D.AddReg ,M787 for HP
;---------------------------------------------------------------------------------

[AVerXBAR_D.AddReg]

;Pin 0 - Tuner In
; Input MUX       : VIN3 for video, VIN4 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin5 
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x03,0x04,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x05,0x00,0x00,0x00

;Pin 1 - Composite 1 (Rear)
; Input Mux       : VIN1 for Composite
; Input Channel   : Ch2 for Composite
; Related PinIndex: Audio Line In 1 - Pin6
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00


;Pin 2 - S-Video 1 (Rear)
; Input Mux       : VIN6 for Luma, VIN5 for Chroma
; Input Channel   : Ch1 for  Lume, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin6
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x06,0x05,0x00,0x00
HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00

;Pin 3 - Composite 2 (Front) 
; Input Mux       : VIN2 for Composite 
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 2 - Pin7
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","InputMux",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 4 - S-Video 2 (Front)
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Luma, Ch2  for Chroma
; Related PinIndex: Audio Line In 2 - Pin7
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x05,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBarPin4","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 5 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin5","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin5","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 6 - Audio Line In 1 (Rear)
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBarPin6","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin6","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Pin 7 - Audio Line In 2 (Front)
; Related PinIndex: Composite 2 - Pin3
HKR,"DriverData\XBarPin7","PinType",0x00010001, 0x08,0x00,0x00,0x00
HKR,"DriverData\XBarPin7","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00

;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

;---------------------------------------------------------------------------------
; AVerXBAR_E.AddReg for A307
;---------------------------------------------------------------------------------
[AVerXBAR_E.AddReg]

;Pin 0 - Tuner In
; Input MUX       : VIN3 for video, VIN4 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin6 
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x02,0x04,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00

;Pin 1 - S-Video
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Lume, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 2 - Composite
; Input Mux       : VIN5 for Composite 
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 2 - Pin8
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 3 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 4 - Audio Line In
; Related PinIndex: S-Video 1 - Pin1
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Tuner In input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

;---------------------------------------------------------------------------------
; AVerXBAR_F.AddReg for M787(Retail)
;---------------------------------------------------------------------------------
[AVerXBAR_F.AddReg]

;Pin 0 - Tuner In
; Input MUX       : VIN3 for video, VIN4 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin3 
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x03,0x04,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00

;Pin 1 - Composite
; Input Mux       : VIN1 for Composite
; Input Channel   : Ch2 for Composite
; Related PinIndex: Audio Line In - Pin4
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 2 - S-Video
; Input Mux       : VIN6 for Luma, VIN5 for Chroma
; Input Channel   : Ch1 for  Lume, Ch3  for Chroma
; Related PinIndex: Audio Line In - Pin4
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x06,0x05,0x00,0x00
HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 3 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 4 - Audio Line In
; Related PinIndex: Composite Pin1
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

;---------------------------------------------------------------------------------
; AVerXBAR_10.AddReg for M787(Retail pure digital)
;---------------------------------------------------------------------------------
[AVerXBAR_10.AddReg]

;Pin 0 - Composite
; Input Mux       : VIN1 for Composite
; Input Channel   : Ch2 for Composite
; Related PinIndex: Audio Line In - Pin2
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x02,0x00,0x00,0x00

;Pin 1 - S-Video
; Input Mux       : VIN6 for Luma, VIN5 for Chroma
; Input Channel   : Ch1 for  Lume, Ch3  for Chroma
; Related PinIndex: Audio Line In - Pin2
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x06,0x05,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x02,0x00,0x00,0x00

;Pin 2 - Audio Line In
; Related PinIndex: Composite Pin1
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

;---------------------------------------------------------------------------------
; AVerXBAR_11.AddReg, no external input for A306
;---------------------------------------------------------------------------------

[AVerXBAR_11.AddReg]

;Pin 0 - Tuner In
; Input MUX       : VIN2 for video, VIN5 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin3 
HKR,"DriverData\XBarPin0","PinType",         0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",        0x00010001, 0x02,0x05,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",    0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex", 0x00010001, 0x01,0x00,0x00,0x00

;Pin 1 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin1","PinType",         0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex", 0x00010001, 0x00,0x00,0x00,0x00

;-------------------------------------------------------------------
; Tuner AddReg sections
;-------------------------------------------------------------------

[Xceive.AddReg]
HKR,"DriverData","TunerType",0x00010001, 0x1A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00

[AVerXceive.AddReg]
HKR,"DriverData","TunerType",0x00010001, 0x64, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00

[AVerXceiveL.AddReg]
HKR,"DriverData","TunerType",0x00010001, 0x65, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00

;-------------------------------------------------------------------
; AddReg sections for TS filter
;-------------------------------------------------------------------

[CXTS.AddReg]
HKLM,%MediaCategories%\%TSPinID%,Display,1, 00,00,00,00
HKLM,%MediaCategories%\%TSPinID%,Name,,%TSPinName%

;
; Interfaces installation
;

;
; Video
;

[VID.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%KsNameFilter%,VID_Interface,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%TVAudioReferenceGuid%,TvAudio_Interface,
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%XBARReferenceGUID%,CX88XBAR_Interface,
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},%TunerReferenceGuid%,CX88TUNE_Interface,
;AddInterface={6994AD04-93EF-11D0-A3CC-00A0C9223196},%AudioReferenceGuid%,AUD_Interface,
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%BDATuneReferenceGuid%,BDATUNE_Interface,
; Debug interface for TS testing
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSReferenceGuid%,TS_Interface,
; Encoder interface
AddInterface=%GUID.Encoder%,%EncoderReferenceGuid%,ENCODER_Interface,
AddInterface=%GUID.Multiplexer%,%EncoderReferenceGuid%,ENCODER_Interface


[VID_Interface]
AddReg=VID_Interface.AddReg

[VID_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%VIDFriendlyName%

[TvAudio_Interface]
AddReg=TvAudio_Interface.AddReg

[TvAudio_Interface.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%TVAudioFriendlyName%

[CX88XBAR_Interface]
AddReg=CX88XBAR_Interface.AddReg

[CX88XBAR_Interface.AddReg]
HKR,,CLSID,,{71F96460-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%XBARFriendlyName%

[CX88TUNE_Interface]
AddReg=CX88TUNE_Interface.AddReg

[CX88TUNE_Interface.AddReg]
HKR,,CLSID,,{266EEE40-6C63-11cf-8A03-00AA006ECB65}
HKR,,FriendlyName,,%TunerFriendlyName%

[AUD_Interface]
AddReg=AUD_Interface.AddReg

[AUD_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%AudioFriendlyName%

[BDATUNE_Interface]
AddReg=BDATUNE_Interface.AddReg

[BDATUNE_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%BDATuneFriendlyName%

[TS_Interface]
AddReg=TS_Interface.AddReg

[TS_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%TSFriendlyName%

[ENCODER_Interface]
AddReg=ENCODER_Interface.AddReg

[ENCODER_Interface.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%EncoderFriendlyName%
;Add an interface for Microsoft's video bit rate property set
HKR,Interfaces\{B43C4EEC-8C32-4791-9102-508ADA5EE8E7},,,
HKR,Interfaces\{b05dabd9-56e5-4fdc-afa4-8a47e91f1c9c},,,
HKR,Capabilities,,,
HKR,Capabilities,"{BB4FAA02-596C-4129-8FB3-74E75421FA02}", 0x00010001,1

;
; Services installation
;

[VID.ServiceInstall]
DisplayName   = %CX23885.DeviceDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\A885VCap.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
KsNameFilter                 = "{9B365890-165F-11D0-A195-0020AFD156E4}"
Proxy.CLSID                  = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
CX23885.DeviceDesc           = "AVerMedia 23885 AvStream Video Capture"
CX23885.Sonora               = "Conexant CX23885 AVStream Video Capture (Sonora)"
CX23885.AFA                  = "AVerMedia CX23885 AVStream Video Capture (AFA)"
CX23885.A577                 = "AVerMedia A577 ExpressCard Hybrid DVB-T"
CX23885.A306                 = "AVerMedia A306 MiniCard Hybrid DVB-T"
CX23885.HC81                 = "AVerMedia HC81 PCI-e Hybrid DVB-T"
CX23885.A303                 = "AVerMedia A303 MiniCard Hybrid DVB-T"
CX23885.M787                 = "AVerMedia M787 PCI-e Hybrid DVB-T"
CX23885.M787ENC              = "AVerMedia M787 PCI-e Hybrid DVB-T(HW Encode)"
CX23888.A307                 = "AVerMedia A307 PCIe Hybrid NTSC/ATSC"
CX23888.A307_B               = "AVerMedia A307 PCI-e Pure Analog"
CX23885.M787HP               = "AVerMedia M787 PCI-e Hybrid DVB-T"
CX23885.M787FU               = "AVerMedia M787 PCI-e Hybrid DVB-T"
CX23885.M787GTW              = "AVerMedia M787 PCI-e Hybrid DVB-T"
CX23885.A577A                = "AVerMedia A577A ExpressCard Analog TV"
CX23885.HC81R                = "AVerMedia HC81R PCI-e Hybrid DVB-T"
CX23885.M787A                = "AVerMedia M787 PCI-e Pure Analog"
CX23885.M787D                = "AVerMedia M787 PCI-e Pure DVB-T"

VIDFriendlyName              = "AVerMedia 23885 Video Capture"
MediaCategories              = "SYSTEM\CurrentControlSet\Control\MediaCategories"
GUID.PINNAME_ANALOG_AUDIO_IN = "{04394D28-52A7-4c46-AED0-65D62CC64DA6}"
Pin.p2AnalogAudioIn          = "Analog Audio In"
GUID.PINNAME_AUDIO_OUT       = "{9DA02733-7910-40f2-95DD-0441676C9A9B}"
PinName.AnalogAudioOut       = "Audio Out"
TVAudioFriendlyName          = "AVerMedia 23885 TvAudio"
TVAudioReferenceGuid         = "{991182D5-71A2-4b5c-9817-F551FBBC8232}"
XBARFriendlyName             = "AVerMedia 23885 Crossbar"
XBARReferenceGUID            = "{77F656DA-696D-407c-BA1C-50E4457C12E8}"
TunerFriendlyName            = "AVerMedia 23885 Tuner"
TunerReferenceGuid           = "{5618011C-A4DA-455b-A448-EC2AF3DCCB02}"
TSPinID                      = "{5237C937-0A21-4f7e-B338-DE0D0793D03F}"
TSPinName                    = "TS Out"
BDATuneFriendlyName          = "AVerMedia 23885 BDA Tuner/Demod"
BDATuneReferenceGuid         = "{E01E1072-3DF3-4c23-B99F-6A27A7CC7CD2}"
TSFriendlyName               = "AVerMedia 23885 AVStream TS Capture"
TSReferenceGuid              = "{5ea9c066-1dfe-41c5-a2de-bf766e83c98e}"
AudioFriendlyName            = "AVerMedia 23885 Audio Capture"
AudioReferenceGuid           = "{AB766B70-AFB3-4461-A4DE-22E9C516B7FE}"

EncoderFriendlyName          = "AVerMedia 23885 MPEG Encoder"
EncoderReferenceGuid         = "{1C10193D-7DCA-4f55-99D8-B017AAD3921D}"
GUID.Encoder                 = "{19689BF6-C384-48fd-AD51-90E58C79F70B}"
GUID.Multiplexer             = "{7A5DE1D3-01A1-452c-B481-4FA2B96271E8}"
Category_Encoders            = "WDM Streaming Encoder Devices"
Category_Multiplexers        = "WDM Streaming Multiplexer Devices"
Node.Encoder                 = "Encoder"
Node.Multiplexer             = "Multiplexer"
GUID.PINNAME_656_IN          = "{DFD530C7-36D9-47ff-B838-9A11D215B140}"
PinName.656_IN               = "656"
GUID.PINNAME_656_OUT         = "{E2EEB283-EB84-4910-BABE-037FFBB03249}"
PinName.656_OUT              = "656"
GUID.PINNAME_MPEG_OUT        = "{1649D2C1-435E-11d3-A94B-00A0C9D8B34E}"
PinName.MpegOut              = "MPEG"

GUID.IVAC_PROPERTIES         = "{87489F71-B890-4ba2-A88B-03E0B1A4EC1D}"
GUID.General_Properties      = "{F6E6FBD9-FE5D-419d-B994-57FB20AAED1D}"
GUID.Video_Properties        = "{5D64F5ED-1526-46f5-B510-AA93437FFA6E}"
GUID.Audio_Properties        = "{9D52CFF7-0DB7-4300-B936-844105E64E9E}"
GUID.MPEG_Properties         = "{A6ABB595-D3B7-4fdf-A418-F2C79E6E1C14}"
GUID.Diagnostic_Properties   = "{18759BBE-6A06-4118-9A57-E833AD670B81}"
GUID.Noise_Properties        = "{10E2DF32-3EC5-4551-BAE6-6D8F6B6C853A}"

MediaSets                    = "System\CurrentControlSet\Control\MediaSets"
ActiveMovieCategories        = "CLSID\{da4e3da0-d07d-11d0-bd50-00a0c911ce86}\Instance"

MediaInterfaces              = "System\CurrentControlSet\Control\MediaInterfaces"

