
;-----------------------------------------------------------------------
;	AVSim Driver Inf File
;	Version 3.0.1.15
;
;       Copyright (c) YUAN High Tech Development Co. Ltd. 
;       All Rights Reserved.
;------------------------------------------------------------------------


[Version]
signature=$Windows NT$
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%Company%
DriverVer=01/17/2007,3.0.1.18
DriverPackageType=PlugAndPlay
DriverPackageDisplayName=%PackageName%
CatalogFile.ntx86=AVSim.cat
CatalogFile.ntia64=AVSimia64.cat
CatalogFile.ntamd64=AVSimamd64.cat


[Manufacturer]
%Company%=YUAN,NTx86,NTamd64

[SourceDisksNames]
1=%DISK_NAME%,,,""

[SourceDisksFiles]
AVSim.sys=1,\x86

[SourceDisksFiles.ia64]
AVSim.sys=1,\ia64

[SourceDisksFiles.amd64]
AVSim.sys=1,\amd64

[ControlFlags]
ExcludeFromSelect =* 


[YUAN.NTia64]
;---------------------------------------
; PG655 Hybrid DVB-T/Global TV Tuner Cardbus , Analog TV/DVB-T using Zarlink mt352 demod with XCevie XC3028 tuner
;---------------------------------------
%AVSim.Audio%	=AVSim.Install,					PCI\VEN_14F1&DEV_8801&SUBSYS_178812AB
%AVSim.Audio881%=AVSim.Install,					PCI\VEN_14F1&DEV_8811&SUBSYS_178812AB
%AVSim.TS%		=AVSim.Install,					PCI\VEN_14F1&DEV_8802&SUBSYS_178812AB
;---------------------------------------
; CB122Analog TV Tuner Cardbus
;---------------------------------------
%AVSim.Audio%	=AVSim.Install,					PCI\VEN_14F1&DEV_8801&SUBSYS_112212AB
%AVSim.Audio881%=AVSim.Install,					PCI\VEN_14F1&DEV_8811&SUBSYS_112212AB
%AVSim.TS%		=AVSim.Install,					PCI\VEN_14F1&DEV_8802&SUBSYS_112212AB



[YUAN.NTamd64]
;---------------------------------------
; PG655 Hybrid DVB-T/Global TV Tuner Cardbus , Analog TV/DVB-T using Zarlink mt352 demod with XCevie XC3028 tuner
;---------------------------------------
%AVSim.Audio%	=AVSim.Install,					PCI\VEN_14F1&DEV_8801&SUBSYS_178812AB
%AVSim.Audio881%=AVSim.Install,					PCI\VEN_14F1&DEV_8811&SUBSYS_178812AB
%AVSim.TS%		=AVSim.Install,					PCI\VEN_14F1&DEV_8802&SUBSYS_178812AB
;---------------------------------------
; CB122Analog TV Tuner Cardbus
;---------------------------------------
%AVSim.Audio%	=AVSim.Install,					PCI\VEN_14F1&DEV_8801&SUBSYS_112212AB
%AVSim.Audio881%=AVSim.Install,					PCI\VEN_14F1&DEV_8811&SUBSYS_112212AB
%AVSim.TS%		=AVSim.Install,					PCI\VEN_14F1&DEV_8802&SUBSYS_112212AB


[YUAN.NTx86]
;---------------------------------------
; PG655 Hybrid DVB-T/Global TV Tuner Cardbus , Analog TV/DVB-T using Zarlink mt352 demod with XCevie XC3028 tuner
;---------------------------------------
%AVSim.Audio%	=AVSim.Install,					PCI\VEN_14F1&DEV_8801&SUBSYS_178812AB
%AVSim.Audio881%=AVSim.Install,					PCI\VEN_14F1&DEV_8811&SUBSYS_178812AB
%AVSim.TS%		=AVSim.Install,					PCI\VEN_14F1&DEV_8802&SUBSYS_178812AB
;---------------------------------------
; CB122Analog TV Tuner Cardbus
;---------------------------------------
%AVSim.Audio%	=AVSim.Install,					PCI\VEN_14F1&DEV_8801&SUBSYS_112212AB
%AVSim.Audio881%=AVSim.Install,					PCI\VEN_14F1&DEV_8811&SUBSYS_112212AB
%AVSim.TS%		=AVSim.Install,					PCI\VEN_14F1&DEV_8802&SUBSYS_112212AB



;;---------------------
;; Installation Section
;;---------------------
[AVSim.Install.NT]
CopyFiles=  AvSim.CopyDrivers

[DestinationDirs]
AvSim.CopyDrivers=12

[AvSim.CopyDrivers]
AVSim.sys



;
; Services installation
;

[AVSim.Install.NT.Services]
AddService = AVSim,2,VID.ServiceInstall

[VID.ServiceInstall]
DisplayName		= %SERVICE_DISPLAY_NAME%
Description		= %SERVICE_DESCRIPTION%
ServiceType		= %SERVICE_KERNEL_DRIVER%
StartType		= %SERVICE_DEMAND_START%
ErrorControl	= %SERVICE_ERROR_NORMAL%
ServiceBinary	= %12%\AVSim.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------
[Strings]
;---------------------------------------------------------------
;				S y s t e m   D e f i n e s
;---------------------------------------------------------------
SERVICE_BOOT_START				= 0x0
SERVICE_SYSTEM_START			= 0x1
SERVICE_AUTO_START				= 0x2
SERVICE_DEMAND_START			= 0x3
SERVICE_DISABLED				= 0x4

SERVICE_KERNEL_DRIVER			= 0x1

SERVICE_ERROR_IGNORE			= 0x0
SERVICE_ERROR_NORMAL			= 0x1
SERVICE_ERROR_SEVERE			= 0x2
SERVICE_ERROR_CRITICAL			= 0x3

SERVICE_DISPLAY_NAME			= "Cx2388x Multifunction Helper driver"
SERVICE_DESCRIPTION				= "Cx2388x Multifunction Helper driver"

;---------------------------------------------------------------
;             *L o c a l i z a b l e*
;---------------------------------------------------------------
;.....................
;  Installation 
;.....................
Company							= "YUAN High-Tech Development Co. Ltd."
DISK_NAME						= "Driver Setup Disk"
PackageName						= "Tuner Driver"

;.....................
;  Device Manager
;.....................

;........
;  Audio
AVSim.Audio						= "YUAN Audio AVStream Device"
;CX23881 audio catpure device (without BSTC)
AVSim.Audio881					= "YUAN Audio Capture Device"

;........
;  TS
AVSim.TS						= "YUAN TS Capture Device"



