; SCR3XX.INF
;
; Installation file (.inf) for the SCR3XX USB Smart Card Readers for Windows 2K/XP/Server2003/Vista/Windows7.
;
; Copyright © SCM Microsystems Inc.,2001-2010
;

[Version]
Signature="$Windows NT$"
Class=SmartCardReader
ClassGuid={50DD5230-BA8A-11D1-BF5D-0000F805F530}
Provider=%Mfg%
CatalogFile=SCR3XX.cat
DriverVer=01/07/2010,4.49

[Manufacturer]
%Mfg% = Models,NTamd64
[ClassInstall32]
AddReg=AddClassReg

[Models]
%PCSC_CCID%    = PCSC_CCID,USB\VID_04E6&PID_E001
%SCR333_CCID% = SCR333_CCID,USB\VID_04E6&PID_5113
%SCR335_CCID% = SCR335_CCID,USB\VID_04E6&PID_5115
%SCR33L_CCID% = SCR33L_CCID,USB\VID_04E6&PID_5116
%SCR3320_CCID% = SCR3320_CCID,USB\VID_04E6&PID_5117
%EXPSIM_CCID% = EXPSIM_CCID,USB\VID_04E6&PID_5118
%EXPCRD_CCID% = EXPCRD_CCID,USB\VID_04E6&PID_5119  
%SCR3311_CCID% = SCR3311_CCID,USB\VID_04E6&PID_511D
%SCR355_CCID%  = SCR355_CCID,USB\VID_04E6&PID_5410
%SCR338_CCID% = SCR338_CCID,USB\VID_04E6&PID_5151&MI_01

[Models.NTamd64]
%PCSC_CCID%   = PCSC_CCIDx64,USB\VID_04E6&PID_E001
%SCR333_CCID% = SCR333_CCIDx64,USB\VID_04E6&PID_5113
%SCR335_CCID% = SCR335_CCIDx64,USB\VID_04E6&PID_5115
%SCR33L_CCID% = SCR33L_CCIDx64,USB\VID_04E6&PID_5116
%SCR3320_CCID% = SCR3320_CCIDx64,USB\VID_04E6&PID_5117
%EXPSIM_CCID% = EXPSIM_CCIDx64,USB\VID_04E6&PID_5118
%EXPCRD_CCID% = EXPCRD_CCIDx64,USB\VID_04E6&PID_5119  
%SCR3311_CCID% = SCR3311_CCIDx64,USB\VID_04E6&PID_511D
%SCR355_CCID% = SCR355_CCIDx64,USB\VID_04E6&PID_5410
%SCR338_CCID% = SCR338_CCIDx64,USB\VID_04E6&PID_5151&MI_01

[ControlFlags]
ExcludeFromSelect.NT=USB\VID_04E6&PID_E001
ExcludeFromSelect.NT=USB\VID_04E6&PID_5113
ExcludeFromSelect.NT=USB\VID_04E6&PID_5115
ExcludeFromSelect.NT=USB\VID_04E6&PID_5116
ExcludeFromSelect.NT=USB\VID_04E6&PID_5117
ExcludeFromSelect.NT=USB\VID_04E6&PID_5118
ExcludeFromSelect.NT=USB\VID_04E6&PID_5119
ExcludeFromSelect.NT=USB\VID_04E6&PID_511D
ExcludeFromSelect.NT=USB\VID_04E6&PID_5410
ExcludeFromSelect.NT=USB\VID_04E6&PID_5151&MI_01

[SourceDisksNames]
1=%Floppy_Description%,SCR3XX2K.sys,,
1=%Floppy_Description%,S3XXx64.sys,,

[SourceDisksFiles]
SCR3XX2K.sys=1
S3XXx64.sys=1

[DestinationDirs]
DefaultDestDir=10,system32\drivers
PCSC_CCID.NTCopyFiles=10,system32\drivers
PCSC_CCIDx64.NTCopyFiles=10,system32\drivers

[AddClassReg]
HKR,,,0,%ClassName%
HKR,,NoInstallClass,,1
HKR,,Installer32,,"winscard.dll,ClassInstall32"
;*******************************************************************************************************
; x86 specific 
;*******************************************************************************************************

[PCSC_CCID.NTCopyFiles]
SCR3XX2K.sys,,

[PCSC_CCID.AddReg]
HKR,,ShortProviderName,0,%ShortProviderName%
HKR,,ReaderName,0,%PCSC_CCID%
HKLM, Software\Microsoft\Cryptography\Calais\Readers,,,
HKLM, System\CurrentControlSet\Services\SCardSvr,Start,0x00010001,2
HKLM, System\CurrentControlSet\Services\CertPropSvc,Start,0x00010001,2
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,DLLName,0,wlnotify.dll
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Logon,0,SCardStartCertProp
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Logoff,0,SCardStopCertProp
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Lock,0,SCardSuspendCertProp
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Unlock,0,SCardResumeCertProp
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Enabled,0x00010001,1
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Impersonate,0x00010001,1
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Asynchronous,0x00010001,1

[PCSC_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[PCSC_CCID.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[PCSC_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, PCSC_CCID.NT.AddReg

[PCSC_CCID.NT.HW]
AddReg= PCSC_CCID.AddReg.HW

[PCSC_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst

[PCSC_CCID_Service_Inst]
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_AUTO_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\SCR3XX2K.sys
DisplayName     = %SERVICE_CCID%
AddReg= PCSC_CCID.AddReg

[PCSC_CCID_EventLog_Inst]
AddReg=PCSC_CCID.AddEventLogReg

[PCSC_CCID.AddEventLogReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\SCR3XX2K.sys"
HKR,,CategoryMessageFile,0x00020000,"%%SystemRoot%%\System32\drivers\SCR3XX2K.sys"
HKR,,CategoryCount,0x00010001,1
HKR,,TypesSupported,0x00010001,7

;;========For SCR335=========
[SCR335_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[SCR335_CCID.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR335_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, SCR335_CCID.NT.AddReg

[SCR335_CCID.NT.HW]
AddReg= SCR335_CCID.AddReg.HW

[SCR335_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst
;;===========================

;;========For SCR333=========
[SCR333_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[SCR333_CCID.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR333_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, SCR333_CCID.NT.AddReg

[SCR333_CCID.NT.HW]
AddReg= SCR333_CCID.AddReg.HW

[SCR333_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst
;;===========================

;;========For SCR33L=========
[SCR33L_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[SCR33L_CCID.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR33L_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, SCR33L_CCID.NT.AddReg

[SCR33L_CCID.NT.HW]
AddReg= SCR33L_CCID.AddReg.HW

[SCR33L_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst
;;===========================


;;========For 3320=============
[SCR3320_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%SCR3320_CCID%
HKR,, VendorName,0,%Mfg%
HKR,, ServerReq , 0x00010001, 0

[SCR3320_CCID.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR3320_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, SCR3320_CCID.NT.AddReg

[SCR3320_CCID.NT.HW]
AddReg= SCR3320_CCID.AddReg.HW

[SCR3320_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst

;;===========================

;;========For EXPSIM=========
[EXPSIM_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[EXPSIM_CCID.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[EXPSIM_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, EXPSIM_CCID.NT.AddReg

[EXPSIM_CCID.NT.HW]
AddReg= EXPSIM_CCID.AddReg.HW

[EXPSIM_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst
;;===========================

;;========For EXPCRD=========
[EXPCRD_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%EXP_CCID%
HKR,, VendorName,0,%Mfg%
HKR,, InstanceFlags,0x00010001,0x01

[EXPCRD_CCID.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 0
HKR,, IdleTime , 0x00010001, 5

[EXPCRD_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, EXPCRD_CCID.NT.AddReg

[EXPCRD_CCID.NT.HW]
AddReg= EXPCRD_CCID.AddReg.HW

[EXPCRD_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst
;;===========================

;;========For SCR3311=========
[SCR3311_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[SCR3311_CCID.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR3311_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, SCR3311_CCID.NT.AddReg

[SCR3311_CCID.NT.HW]
AddReg= SCR3311_CCID.AddReg.HW

[SCR3311_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst

;;========For SCR355=========
[SCR355_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%SCR355_CCID%
HKR,, VendorName,0,%Mfg%

[SCR355_CCID.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR355_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, SCR355_CCID.NT.AddReg

[SCR355_CCID.NT.HW]
AddReg= SCR355_CCID.AddReg.HW

[SCR355_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst
;;===========================
;;========For SCR338=========
[SCR338_CCID.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%SCR338_CCID%
HKR,, VendorName,0,%Mfg%

[SCR338_CCID.AddReg.HW]
HKR,, WaitWakeEnabled , 0x00010001, 1

[SCR338_CCID.NT]
CopyFiles= PCSC_CCID.NTCopyFiles
AddReg= PCSC_CCID.AddReg, SCR338_CCID.NT.AddReg

[SCR338_CCID.NT.HW]
AddReg= SCR338_CCID.AddReg.HW

[SCR338_CCID.NT.Services]
AddService = SCR3XX2K,0x00000002,PCSC_CCID_Service_Inst,PCSC_CCID_EventLog_Inst
;;===========================
;*************************************************************************************************************************
; x64 specific section
;*************************************************************************************************************************

[PCSC_CCIDx64.NTCopyFiles]
S3XXx64.sys,,

[PCSC_CCIDx64.AddReg]
HKR,,ShortProviderName,0,%ShortProviderName%
HKR,,ReaderName,0,%PCSC_CCID%
HKLM, Software\Microsoft\Cryptography\Calais\Readers,,,
HKLM, System\CurrentControlSet\Services\SCardSvr,Start,0x00010001,2
HKLM, System\CurrentControlSet\Services\CertPropSvc,Start,0x00010001,2
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,DLLName,0,wlnotify.dll
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Logon,0,SCardStartCertProp
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Logoff,0,SCardStopCertProp
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Lock,0,SCardSuspendCertProp
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Unlock,0,SCardResumeCertProp
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Enabled,0x00010001,1
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Impersonate,0x00010001,1
HKLM, SOFTWARE\Microsoft\Windows NT\CurrentVersion\Winlogon\Notify\ScCertProp,Asynchronous,0x00010001,1

[PCSC_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[PCSC_CCIDx64.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[PCSC_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, PCSC_CCIDx64.NT.AddReg

[PCSC_CCIDx64.NT.HW]
AddReg= PCSC_CCIDx64.AddReg.HW

[PCSC_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst

[PCSC_CCIDx64_Service_Inst]
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_AUTO_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\S3XXx64.sys
DisplayName     = %SERVICE_CCID64%
AddReg= PCSC_CCIDx64.AddReg

[PCSC_CCIDx64_EventLog_Inst]
AddReg=PCSC_CCIDx64.AddEventLogReg

[PCSC_CCIDx64.AddEventLogReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\S3XXx64.sys"
HKR,,CategoryMessageFile,0x00020000,"%%SystemRoot%%\System32\drivers\S3XXx64.sys"
HKR,,CategoryCount,0x00010001,1
HKR,,TypesSupported,0x00010001,7

;;========For SCR335=========
[SCR335_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[SCR335_CCIDx64.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR335_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, SCR335_CCIDx64.NT.AddReg

[SCR335_CCIDx64.NT.HW]
AddReg= SCR335_CCIDx64.AddReg.HW

[SCR335_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst
;;===========================

;;========For SCR333=========
[SCR333_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[SCR333_CCIDx64.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR333_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, SCR333_CCIDx64.NT.AddReg

[SCR333_CCIDx64.NT.HW]
AddReg= SCR333_CCIDx64.AddReg.HW

[SCR333_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst
;;===========================

;;========For SCR33L=========
[SCR33L_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[SCR33L_CCIDx64.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR33L_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, SCR33L_CCIDx64.NT.AddReg

[SCR33L_CCIDx64.NT.HW]
AddReg= SCR33L_CCIDx64.AddReg.HW

[SCR33L_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst
;;===========================

;========For SCR3320=========
[SCR3320_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%SCR3320_CCID%
HKR,, VendorName,0,%Mfg%
HKR,, ServerReq , 0x00010001, 0

[SCR3320_CCIDx64.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR3320_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, SCR3320_CCIDx64.NT.AddReg

[SCR3320_CCIDx64.NT.HW]
AddReg= SCR3320_CCIDx64.AddReg.HW

[SCR3320_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst

;;========For EXPSIM=========
[EXPSIM_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[EXPSIM_CCIDx64.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[EXPSIM_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, EXPSIM_CCIDx64.NT.AddReg

[EXPSIM_CCIDx64.NT.HW]
AddReg= EXPSIM_CCIDx64.AddReg.HW

[EXPSIM_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst

;;===========================

;;========For EXPCRD=========
[EXPCRD_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%EXP_CCID%
HKR,, VendorName,0,%Mfg%
HKR,, InstanceFlags,0x00010001,0x01

[EXPCRD_CCIDx64.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 0
HKR,, IdleTime , 0x00010001, 5

[EXPCRD_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, EXPCRD_CCIDx64.NT.AddReg

[EXPCRD_CCIDx64.NT.HW]
AddReg= EXPCRD_CCIDx64.AddReg.HW

[EXPCRD_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst
;;===========================

;;========For SCR3311=========
[SCR3311_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%PCSC_CCID%
HKR,, VendorName,0,%Mfg%

[SCR3311_CCIDx64.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR3311_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, SCR3311_CCIDx64.NT.AddReg

[SCR3311_CCIDx64.NT.HW]
AddReg= SCR3311_CCIDx64.AddReg.HW

[SCR3311_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst

;;========For SCR355=========
[SCR355_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%SCR355_CCID%
HKR,, VendorName,0,%Mfg%

[SCR355_CCIDx64.AddReg.HW]
HKR,, SelectiveSuspend , 0x00010001, 0
HKR,, WaitWakeEnabled , 0x00010001, 1
HKR,, IdleTime , 0x00010001, 5

[SCR355_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, SCR355_CCIDx64.NT.AddReg

[SCR355_CCIDx64.NT.HW]
AddReg= SCR355_CCIDx64.AddReg.HW

[SCR355_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst

;;========For SCR338=========
[SCR338_CCIDx64.NT.AddReg]
; Configurable F and D values
;HKR,, FValue , 0x00010001, 1
;HKR,, DValue , 0x00010001, 1
HKR,, BufferSize , 0x00010001, 131072
;HKR,, CardSpecificATR, 1, 3B,34,D6,00,30,42,30,30
;HKR,, TranslatedATR, 1, 3B,34,B5,00,30,42,30,30
HKR,, IFDType,0,%SCR338_CCID%
HKR,, VendorName,0,%Mfg%

[SCR338_CCIDx64.AddReg.HW]
HKR,, WaitWakeEnabled , 0x00010001, 1

[SCR338_CCIDx64.NT]
CopyFiles= PCSC_CCIDx64.NTCopyFiles
AddReg= PCSC_CCIDx64.AddReg, SCR338_CCIDx64.NT.AddReg

[SCR338_CCIDx64.NT.HW]
AddReg= SCR338_CCIDx64.AddReg.HW

[SCR338_CCIDx64.NT.Services]
AddService = S3XXx64,0x00000002,PCSC_CCIDx64_Service_Inst,PCSC_CCIDx64_EventLog_Inst
;;===========================


[Strings]
Mfg = "SCM Microsystems Inc."
ShortProviderName = "SCM"
Description = "Server for SmartCard Reader"
Floppy_Description = "Installation Disk"
PCSC_CCID="SCR33x USB Smart Card Reader"
SCR333_CCID="SCR333 Internal Smart Card Reader"
SCR335_CCID="SCR335 USB Smart Card Reader"
SCR33L_CCID="SCR3310 USB Smart Card Reader"
SCR3320_CCID="SCR3320 USB Smart Card Reader"
EXPSIM_CCID="Expresscard USB SIM Card Reader"
EXPCRD_CCID="SCR3340 - ExpressCard54 Smart Card Reader"
EXP_CCID="SCR3340 ExpressCard Reader"
SCR3311_CCID="SCR3311 USB Smart Card Reader"
SCR355_CCID="SCR35xx USB Smart Card Reader"
SCR338_CCID="SCR338 USB Keyboard Smart Card Reader"
SERVICE_CCID="SCR3xx USB SmartCardReader"
SERVICE_CCID64="SCR3xx USB SmartCardReader64"
ClassName="Smart Card Readers"