; Copyright 2007 NXP Semiconductors

[Version]
signature           = "$CHICAGO$" ;all windows os
Class               = MEDIA
ClassGUID           = {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider            = %AVer%
DriverVer           =07/07/2009,1.3.0.77
CatalogFile	    = AVerBDA6x.cat


[Manufacturer]
%AVer% = AVerMedia,NT.6

;---> 32 BIT SUPPORT <---
[AVerMedia]
;%60Hybrid.DeviceDesc% = PAverCap,PCI\VEN_1131&DEV_7160
;%61Hybrid.DeviceDesc% = PAverCap,PCI\VEN_1131&DEV_7161
;%62Hybrid.DeviceDesc% = PAverCap,PCI\VEN_1131&DEV_7162
;%63Hybrid.DeviceDesc% = PAverCap,PCI\VEN_1131&DEV_7163

;******** AVerMedia A177 ***
%AVer.DeviceDesc22% = AVer_A177_RC.NTx86 , PCI\VEN_1131&DEV_7162&SUBSYS_011C1461 ; A177

;******** AVerMedia A568 ***

;******** AVerMedia M789 ***
%AVer.DeviceDesc00% = AVer_M789.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_01511461 ; M789 (I)
%AVer.DeviceDesc01% = AVer_M789.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_02511461 ; M789 (II)

;******** AVerMedia M788 ***
%AVer.DeviceDesc02% = AVer_M788.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_01551461 ; M788 (I)

;******** AVerMedia H788 HyBrid DVBT ***
%AVer.DeviceDesc08% = AVer_H788_HyDVBT_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_0B551461 ; H788 HyBrid DVBT (I)

;******** AVerMedia H788 Pure DVBT***
%AVer.DeviceDesc09% = AVer_H788_PuDVBT_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_0C551461 ; H788 Pure DVBT (I)

;******** AVerMedia H788 Hybrid ATSC***
%AVer.DeviceDesc10% = AVer_H788_HyATSC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_06551461 ; H788 Hybrid ATSC (I)

;******** AVerMedia H788 Pure ATSC***
%AVer.DeviceDesc11% = AVer_H788_PuATSC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_07551461 ; H788 Pure ATSC (I)

;******** AVerMedia H788 Hybrid ATSC IR***
%AVer.DeviceDesc10% = AVer_H788_HyATSC_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_1A551461 ; H788 Hybrid ATSC with RC(I)

;******** AVerMedia H788 Pure ATSC IR***
%AVer.DeviceDesc11% = AVer_H788_PuATSC_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_1B551461 ; H788 Pure ATSC with RC(I)

;******** AVerMedia H788 Pure Analog***
%AVer.DeviceDesc12% = AVer_H788_Analog_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_08551461 ; H788 Pure Analog (I)

;******** AVerMedia H788 Hybrid ATSC 2 AV-in***
%AVer.DeviceDesc10% = AVer_H788_HyATSC_II.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_11551461 ; H788 Hybrid ATSC 2 AV-in (I)

;******** AVerMedia H788 HyBrid DVBT II***
%AVer.DeviceDesc08% = AVer_H788_HyDVBT_II_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_14551461 ; H788 HyBrid DVBT (II)

;******** AVerMedia H788 Pure DVBT II***
%AVer.DeviceDesc09% = AVer_H788_PuDVBT_II_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_15551461 ; H788 Pure DVBT (II)

;******** AVerMedia H788 Pure Analog II***
%AVer.DeviceDesc12% = AVer_H788_Analog_II_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_16551461 ; H788 Pure Analog (II)

;******** AVerMedia A701 ***
%AVer.DeviceDesc04% = AVer_A701.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_03551461 ; A701 (I)

;******** AVerMedia HC83_ATSC***                                                                    
%AVer.DeviceDesc25% = AVer_HC83_ATSC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_28551461 ; HC83_ATSC (I)  
                                                                                                    
;******** AVerMedia HC83_DVBT***                                                                    
%AVer.DeviceDesc26% = AVer_HC83_DVBT.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_29551461 ; HC83_DVBT (I)  

;******** AVerMedia M799 ***
%AVer.DeviceDesc13% = AVer_M799_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_09551461 ; M799

;******** AVerMedia A188 ***
%AVer.DeviceDesc17% = AVer_A188_RC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_18551461 ; A188 (DUAL HYBRID DVB_T)
%AVer.DeviceDesc18% = AVer_A188_ATSC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_19551461 ; A188C (DUAL HYBRID ATSC)
%AVer.DeviceDesc19% = AVer_A188_RC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_1C551461 ; A188 (PURE ANALOG)
%AVer.DeviceDesc20% = AVer_A188_RC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_1D551461 ; A188 (PURE DVB_T)
%AVer.DeviceDesc21% = AVer_A188_ATSC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_1E551461 ; A188C (PURE ATSC)
%AVer.DeviceDesc18% = AVer_A188_ATSC_RC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_24551461 ; A188C (DUAL HYBRID ATSC)
%AVer.DeviceDesc21% = AVer_A188_ATSC_RC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_25551461 ; A188C (PURE ATSC)
%AVer.DeviceDesc24% = AVer_A188.NTx86, 		PCI\VEN_1131&DEV_7160&SUBSYS_27551461 ; A188O (DUAL HYBRID DVB_T)
%AVer.DeviceDesc21% = AVer_A188_ATSC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_30551461 ; A188C (PURE ATSC)(USA Retail Box)

;******** AVerMedia A707 ***
%AVer.DeviceDesc23% = AVer_A707_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_26551461 ; A707

;******** AVerMedia A707 Pure DVBT CI/CA ***
%AVer.DeviceDesc29% = AVer_A707_DVBT.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_2E551461 ; A707_PURE_DVBT_CICA

;******** AVerMedia A750 ***
%AVer.DeviceDesc28% = AVer_A750.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_03511461 ; A750

[AVerMedia.NT.6]
;******** AVerMedia A177 ***
%AVer.DeviceDesc22% = AVer_A177_vistaRC.NTx86 , PCI\VEN_1131&DEV_7162&SUBSYS_011C1461 ; A177

;******** AVerMedia A568 ***

;******** AVerMedia M789 ***
%AVer.DeviceDesc00% = AVer_M789.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_01511461 ; M789 (I)
%AVer.DeviceDesc01% = AVer_M789.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_02511461 ; M789 (II)

;******** AVerMedia M788 ***
%AVer.DeviceDesc02% = AVer_M788.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_01551461 ; M788 (I)

;******** AVerMedia H788 HyBrid DVBT ***
%AVer.DeviceDesc08% = AVer_H788_HyDVBT_vistaRC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_0B551461 ; H788 HyBrid DVBT (I)

;******** AVerMedia H788 Pure DVBT***
%AVer.DeviceDesc09% = AVer_H788_PuDVBT_vistaRC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_0C551461 ; H788 Pure DVBT (I)

;******** AVerMedia H788 Hybrid ATSC***
%AVer.DeviceDesc10% = AVer_H788_HyATSC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_06551461 ; H788 Hybrid ATSC (I)

;******** AVerMedia H788 Pure ATSC***
%AVer.DeviceDesc11% = AVer_H788_PuATSC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_07551461 ; H788 Pure ATSC (I)

;******** AVerMedia H788 Hybrid ATSC IR***
%AVer.DeviceDesc10% = AVer_H788_HyATSC_vistaRC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_1A551461 ; H788 Hybrid ATSC with RC(I)

;******** AVerMedia H788 Pure ATSC IR***
%AVer.DeviceDesc11% = AVer_H788_PuATSC_vistaRC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_1B551461 ; H788 Pure ATSC with RC(I)

;******** AVerMedia H788 Pure Analog***
%AVer.DeviceDesc12% = AVer_H788_Analog_vistaRC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_08551461 ; H788 Pure Analog (I)

;******** AVerMedia H788 Hybrid ATSC 2 AV-in***
%AVer.DeviceDesc10% = AVer_H788_HyATSC_II.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_11551461 ; H788 Hybrid ATSC 2 AV-in (I)

;******** AVerMedia H788 HyBrid DVBT II***
%AVer.DeviceDesc08% = AVer_H788_HyDVBT_II_vistaRC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_14551461 ; H788 HyBrid DVBT (II)

;******** AVerMedia H788 Pure DVBT II***
%AVer.DeviceDesc09% = AVer_H788_PuDVBT_II_vistaRC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_15551461 ; H788 Pure DVBT (II)

;******** AVerMedia H788 Pure Analog II***
%AVer.DeviceDesc12% = AVer_H788_Analog_II_vistaRC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_16551461 ; H788 Pure Analog (II)

;******** AVerMedia A701 ***
%AVer.DeviceDesc04% = AVer_A701.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_03551461 ; A701 (I)

;******** AVerMedia HC83_ATSC***                                                                    
%AVer.DeviceDesc25% = AVer_HC83_ATSC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_28551461 ; HC83_ATSC (I)  
                                                                                                    
;******** AVerMedia HC83_DVBT***                                                                    
%AVer.DeviceDesc26% = AVer_HC83_DVBT.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_29551461 ; HC83_DVBT (I)  

;******** AVerMedia M799 ***
%AVer.DeviceDesc13% = AVer_M799_RC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_09551461 ; M799

;******** AVerMedia A188 ***
%AVer.DeviceDesc17% = AVer_A188_VistaRC.NTx86, 		PCI\VEN_1131&DEV_7160&SUBSYS_18551461 ; A188 (DUAL HYBRID DVB_T)
%AVer.DeviceDesc18% = AVer_A188_ATSC_Vista.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_19551461 ; A188C (DUAL HYBRID ATSC)
%AVer.DeviceDesc19% = AVer_A188_VistaRC.NTx86, 		PCI\VEN_1131&DEV_7160&SUBSYS_1C551461 ; A188 (PURE ANALOG)
%AVer.DeviceDesc20% = AVer_A188_VistaRC.NTx86, 		PCI\VEN_1131&DEV_7160&SUBSYS_1D551461 ; A188 (PURE DVB_T)
%AVer.DeviceDesc21% = AVer_A188_ATSC_Vista.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_1E551461 ; A188C (PURE ATSC)

%AVer.DeviceDesc18% = AVer_A188_ATSC_VistaRC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_24551461 ; A188C (DUAL HYBRID ATSC)
%AVer.DeviceDesc21% = AVer_A188_ATSC_VistaRC.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_25551461 ; A188C (PURE ATSC)
%AVer.DeviceDesc24% = AVer_A188_Vista.NTx86, 		PCI\VEN_1131&DEV_7160&SUBSYS_27551461 ; A188O (DUAL HYBRID DVB_T)
%AVer.DeviceDesc21% = AVer_A188_ATSC_Vista.NTx86, 	PCI\VEN_1131&DEV_7160&SUBSYS_30551461 ; A188C (PURE ATSC)(USA Retail Box)

;******** AVerMedia A707 ***
%AVer.DeviceDesc23% = AVer_A707_VistaRC.NTx86   , PCI\VEN_1131&DEV_7160&SUBSYS_26551461 ; A707

;******** AVerMedia A707 Pure DVBT CI/CA ***
%AVer.DeviceDesc29% = AVer_A707_DVBT.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_2E551461 ; A707_PURE_DVBT_CICA

;******** AVerMedia A750 ***
%AVer.DeviceDesc28% = AVer_A750_VistaRC.NTx86 , PCI\VEN_1131&DEV_7160&SUBSYS_03511461 ; A750

[SourceDisksNames]
1 = %AVSTRM_INSTALLATION_DISK%,,

[SourceDisksFiles]
716xCoInstaller.dll  = 1
;NXPMV32.dll         = 1
AVerBDA716x.sys      = 1
MV716x.ax            = 1
CoSetup.ax           = 1

[DestinationDirs]
PAverCap.CopyCoInst.NTx86   = 11
PAverCap.CopyDll.NTx86      = 11
PAverCap.CopyFiles.NTx86    = 10,system32\drivers


[PAverCap.CopyCoInst.NTx86]
716xCoInstaller.dll

[PAverCap.CopyFiles.NTx86]
AVerBDA716x.sys

[PAverCap.CopyDll.NTx86]
;NXPMV32.dll
MV716x.ax


;======================================
;
;       Initialization Entries
;
;======================================

;******** AVerMedia M789 ***
[AVer_M789.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_M789.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_M789.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_M789.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia M788 ***
[AVer_M788.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_M788.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_M788.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_M788.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 HyBrid DVBT_RC ***
[AVer_H788_HyDVBT_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_HyDVBT_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_HyDVBT_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_HyDVBT_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 HyBrid DVBT_vista_RC***
[AVer_H788_HyDVBT_vistaRC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_HyDVBT_vistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_HyDVBT_vistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_HyDVBT_vistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Pure DVBT_RC ***
[AVer_H788_PuDVBT_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_PuDVBT_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_PuDVBT_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_PuDVBT_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Pure DVBT_vista_RC ***
[AVer_H788_PuDVBT_vistaRC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_PuDVBT_vistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_PuDVBT_vistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_PuDVBT_vistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86


;******** AVerMedia H788 Hybrid ATSC ***
[AVer_H788_HyATSC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_HyATSC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_HyATSC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_HyATSC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Hybrid ATSC_RC ***
[AVer_H788_HyATSC_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_HyATSC_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_HyATSC_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_HyATSC_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Hybrid ATSC_vistaRC ***
[AVer_H788_HyATSC_vistaRC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_HyATSC_vistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_HyATSC_vistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_HyATSC_vistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Hybrid ATSC 2 AV-in***
[AVer_H788_HyATSC_II.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_HyATSC_II.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_HyATSC_II.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_HyATSC_II.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Pure ATSC ***
[AVer_H788_PuATSC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_PuATSC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_PuATSC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_PuATSC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Pure ATSC_RC ***
[AVer_H788_PuATSC_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_PuATSC_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_PuATSC_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_PuATSC_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Pure ATSC_vistaRC ***
[AVer_H788_PuATSC_vistaRC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_PuATSC_vistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_PuATSC_vistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_PuATSC_vistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86


;******** AVerMedia H788 Pure Analog_RC ***
[AVer_H788_Analog_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_Analog_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_Analog_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_Analog_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86


;******** AVerMedia H788 Pure Analog_vistaRC ***
[AVer_H788_Analog_vistaRC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_Analog_vistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_Analog_vistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_Analog_vistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86


;******** AVerMedia H788 HyBrid DVBT II_RC ***
[AVer_H788_HyDVBT_II_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_HyDVBT_II_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_HyDVBT_II_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_HyDVBT_II_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 HyBrid DVBT II_vistaRC ***
[AVer_H788_HyDVBT_II_vistaRC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_HyDVBT_II_vistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_HyDVBT_II_vistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_HyDVBT_II_vistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Pure DVBT II_RC ***
[AVer_H788_PuDVBT_II_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_PuDVBT_II_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_PuDVBT_II_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_PuDVBT_II_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Pure DVBT II_vistaRC ***
[AVer_H788_PuDVBT_II_vistaRC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_PuDVBT_II_vistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_PuDVBT_II_vistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_PuDVBT_II_vistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86


;******** AVerMedia H788 Pure Analog II_RC ***
[AVer_H788_Analog_II_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_Analog_II_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_Analog_II_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_Analog_II_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia H788 Pure Analog II_vistaRC ***
[AVer_H788_Analog_II_vistaRC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_H788_Analog_II_vistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_H788_Analog_II_vistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_H788_Analog_II_vistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A701 ***
[AVer_A701.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A701.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A701.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A701.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia HC83_ATSC***
[AVer_HC83_ATSC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_HC83_ATSC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_HC83_ATSC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_HC83_ATSC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia HC83_DVBT***
[AVer_HC83_DVBT.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_HC83_DVBT.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_HC83_DVBT.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_HC83_DVBT.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia M799_RC ***
[AVer_M799_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_M799_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_M799_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_M799_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A188 ***
[AVer_A188.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A188.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A188.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A188.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A188_RC ***
[AVer_A188_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A188_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A188_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A188_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A188_ATSC ***  
[AVer_A188_ATSC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A188_ATSC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A188_ATSC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A188_ATSC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A188_ATSC_RC *** 
[AVer_A188_ATSC_RC.ntx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A188_ATSC_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A188_ATSC_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A188_ATSC_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A188_Vista ***
[AVer_A188_Vista.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A188_Vista.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A188_Vista.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A188_Vista.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A188_VistaRC ***
[AVer_A188_VistaRC.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A188_VistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A188_VistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A188_VistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A188_ATSC_Vista *** 
[AVer_A188_ATSC_Vista.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A188_ATSC_Vista.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A188_ATSC_Vista.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A188_ATSC_Vista.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A188_ATSC_VistaRC *** 
[AVer_A188_ATSC_VistaRC.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A188_ATSC_VistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A188_ATSC_VistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A188_ATSC_VistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86


;******** AVerMedia A177_RC ***
[AVer_A177_RC.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A177_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A177_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A177_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A177_vistaRC ***
[AVer_A177_vistaRC.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A177_vistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A177_vistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A177_vistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86


;******** AVerMedia A707_RC ***
[AVer_A707_RC.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A707_RC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A707_RC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A707_RC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A707_DVBT ***
[AVer_A707_DVBT.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A707_DVBT.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A707_DVBT.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A707_DVBT.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A707_VistaRC ***
[AVer_A707_VistaRC.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A707_VistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A707_VistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A707_VistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A750 ***
[AVer_A750.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A750.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A750.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A750.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;******** AVerMedia A750_VistaRc ***
[AVer_A750_VistaRC.NTx86.CoInstallers]
CopyFiles = PAverCap.CopyCoInst.NTx86
AddReg    = PAverCap.CoInstaller_AddReg.NTx86

[AVer_A750_VistaRC.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = PAverCap.CopyFiles.NTx86, PAverCap.CopyDll.NTx86
AddReg        = PAverCap.AddReg.NTx86, AVer_A750_VistaRC.AddReg
RegisterDlls  = PAverCap.Register.NTx86

[AVer_A750_VistaRC.NTx86.Services]
AddService = %SERVICE_NAME_X32%, 0x00000002, PAverCap.ServiceInstall.NTx86, PAverCap.EventInstall.NTx86

;---------------------------------------------------------------
[PAverCap.ServiceInstall.NTx86]
DisplayName   = %DISPLAY_NAME%
Description   = %SERVICE_DESCRIPTION%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_IGNORE%
ServiceBinary = %12%\AVerBDA716x.sys

[PAverCap.EventInstall.NTx86]
AddReg = PAverCapEvent_AddReg.NTx86

;======================================
;
;           Registry Entries
;
;======================================
; [StartName=driver-object-name]
; [AddReg=add-registry-section[, add-registry-section] ...]
; [DelReg=del-registry-section[, del-registry-section] ...]
; [BitReg=bit-registry-section[, bit-registry-section] ...]
; [LoadOrderGroup=load-order-group-name]
; [Dependencies=depend-on-item-name[, depend-on-item-name]...]
;
;******** General DLL Registry Entries ***
;

[PAverCap.CoInstaller_AddReg.NTx86]
HKR,,CoInstallers32,0x00010000,"716xCoInstaller.dll, CoInstallerEntry"

[PAverCap.Register.NTx86]
;11,,NXPMV32.dll,1 ;FLG_REGSVR_DLLREGISTER
11,,MV716x.ax,1

[PAverCapEvent_AddReg.NTx86]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\AVerBDA716x.sys"
HKR,,TypesSupported,0x00010001,7

;
;******** General Driver Registry Entries ***
;
[PAverCap.AddReg.NTx86]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,AVerBDA716x.sys

; Audio capture registry entries
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,AVerBDA716x.sys


; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_PIN%,"Name",,"~Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_PIN%,"Name",,"~Capture"
HKLM,%MediaInterfaces%\{6a2e0650-28e4-11d0-A18c-00A0C9118959},,,"Copy Protect Notification Filter"
HKLM,%MediaInterfaces%\{6a2e0650-28e4-11d0-A18c-00A0C9118959},IID,1,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00
HKLM,%MediaInterfaces%\{1704290E-658E-4818-BBE3-A18A8E4ECD2B},,,"CState Control Filter"
HKLM,%MediaInterfaces%\{1704290E-658E-4818-BBE3-A18A8E4ECD2B},IID,1,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

HKR, "Parameters", Prefix,,"AVerMedia 716x BDA"

HKR, "AudioDecoder\Path0", "DefaultDecoderLevel",0x00010001,0x00
HKR, "AudioDecoder\Path0", "DefaultMonoLevel",0x00010001,0x07
HKR, "AudioDecoder\Path0", "DefaultSAPLevel",0x00010001,0x07

HKR, "VideoDecoder\Path0", "AutoBlank",0x00010001,0

HKR, "AudioDecoder\Path0", "VolumeTuner",0x00010001,0x04
HKR, "AudioDecoder\Path0", "VolumeExt1",0x00010001,0

HKR, "AudioDecoder", "EnableAudioStdDetectionEx",0x00010001,1

;HKR, "AnlgVideoCap", "EarlyCheckWindow", 0x00010001, 30	; Bob_0010 20071207
;HKR, "AnlgVideoCap", "EarlyMuteNumber", 0x00010001, 5		; Bob_0010 20071207
;HKR, "AnlgVideoCap", "VideoFillData", 0x00010001, 0x80808080	; Bob_0010 20071207
;HKR, "AnlgVideoCap", "ForceMute", 0x00010001, 0		; Bob_0010 20071207

HKR, "Parameters", "Debug AFT thread", 0x00010001, 0		; Bob_0013 20071218
HKR, "Parameters", "Force C1 code", 0x00010001, 0		; Bob_0014 20071220

HKR, "VideoDecoder\Tuner\Path0", "DefaultBrightness",0x00010001,126
HKR, "VideoDecoder\Tuner\Path0", "DefaultContrast",0x00010001,67
HKR, "VideoDecoder\Tuner\Path0", "DefaultHue",0x00010001,129
HKR, "VideoDecoder\Tuner\Path0", "DefaultSaturation",0x00010001,63
HKR, "VideoDecoder\Tuner\Path0", "DefaultSharpness",0x00010001,8

HKR, "VideoDecoder\Tuner\Path1", "DefaultBrightness",0x00010001,126
HKR, "VideoDecoder\Tuner\Path1", "DefaultContrast",0x00010001,67
HKR, "VideoDecoder\Tuner\Path1", "DefaultHue",0x00010001,129
HKR, "VideoDecoder\Tuner\Path1", "DefaultSaturation",0x00010001,63
HKR, "VideoDecoder\Tuner\Path1", "DefaultSharpness",0x00010001,8

HKR, "Parameters", "QAMNode",0x00010001,0x01

;
;******** Board - Specific Registry Entries ***
;

;******** AVerMedia M789 ***
[AVer_M789.AddReg]


;******** AVerMedia M788 ***
[AVer_M788.AddReg]

;******** AVerMedia H788 HyBrid DVBT_RC ***
[AVer_H788_HyDVBT_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 HyBrid DVBT_vistaRC ***
[AVer_H788_HyDVBT_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR, "ENUM\CIR",pnpid,,"AVerIR"


;******** AVerMedia H788 Pure DVBT_RC***
[AVer_H788_PuDVBT_RC.AddReg]
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 0

;******** AVerMedia H788 Pure DVBT_vistaRC***
[AVer_H788_PuDVBT_vistaRC.AddReg]
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "IRSource", 0x00010001, 1

HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 0

;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia H788 Hybrid ATSC***
[AVer_H788_HyATSC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Hybrid ATSC_RC***
[AVer_H788_HyATSC_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Hybrid ATSC_vistaRC***
[AVer_H788_HyATSC_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Hybrid ATSC 2 AV-in***
[AVer_H788_HyATSC_II.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Pure ATSC***
[AVer_H788_PuATSC.AddReg]
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Pure ATSC_RC***
[AVer_H788_PuATSC_RC.AddReg]
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Pure ATSC_vistaRC***
[AVer_H788_PuATSC_vistaRC.AddReg]
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Pure Analog_RC***
[AVer_H788_Analog_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 Pure Analog_vistaRC***
[AVer_H788_Analog_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia H788 Hybrid DVBT II_RC***
[AVer_H788_HyDVBT_II_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 Hybrid DVBT II_vistaRC***
[AVer_H788_HyDVBT_II_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia H788 Pure DVBT II_RC***
[AVer_H788_PuDVBT_II_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 Pure DVBT II_vistaRC***
[AVer_H788_PuDVBT_II_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia H788 Pure Analog II_RC ***
[AVer_H788_Analog_II_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 Pure Analog II_vistaRC ***
[AVer_H788_Analog_II_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia A701 ***
[AVer_A701.AddReg]
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,4
HKR, "Parameters", Prefix,,"AVerMedia BDA"

;******** AVerMedia HC83_ATSC ***
[AVer_HC83_ATSC.AddReg]
HKR, "Parameters", "PowerSaveMode",0x00010001,1
HKR, "Parameters", "AVerParam_1",0x00010001,1

HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_AnalogIFLevel",0x00010001,3

;******** AVerMedia HC83_DVBT ***
[AVer_HC83_DVBT.AddReg]
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,4
HKR, "Parameters", "PowerSaveMode",0x00010001,1

HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_AnalogIFLevel",0x00010001,3

;******** AVerMedia M799_RC ***
[AVer_M799_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", ForceTunerStdName,," SBTD-T Tuner"

;******** AVerMedia A188 ***
[AVer_A188.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "I2CBus0Speed",0x00010001,3 
HKR, "Parameters", "I2CBus1Speed",0x00010001,3

;IF Frequency 
HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,5095000
HKR, "Parameters", "Afa9013_8M_IF_FREQ",0x00010001,5095000

;******** AVerMedia A188_RC ***
[AVer_A188_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "I2CBus0Speed",0x00010001,3 
HKR, "Parameters", "I2CBus1Speed",0x00010001,3

;IF Frequency 
HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,5095000
HKR, "Parameters", "Afa9013_8M_IF_FREQ",0x00010001,5095000

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 1

;******** AVerMedia A188_ATSC *** 
[AVer_A188_ATSC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "I2CBus0Speed",0x00010001,3 
HKR, "Parameters", "I2CBus1Speed",0x00010001,3
HKR, "Parameters", "AVerParam_1",0x00010001,1

;ATSC: 
HKR, "Parameters", "TDA18271_IF_FREQ",0x00010001,6000000
HKR, "Parameters", "TDA18271_ATSC_STD",0x00010001,0x1E
HKR, "Parameters", "Enable_SAW_FILTER",0x00010001,1
HKR, "Parameters", "3304_8VSB_IF_1",0x00010001,0xfe
HKR, "Parameters", "3304_8VSB_IF_2",0x00010001,0x9c
HKR, "Parameters", "3304_8VSB_IF_3",0x00010001,0x08
HKR, "Parameters", "3304_8VSB_IF_4",0x00010001,0xe3
 
HKR, "Parameters", "IFAGC_TOP",0x00010001,0x0a
HKR, "Parameters", "RFAGC_TOP",0x00010001,0x03

HKR, "Parameters", "REG_0X30E_8VSB",0x00010001,0x4C
HKR, "Parameters", "TDA18271_IFLevel_ATSC",0x00010001,0
 
;QAM:
HKR, "Parameters", "TDA18271_IF_FREQ_QAM",0x00010001,4200000
HKR, "Parameters", "TDA18271_QAM_STD",0x00010001,0x10
HKR, "Parameters", "Enable_SAW_FILTER_QAM",0x00010001,0
HKR, "Parameters", "3304_QAM_IF_1",0x00010001,0xca
HKR, "Parameters", "3304_QAM_IF_2",0x00010001,0xc0
HKR, "Parameters", "3304_QAM_IF_3",0x00010001,0x83
HKR, "Parameters", "3304_QAM_IF_4",0x00010001,0x12

;******** AVerMedia A188_ATSC_RC *** 
[AVer_A188_ATSC_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "I2CBus0Speed",0x00010001,3 
HKR, "Parameters", "I2CBus1Speed",0x00010001,3
HKR, "Parameters", "AVerParam_1",0x00010001,1

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 1

;ATSC: 
HKR, "Parameters", "TDA18271_IF_FREQ",0x00010001,6000000
HKR, "Parameters", "TDA18271_ATSC_STD",0x00010001,0x1E
HKR, "Parameters", "Enable_SAW_FILTER",0x00010001,1
HKR, "Parameters", "3304_8VSB_IF_1",0x00010001,0xfe
HKR, "Parameters", "3304_8VSB_IF_2",0x00010001,0x9c
HKR, "Parameters", "3304_8VSB_IF_3",0x00010001,0x08
HKR, "Parameters", "3304_8VSB_IF_4",0x00010001,0xe3
 
HKR, "Parameters", "IFAGC_TOP",0x00010001,0x0a
HKR, "Parameters", "RFAGC_TOP",0x00010001,0x03

HKR, "Parameters", "REG_0X30E_8VSB",0x00010001,0x4C
HKR, "Parameters", "TDA18271_IFLevel_ATSC",0x00010001,0
 
;QAM:
HKR, "Parameters", "TDA18271_IF_FREQ_QAM",0x00010001,4200000
HKR, "Parameters", "TDA18271_QAM_STD",0x00010001,0x10
HKR, "Parameters", "Enable_SAW_FILTER_QAM",0x00010001,0
HKR, "Parameters", "3304_QAM_IF_1",0x00010001,0xca
HKR, "Parameters", "3304_QAM_IF_2",0x00010001,0xc0
HKR, "Parameters", "3304_QAM_IF_3",0x00010001,0x83
HKR, "Parameters", "3304_QAM_IF_4",0x00010001,0x12

;******** AVerMedia A188_vista ***
[AVer_A188_vista.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "I2CBus0Speed",0x00010001,3 
HKR, "Parameters", "I2CBus1Speed",0x00010001,3

;IF Frequency 
HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,5095000
HKR, "Parameters", "Afa9013_8M_IF_FREQ",0x00010001,5095000

;******** AVerMedia A188_vistaRC ***
[AVer_A188_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "I2CBus0Speed",0x00010001,3 
HKR, "Parameters", "I2CBus1Speed",0x00010001,3

;IF Frequency 
HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,5095000
HKR, "Parameters", "Afa9013_8M_IF_FREQ",0x00010001,5095000

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia A188_ATSC_vista *** 
[AVer_A188_ATSC_vista.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "I2CBus0Speed",0x00010001,3 
HKR, "Parameters", "I2CBus1Speed",0x00010001,3
HKR, "Parameters", "AVerParam_1",0x00010001,1

;ATSC: 
HKR, "Parameters", "TDA18271_IF_FREQ",0x00010001,6000000
HKR, "Parameters", "TDA18271_ATSC_STD",0x00010001,0x1E
HKR, "Parameters", "Enable_SAW_FILTER",0x00010001,1
HKR, "Parameters", "3304_8VSB_IF_1",0x00010001,0xfe
HKR, "Parameters", "3304_8VSB_IF_2",0x00010001,0x9c
HKR, "Parameters", "3304_8VSB_IF_3",0x00010001,0x08
HKR, "Parameters", "3304_8VSB_IF_4",0x00010001,0xe3
 
HKR, "Parameters", "IFAGC_TOP",0x00010001,0x0a
HKR, "Parameters", "RFAGC_TOP",0x00010001,0x03

HKR, "Parameters", "REG_0X30E_8VSB",0x00010001,0x4C
HKR, "Parameters", "TDA18271_IFLevel_ATSC",0x00010001,0
 
;QAM:
HKR, "Parameters", "TDA18271_IF_FREQ_QAM",0x00010001,4200000
HKR, "Parameters", "TDA18271_QAM_STD",0x00010001,0x10
HKR, "Parameters", "Enable_SAW_FILTER_QAM",0x00010001,0
HKR, "Parameters", "3304_QAM_IF_1",0x00010001,0xca
HKR, "Parameters", "3304_QAM_IF_2",0x00010001,0xc0
HKR, "Parameters", "3304_QAM_IF_3",0x00010001,0x83
HKR, "Parameters", "3304_QAM_IF_4",0x00010001,0x12

;******** AVerMedia A188_ATSC_vistaRC *** 
[AVer_A188_ATSC_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "I2CBus0Speed",0x00010001,3 
HKR, "Parameters", "I2CBus1Speed",0x00010001,3
HKR, "Parameters", "AVerParam_1",0x00010001,1

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;ATSC: 
HKR, "Parameters", "TDA18271_IF_FREQ",0x00010001,6000000
HKR, "Parameters", "TDA18271_ATSC_STD",0x00010001,0x1E
HKR, "Parameters", "Enable_SAW_FILTER",0x00010001,1
HKR, "Parameters", "3304_8VSB_IF_1",0x00010001,0xfe
HKR, "Parameters", "3304_8VSB_IF_2",0x00010001,0x9c
HKR, "Parameters", "3304_8VSB_IF_3",0x00010001,0x08
HKR, "Parameters", "3304_8VSB_IF_4",0x00010001,0xe3
 
HKR, "Parameters", "IFAGC_TOP",0x00010001,0x0a
HKR, "Parameters", "RFAGC_TOP",0x00010001,0x03

HKR, "Parameters", "REG_0X30E_8VSB",0x00010001,0x4C
HKR, "Parameters", "TDA18271_IFLevel_ATSC",0x00010001,0
 
;QAM:
HKR, "Parameters", "TDA18271_IF_FREQ_QAM",0x00010001,4200000
HKR, "Parameters", "TDA18271_QAM_STD",0x00010001,0x10
HKR, "Parameters", "Enable_SAW_FILTER_QAM",0x00010001,0
HKR, "Parameters", "3304_QAM_IF_1",0x00010001,0xca
HKR, "Parameters", "3304_QAM_IF_2",0x00010001,0xc0
HKR, "Parameters", "3304_QAM_IF_3",0x00010001,0x83
HKR, "Parameters", "3304_QAM_IF_4",0x00010001,0x12

;******** AVerMedia A177_RC ***
[AVer_A177_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1

HKR, "Parameters", "FMPath",0x00010001, 4

; Enable RF frequency offset auto detection for DVB-T, 
HKR, "Parameters","EnableAutoOffset",0x00010001,0x01

; Don't use tuning thread, 
HKR, "Parameters", "TDA8275A_UseTuningThread" , 0x00010001, 0x00

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia A177_vistaRC ***
[AVer_A177_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1

HKR, "Parameters", "FMPath",0x00010001, 4

; Enable RF frequency offset auto detection for DVB-T, 
HKR, "Parameters","EnableAutoOffset",0x00010001,0x01

; Don't use tuning thread, 
HKR, "Parameters", "TDA8275A_UseTuningThread" , 0x00010001, 0x00

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia A707_RC ***
[AVer_A707_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,1

HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,4000000
HKR, "Parameters", "Afa9033_8M_IF_FREQ",0x00010001,4000000
HKR, "Parameters", "TDA18271_DVBT_8M_STD",0x00010001,0x19

;HKR, "Parameters", "TDA18271_AnalogIFLevel_PAL_B",0x00010001,0
;HKR, "Parameters", "TDA18271_AnalogIFLevel_SCEAM_L",0x00010001,1

;HKR, "Parameters", "Gafixd_PAL_B",0x00010001,1
;HKR, "Parameters", "Gafixd_SCEAM_L",0x00010001,1
;HKR, "Parameters", "DTV_GAIN1_PAL_B",0x00010001,5
;HKR, "Parameters", "DTV_GAIN1_SCEAM_L",0x00010001,0
HKR, "Parameters", "SECAML_SSIF_LEVEL",0x00010001,2

HKR, "Parameters", "I2CBus0Speed",0x00010001,0
HKR, "Parameters", "I2CBus1Speed",0x00010001,4

HKR, "Parameters", "DgtlPacketNumber",0x00010001,312

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

HKR, "Parameters", "DVBS_I2C_DelayTime", 0x00010001, 5
;AVEREth.sys
HKR, "ENUM\Device1",pnpid,,"AVerMedia.EtherNet"		  ; Virtual Network driver for data service.

;CICA Support
HKR, "Parameters", "CICAEnable", 0x00010001, 1
HKR, "Parameters", "CICAI2CBus", 0x00010001, 0

;******** AVerMedia A707_DVBT ***
[AVer_A707_DVBT.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,1

HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,4000000
HKR, "Parameters", "Afa9033_8M_IF_FREQ",0x00010001,4000000
HKR, "Parameters", "TDA18271_DVBT_8M_STD",0x00010001,0x19
HKR, "Parameters", "SECAML_SSIF_LEVEL",0x00010001,2

HKR, "Parameters", "I2CBus0Speed",0x00010001,0
HKR, "Parameters", "I2CBus1Speed",0x00010001,4

HKR, "Parameters", "DgtlPacketNumber",0x00010001,312

;CICA Support
HKR, "Parameters", "CICAEnable", 0x00010001, 1
HKR, "Parameters", "CICAI2CBus", 0x00010001, 0

;******** AVerMedia A707_VistaRC ***
[AVer_A707_VistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,1

HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,4000000
HKR, "Parameters", "Afa9033_8M_IF_FREQ",0x00010001,4000000
HKR, "Parameters", "TDA18271_DVBT_8M_STD",0x00010001,0x19

;HKR, "Parameters", "TDA18271_AnalogIFLevel_PAL_B",0x00010001,0
;HKR, "Parameters", "TDA18271_AnalogIFLevel_SCEAM_L",0x00010001,1
HKR, "Parameters", "SECAML_SSIF_LEVEL",0x00010001,2

;HKR, "Parameters", "Gafixd_PAL_B",0x00010001,1
;HKR, "Parameters", "Gafixd_SCEAM_L",0x00010001,1
;HKR, "Parameters", "DTV_GAIN1_PAL_B",0x00010001,5
;HKR, "Parameters", "DTV_GAIN1_SCEAM_L",0x00010001,0

HKR, "Parameters", "I2CBus0Speed",0x00010001,0
HKR, "Parameters", "I2CBus1Speed",0x00010001,4

HKR, "Parameters", "DgtlPacketNumber",0x00010001,312

HKR, "Parameters", "DVBS_I2C_DelayTime", 0x00010001, 5

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;AVEREth.sys
HKR, "ENUM\Device1",pnpid,,"AVerMedia.EtherNet"		  ; Virtual Network driver for data service.

;CICA Support
HKR, "Parameters", "CICAEnable", 0x00010001, 1
HKR, "Parameters", "CICAI2CBus", 0x00010001, 0

;******** AVerMedia A750 ***
[AVer_A750.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 1

HKR, "Parameters", "I2CBus0Speed",0x00010001,1	; 400KHz
HKR, "Parameters", "I2CBus1Speed",0x00010001,3	; 75KHz
HKR, "Parameters", ForceTunerStdName,," DTMB Tuner"

;******** AVerMedia A750_VistaRc ***
[AVer_A750_VistaRc.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 1

HKR, "Parameters", "I2CBus0Speed",0x00010001,1	; 400KHz
HKR, "Parameters", "I2CBus1Speed",0x00010001,3	; 75KHz
HKR, "Parameters", ForceTunerStdName,," DTMB Tuner"

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;*** strings, GUIDs and names
;
[Strings]

SERVICE_NAME_X32         = "AVerBDA6x"

; Proxy GUIDs

KSProxy.CLSID            = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSXBar.CLSID             = "{71F96460-78F3-11d0-A18C-00A0C9118956}"
KSTVAudio.CLSID          = "{71F96462-78F3-11d0-A18C-00A0C9118956}"
KSTvTune.CLSID           = "{266EEE40-6C63-11cf-8A03-00AA006ECB65}"

; Category GUIDs

KSCATEGORY_MULTIPLEXER   = "{7A5DE1D3-01A1-452c-B481-4FA2B96271E8}"
KSCATEGORY_ENCODER       = "{19689BF6-C384-48fd-AD51-90E58C79F70B}"
KSCATEGORY_CAPTURE       = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO         = "{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_AUDIO         = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}"

; Our Pin Name GUIDs

AVSTREAM_ANLG_AUDIO_IN_PIN   = "{7BB284B9-714D-493d-A101-B1B028E782BD}"
AVSTREAM_ANLG_AUDIO_OUT_PIN  = "{5582E657-E596-42b5-9DB3-541B27A2355F}"
AVSTREAM_ANLG_VIDEO_ITU_PIN  = "{82631A2E-403C-4581-A4B0-EC173D004410}"
AVSTREAM_ANLG_AUDIO_I2S_PIN  = "{C2E46358-F032-4d88-B802-06B59D162730}"
AVSTREAM_ANLG_VIDEO_PIN      = "{16FFBD0A-F770-4692-A2FF-DD394DFE9564}"
AVSTREAM_ANLG_AUDIO_PIN      = "{BA9E27B1-CF44-490e-8EAB-5F662E5FFE74}"

; system defines

SERVICE_BOOT_START     = 0x0 
SERVICE_SYSTEM_START   = 0x1 
SERVICE_AUTO_START     = 0x2 
SERVICE_DEMAND_START   = 0x3 
SERVICE_DISABLED       = 0x4 

SERVICE_KERNEL_DRIVER  = 0x1 
SERVICE_ERROR_IGNORE   = 0x0 
SERVICE_ERROR_NORMAL   = 0x1 
SERVICE_ERROR_SEVERE   = 0x2
SERVICE_ERROR_CRITICAL = 0x3 

FLG_REGSVR_DLLREGISTER = 0x00000001

;Our strings

AVer                     = "AVerMedia TECHNOLOGIES, Inc."
60Hybrid.DeviceDesc      = "NXP SAA7160, Hybrid Capture Device"
61Hybrid.DeviceDesc      = "NXP SAA7161, Hybrid Capture Device"
62Hybrid.DeviceDesc      = "NXP SAA7162, Hybrid Capture Device"
63Hybrid.DeviceDesc      = "NXP SAA7163  Hybrid Capture Device"

AVer.DeviceDesc00        = "AVerMedia M789 PCIe Pure DVBT"
AVer.DeviceDesc01        = "AVerMedia M789 PCIe Dual DVBT"
AVer.DeviceDesc02        = "AVerMedia M788 PCIe Hybrid Analog/ATSC"
AVer.DeviceDesc03        = "AVerMedia A317 Mini-Card Hybrid Analog/ATSC"
AVer.DeviceDesc04        = "AVerMedia A701 PCIe Hybrid Analog/DVBT, Combo DVBS"
AVer.DeviceDesc05        = "AVerMedia HC82 Express-Card Hybrid Analog/ATSC"
AVer.DeviceDesc06        = "AVerMedia HC82 Express-Card Hybrid Analog/DVBT"
AVer.DeviceDesc07        = "AVerMedia A316 Mini-Card Hybrid Analog/DVBT"
AVer.DeviceDesc08        = "AVerMedia H788 PCIe Hybrid Analog/DVBT"
AVer.DeviceDesc09        = "AVerMedia H788 PCIe DVBT"
AVer.DeviceDesc10        = "AVerMedia H788 PCIe Hybrid Analog/ATSC"
AVer.DeviceDesc11        = "AVerMedia H788 PCIe ATSC"
AVer.DeviceDesc12        = "AVerMedia H788 PCIe Analog"
AVer.DeviceDesc13        = "AVerMedia M799 PCIe Hybrid SBTD-T"
AVer.DeviceDesc14        = "AVerMedia A317D Mini-Card ATSC"
AVer.DeviceDesc15        = "AVerMedia A327 Mini-Card Hybrid Analog/ATSC"
AVer.DeviceDesc16        = "AVerMedia A326 Mini-Card Hybrid Analog/DVBT"
AVer.DeviceDesc17        = "AVerMedia A188 PCIe Duo Hybrid Analog/DVBT"
AVer.DeviceDesc18        = "AVerMedia A188C PCIe Duo Hybrid Analog/ATSC"
AVer.DeviceDesc19        = "AVerMedia A188 PCIe Analog"
AVer.DeviceDesc20        = "AVerMedia A188 PCIe Pure DVBT"
AVer.DeviceDesc21        = "AVerMedia A188C PCIe Pure ATSC"
AVer.DeviceDesc22        = "AVerMedia A177 PCIe Dual Hybrid Analog/DVBT"
AVer.DeviceDesc23        = "AVerMedia A707 PCIe Dual Hybrid Analog/DVBT/DVBS"
AVer.DeviceDesc24        = "AVerMedia A188O PCIe Duo Hybrid Analog/DVBT"
AVer.DeviceDesc25        = "AVerMedia HC83 Express-Card Hybrid Analog/ATSC"
AVer.DeviceDesc26        = "AVerMedia HC83 Express-Card Hybrid Analog/DVBT"
AVer.DeviceDesc27        = "AVerMedia A311 Mini-Card Dual DVBT"
AVer.DeviceDesc28        = "AVerMedia A750 PCIe DTMB"
AVer.DeviceDesc29        = "AVerMedia A707 PCIe Pure DVBT"

AVSTRM_INSTALLATION_DISK = "AVerBDA6x installation disk"
DISPLAY_NAME             = "AVerBDA6x service"
SERVICE_DESCRIPTION      = "The PCIe capture driver"
MediaInterfaces          = "System\CurrentControlSet\Control\MediaInterfaces"
