;==============================================================================
; TerraTec Cinergy 400 mobile
; WDM Driver Install Script
; Copyright (c) 2004, TerraTec Electronic GmbH
;------------------------------------------------------------------------------
; Notes:
;  a) Driver filenames must be <= 8 characters (8.3 format) !
;  b) Win9x: On Windows 98/Me, section names should be no longer than 28 characters.
;  c) Win9x: [SourceDisksNames] must always come before [SourceDisksFiles]  !!!   
;  d) Win9x: Filenames must be in 8.3 format  !              
;  e) Win9x: Registry pathes must use single slashes
;  f) [xxx.KnownFiles] sections are used by Win9x only
;  g) [xxx.Services] sections are used by WinNT only
;  h) If we have OS specific DDInstall sections we must have 
;     OS specific [xxx.Interfaces] and [.HW] also!
;
;
; History:
;------------------------------------------------------------------------------
; 07-Jul-04 - FMB initial version
;==============================================================================

[Version]
LayoutFile=layout.inf, layout1.inf, layout2.inf
Signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%TerraTec%
; _OEM_  Enter name of .cat file from WHQL, containing the digital signature.
; _OEM_  The catalog file has to be in the same location as the INF file.
CatalogFile=vm7133.cat
DriverVer=07/07/2004, 2.5.11.5228


[SourceDisksNames]
1=%DiskName%,,
;1=%DiskName%,"Cinergy400mobile.CAB",

[SourceDisksFiles]
;Philips files
vm7133.sys=1
34api.dll=1
34pciurd.dll=1
34i2curd.dll=1
34dd.dll=1
34ds.dll=1
34dialog.dll=1
34dlg2.dll=1
34TvCtrl.dll=1
34com.dll=1
Prop7134.dll=1
vm7133.hlp=1

[ControlFlags]

[DestinationDirs]
Cap7134.CopyDrivers = 10,system32\drivers
KSUpdate.Dll = 11
;Uninst.CopyFiles = 10

[Manufacturer]
%TerraTec%=TerraTec

[TerraTec]                   
; TerraTec Cinergy 400 mobile (SAA7133/5)
%CinergyCap.Desc%    = Cap7134.Device,PCI\VEN_1131&DEV_7133&SUBSYS_1162153B
; TerraTec Cinergy 400 mobile (SAA7134)
%CinergyCap.Desc%    = Cap7134.Device,PCI\VEN_1131&DEV_7134&SUBSYS_1162153B

;Prototypes
%CinergyCap.Desc%    = Cap7134.Device,PCI\VEN_1131&DEV_7133&SUBSYS_4ee91131
%CinergyCap.Desc%    = Cap7134.Device,PCI\VEN_1131&DEV_7134&SUBSYS_4ee91131

;------------------------------------------------------------------------------
; Cinergy 400 mobile
;------------------------------------------------------------------------------
[Cap7134.Device]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, ComRegister.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
; FMB NOTE: KnownFiles only supported by Win9x
KnownFiles=   Cap7134.KnownFiles

[Cap7134.Device.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
; RegisterDlls:This directive is supported on Windows 2000 and later
; but it doesn't work under Win2K. However, calling RegSvr32.exe via RunOnce is not allowed for WHQL
RegisterDlls= ComRegister.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

;==============================================================================
; Main Registry settings
;==============================================================================
[Cap713x.AddRegProteus]
;------------------------------------------------------------------------------
; Video routing
;------------------------------------------------------------------------------
; the values map to the video input modes
; as described in the SAA7134 User Manual p.24
HKR, "Decoder", "Tuner Channel",0x00010001,1
HKR, "Decoder", "CVBS Channel",0x00010001,3
HKR, "Decoder", "CVBS Channel2",0x00010001,0
HKR, "Decoder", "SVHS Channel",0x00010001,6
HKR, "Decoder", "SVHS Channel2",0x00010001,9
; _OEM_  Insert the appropriate preferred video standard here.
; _OEM_  If no video standard can be detected (e.g. if no
; _OEM_  video source is connected), this standard is assumed:
; _OEM_     KS_AnalogVideo_PAL_B    = 0x00000010
; _OEM_     KS_AnalogVideo_NTSC_M   = 0x00000001
; _OEM_     KS_AnalogVideo_NTSC_M_J = 0x00000002
; _OEM_     see Windows DDK for other video standards
HKR, "Decoder", "Preferred Video Standard",0x00010001,0x00000010    ; KS_AnalogVideo_PAL_B
; _OEM_  Insert the default VBI sampling frequency and line length here.
HKR, "Decoder", "VBI Sampling Frequency",0x00010001,27000000
HKR, "Decoder", "VBI Pitch",0x00010001,1440

;Common registry entries for SAA7134 and SAA7130
[Cap713x.AddReg]
; 34 Proteus Board Settings
;------------------------------------------------------------------------------
; Audio routing
;------------------------------------------------------------------------------
; maps user setting to hardware input (1=SIF, 2=Analog1, 3=Analog2)  
HKR, "BoardSetting", "Tuner"     , 0x00010001,1
HKR, "BoardSetting", "Composite1", 0x00010001,3
HKR, "BoardSetting", "SVideo1"   , 0x00010001,3
HKR, "BoardSetting", "Composite2", 0x00010001,3
HKR, "BoardSetting", "SVideo2"   , 0x00010001,3
HKR, "BoardSetting", "FM"        , 0x00010001,2

; _OEM_  Set this value to 1, if the chip supports FM Radio decoding from SIF input
HKR, "BoardSetting", "FM Radio from SIF",0x00010001,0

HKR, "BoardSetting", "GPIO18 Setting",0x00010001,1	; GPIO18

HKR, "BoardSetting", "VM0001 Setting*",0x00010001,1
HKR, "BoardSetting", "VM0101 Setting*",0x00010001,1
HKR, "BoardSetting", "VM0201 Setting*",0x00010001,1

HKR,"","WorkaroundforTVBrightness",0x00010001,-11
;------------------------------------------------------------------------------
; Workarounds
;------------------------------------------------------------------------------
HKR, "", "WorkaroundforStandardChange",0x00010001,0

HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,vm7133.sys
HKR,,PageOutWhenUnopened,3,0
HKR,,DontSuspendIfStreamsAreRunning,3,00
;------------------------------------------------------------------------------
; Crossbar pins
;------------------------------------------------------------------------------
; _OEM_ Here you can select, which pins are exposed by the crossbar filter
HKR, "Parameters", "VideoTunerEnabled",0x00010001,1
HKR, "Parameters", "SVideoEnabled",0x00010001,1
HKR, "Parameters", "CompositeEnabled",0x00010001,1
HKR, "Parameters", "SVideo2Enabled",0x00010001,1

; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "vmPhTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"vmPhTune"
;------------------------------------------------------------------------------
; Settings for video inputs
;------------------------------------------------------------------------------

;>>> decoder defaults for tuner input
HKR, "Decoder\SRC0", "Brightness" ,0x00010001,0x80
HKR, "Decoder\SRC0", "Contrast"   ,0x00010001,0x44
HKR, "Decoder\SRC0", "Saturation" ,0x00010001,0x40
HKR, "Decoder\SRC0", "HUE"        ,0x00010001,0x00
HKR, "Decoder\SRC0", "Sharpness"  ,0x00010001,0x00
HKR, "Decoder\SRC0", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC0", "Y-Filter"   ,0x00010001,0x01
HKR, "Decoder\SRC0", "C-Filter"   ,0x00010001,0x01
HKR, "Decoder\SRC0", "C-Bypass"   ,0x00010001,0x00
HKR, "Decoder\SRC0", "White Peak Control",0x00010001,0x01
HKR, "Decoder\SRC0", "Gain Auto",0x00010001,0x01
HKR, "Decoder\SRC0", "Gain1",0x00010001,0x7F
HKR, "Decoder\SRC0", "Gain2",0x00010001,0x7F
;>>>  decoder defaults for composite 1 source
HKR, "Decoder\SRC1", "Brightness" ,0x00010001,0x80
HKR, "Decoder\SRC1", "Contrast"   ,0x00010001,0x44
HKR, "Decoder\SRC1", "Saturation" ,0x00010001,0x40
HKR, "Decoder\SRC1", "HUE"        ,0x00010001,0x00
HKR, "Decoder\SRC1", "Sharpness"  ,0x00010001,0x00
HKR, "Decoder\SRC1", "Source Type",0x00010001,0x01
HKR, "Decoder\SRC1", "Y-Filter"   ,0x00010001,0x01
HKR, "Decoder\SRC1", "C-Filter"   ,0x00010001,0x01
HKR, "Decoder\SRC1", "C-Bypass"   ,0x00010001,0x00
HKR, "Decoder\SRC1", "White Peak Control",0x00010001,0x01
HKR, "Decoder\SRC1", "Gain Auto",0x00010001,0x01
HKR, "Decoder\SRC1", "Gain1",0x00010001,0x7F
HKR, "Decoder\SRC1", "Gain2",0x00010001,0x7F
;>>>  decoder defaults for composite 2 source
HKR, "Decoder\SRC2", "Brightness" ,0x00010001,0x80
HKR, "Decoder\SRC2", "Contrast"   ,0x00010001,0x44
HKR, "Decoder\SRC2", "Saturation" ,0x00010001,0x40
HKR, "Decoder\SRC2", "HUE"        ,0x00010001,0x00
HKR, "Decoder\SRC2", "Sharpness"  ,0x00010001,0x00
HKR, "Decoder\SRC2", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC2", "Y-Filter"   ,0x00010001,0x01
HKR, "Decoder\SRC2", "C-Filter"   ,0x00010001,0x01
HKR, "Decoder\SRC2", "C-Bypass"   ,0x00010001,0x00
HKR, "Decoder\SRC2", "White Peak Control",0x00010001,0x01
HKR, "Decoder\SRC2", "Gain Auto",0x00010001,0x01
HKR, "Decoder\SRC2", "Gain1",0x00010001,0x7F
HKR, "Decoder\SRC2", "Gain2",0x00010001,0x7F
;>>>  decoder defaults for SVHS 1 source
HKR, "Decoder\SRC3", "Brightness" ,0x00010001,0x80
HKR, "Decoder\SRC3", "Contrast"   ,0x00010001,0x44
HKR, "Decoder\SRC3", "Saturation" ,0x00010001,0x40
HKR, "Decoder\SRC3", "HUE"        ,0x00010001,0x00
HKR, "Decoder\SRC3", "Sharpness"  ,0x00010001,0x00
HKR, "Decoder\SRC3", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC3", "Y-Filter"   ,0x00010001,0x00
HKR, "Decoder\SRC3", "C-Filter"   ,0x00010001,0x01
HKR, "Decoder\SRC3", "C-Bypass"   ,0x00010001,0x01
HKR, "Decoder\SRC3", "White Peak Control",0x00010001,0x01
HKR, "Decoder\SRC3", "Gain Auto",0x00010001,0x01
HKR, "Decoder\SRC3", "Gain1",0x00010001,0x7F
HKR, "Decoder\SRC3", "Gain2",0x00010001,0x7F
;>>>  decoder defaults for SVHS 2 source
HKR, "Decoder\SRC4", "Brightness" ,0x00010001,0x80
HKR, "Decoder\SRC4", "Contrast"   ,0x00010001,0x44
HKR, "Decoder\SRC4", "Saturation" ,0x00010001,0x40
HKR, "Decoder\SRC4", "HUE"        ,0x00010001,0x00
HKR, "Decoder\SRC4", "Sharpness"  ,0x00010001,0x00
HKR, "Decoder\SRC4", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC4", "Y-Filter"   ,0x00010001,0x00
HKR, "Decoder\SRC4", "C-Filter"   ,0x00010001,0x01
HKR, "Decoder\SRC4", "C-Bypass"   ,0x00010001,0x01
HKR, "Decoder\SRC4", "White Peak Control",0x00010001,0x01
HKR, "Decoder\SRC4", "Gain Auto",0x00010001,0x01
HKR, "Decoder\SRC4", "Gain1",0x00010001,0x7F
HKR, "Decoder\SRC4", "Gain2",0x00010001,0x7F

;Registry entries irrelevant for SAA7130
[Cap7134.AddReg]
HKR,,Driver,,vm7133.sys

; possible 'software' audio enable/disable switch (0=disable,1=enable)
HKR, "Parameters", "AudioEnabled",0x00010001,1          ; all audio
HKR, "Parameters", "AudioTunerEnabled",0x00010001,1     ; tuner audio
HKR, "Parameters", "AudioFMEnabled",0x00010001,0        ; FM audio

;>>> audio settings for tuner input

; 'CountryCode' reflects the used Country
; and is used as a table entry to 'DefaultStandard' and 'StandardTable'
; in order to perform a country dependant audio standard search
HKR, "", "CountryCode",,"49"    ; Germany

; 'XTAL' reflects the used hardware crystal (0=32.11MHz,1=24.567MHz)
HKR, "Audio", "XTAL",0x00010001,0x00
; 'DetectMode' reflects the used audio detection mode (1=automatic mode,0=manual mode)
HKR, "Audio", "DetectMode",0x00010001,0x01
; 'Voltage Input Select' defines the input voltage of the 2 external inputs (0=1.0 Vrms/1=2.0 Vrms)
HKR, "Audio", "Voltage Input Select Ext1",0x00010001,0x00
HKR, "Audio", "Voltage Input Select Ext2",0x00010001,0x00
; 'I2S Output' reflects the state of the two I2S output channels (1=enabled/0=disabled)
HKR, "Audio", "I2S Output",0x00010001,0x01
HKR, "Audio", "I2S2 Output",0x00010001,0x01
; 'Virtual Stereo Effect' is the pre-defined width of 'Philips Incredible Stereo' (0=narrow...5=wide)
HKR, "Audio", "Virtual Stereo Effect",0x00010001,0x04
; Audio master clock settings
HKR, "Audio", "MClk Output Enable",0x00010001,0x0
HKR, "Audio", "MClk Frequency",0x00010001,0x0
HKR, "Audio", "MClk Reference Switch",0x00010001,0x0
HKR, "Audio", "MClk Reference Divider",0x00010001,0x2

; 'DefaultStandard'
; in automatic mode: 'DefaultStandard' is used as a fallback if nothing is detected
; in manual mode:    'DefaultStandard' is used as standard to be set
;   2  = B/G   Mono           
;   3  = D/K   Mono           
;   4  = M     Mono           
;   5  = B/G   A2
;   6  = B/G   Nicam
;   7  = D/K   A2 Type 1
;   8  = D/K   A2 Type 2
;   9  = D/K   A2 Type 3
;   10 = D/K   Nicam
;   11 = L/L'  Nicam
;   12 = L/L'  AM
;   13 = I     Nicam
;   14 = I     Mono
;   15 = M     Korea
;   16 = M     BTSC
HKR, "Audio\DefaultStandard", "01",0x00010001,16   ; USA:            M    BTSC
HKR, "Audio\DefaultStandard", "31",0x00010001,5    ; Netherlands:    B/G  A2
HKR, "Audio\DefaultStandard", "32",0x00010001,6    ; Belgium:        B/G  Nicam
HKR, "Audio\DefaultStandard", "33",0x00010001,11   ; France:         L/L' Nicam
HKR, "Audio\DefaultStandard", "34",0x00010001,5    ; Spain:          B/G  A2
HKR, "Audio\DefaultStandard", "39",0x00010001,5    ; Italy:          B/G  A2
HKR, "Audio\DefaultStandard", "41",0x00010001,5    ; Switzerland:    B/G  A2
HKR, "Audio\DefaultStandard", "44",0x00010001,13   ; Great Britain:  I    Nicam
HKR, "Audio\DefaultStandard", "45",0x00010001,6    ; Denmark         B/G  Nicam
HKR, "Audio\DefaultStandard", "46",0x00010001,6    ; Sweden:         B/G  Nicam
HKR, "Audio\DefaultStandard", "47",0x00010001,6    ; Norway:         B/G  Nicam
HKR, "Audio\DefaultStandard", "49",0x00010001,5    ; Germany:        B/G  A2
HKR, "Audio\DefaultStandard", "81",0x00010001,16   ; Japan:          M    BTSC
HKR, "Audio\DefaultStandard", "86",0x00010001,7    ; China:          D/K  A2 Type 1
HKR, "Audio\DefaultStandard","351",0x00010001,5    ; Portugal/Azores:B/G  A2
HKR, "Audio\DefaultStandard","358",0x00010001,6    ; Finland:        B/G  Nicam
HKR, "Audio\DefaultStandard","420",0x00010001,10   ; Czech Republic: D/K  Nicam

; 'StandardTable'
; in automatic mode: StandardTable is used to set the standard groups to be searched
; bit array:
;   bit1 = B/G
;   bit2 = D/K
;   bit3 = L/L'
;   bit4 = I
;   bit5 = M
HKR, "Audio\StandardTable", "01",0x00010001,0x10   ; USA:            M
HKR, "Audio\StandardTable", "31",0x00010001,0x01   ; Netherlands:    B/G
HKR, "Audio\StandardTable", "32",0x00010001,0x01   ; Belgium:        B/G
HKR, "Audio\StandardTable", "33",0x00010001,0x04   ; France:         L/L'
HKR, "Audio\StandardTable", "34",0x00010001,0x01   ; Spain:          B/G
HKR, "Audio\StandardTable", "39",0x00010001,0x01   ; Italy:          B/G
HKR, "Audio\StandardTable", "41",0x00010001,0x01   ; Switzerland:    B/G
HKR, "Audio\StandardTable", "44",0x00010001,0x08   ; Great Britain:  I
HKR, "Audio\StandardTable", "45",0x00010001,0x01   ; Denmark         B/G
HKR, "Audio\StandardTable", "46",0x00010001,0x01   ; Sweden:         B/G
HKR, "Audio\StandardTable", "47",0x00010001,0x01   ; Norway:         B/G
HKR, "Audio\StandardTable", "49",0x00010001,0x01   ; Germany:        B/G
HKR, "Audio\StandardTable", "81",0x00010001,0x10   ; Japan:          M
HKR, "Audio\StandardTable", "86",0x00010001,0x02   ; China:          D/K
HKR, "Audio\StandardTable","351",0x00010001,0x01   ; Portugal/Azores:B/G
HKR, "Audio\StandardTable","358",0x00010001,0x01   ; Finland:        B/G
HKR, "Audio\StandardTable","420",0x00010001,0x02   ; Czech Republic: D/K

; 'GPIO settings'
;
HKR, "GPIO\TransportStream\Parallel", "ClockControl",0x00010001,0x04
;==============================================================================
; Other settings
;==============================================================================





[ComRegister.AddReg]
; FMB NOTE: RunOnce entries must consist only of calls to rundll32.exe. 
; Otherwise, Microsoft will not digitally sign the driver package. (WHQL)
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"AudioProperties",,"%11%\Regsvr32 /s %11%\Prop7134.dll"
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"COMInterface",,"%11%\Regsvr32 /s %11%\34com.dll"


[ComRegister.Register]
;1 = FLG_REGSVR_DLLREGISTER
11,,Prop7134.dll,1 ;FLG_REGSVR_DLLREGISTER
11,,34COM.dll,1    ;FLG_REGSVR_DLLREGISTER

;==============================================================================
; FILE COPY
;==============================================================================

[Cap7134.CopyDrivers]
vm7133.sys


[KSUpdate.Dll]
34api.dll
34pciurd.dll
34i2curd.dll
34dd.dll
34ds.dll
34dialog.dll
34dlg2.dll
34TvCtrl.dll
34com.dll	  ; COM API interface
Prop7134.dll      ; audio property dialog
vm7133.hlp

[Cap7134.KnownFiles]
; FMB NOTE: KnownFiles section for Win9x only
vm7133.sys=safe

;==============================================================================
; CAPTURE INTERFACES 
;==============================================================================
[Cap7134.Device.Interfaces]
AddInterface=%KSCATEGORY_VIDEO%   ,"GLOBAL",VideoCapture
AddInterface=%KSCATEGORY_CAPTURE% ,"GLOBAL",VideoCapture
AddInterface=%KSCATEGORY_CROSSBAR%,"GLOBAL",Crossbar
AddInterface=%KSCATEGORY_TVAUDIO% ,"GLOBAL",TvAudio

[Cap7134.Device.NT.Interfaces]
AddInterface=%KSCATEGORY_VIDEO%   ,"GLOBAL",VideoCapture
AddInterface=%KSCATEGORY_CAPTURE% ,"GLOBAL",VideoCapture
AddInterface=%KSCATEGORY_CROSSBAR%,"GLOBAL",Crossbar
AddInterface=%KSCATEGORY_TVAUDIO% ,"GLOBAL",TvAudio


;------------------------------------------------------------------------------
; Capture
;------------------------------------------------------------------------------

[VideoCapture]
AddReg=VideoCapture.AddReg



[VideoCapture.AddReg]
HKR,,CLSID,,%PROXY_CAPTURE%
HKR,,FriendlyName,,%Cinergy.Capture%    
; Private Pin Names:
; MEDIATYPE_Audio:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{73647561-0000-0010-8000-00AA00389B71},"Name",0x00000000,"Audio"
; GUID_VSB_OUT:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{F3954424-34F6-11D1-821D-0000F8300212},"Name",0x00000000,"Transport In"
; MEDIUM_AUDIO_PHILDEC_ANALOGAUDIOIN:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{0482DEE1-7817-11cf-8a03-00aa006ecb65},"Name",0x00000000,"Analog Audio In"
; GUID_7133XOPIN:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{79C268A2-338C-470C-B1CB-5e233FE34032},"Name",0x00000000,"Transport Out"

;------------------------------------------------------------------------------
; Crossbar
;------------------------------------------------------------------------------
[Crossbar]
AddReg=Crossbar.AddReg

[Crossbar.AddReg]
HKR,,CLSID,,%PROXY_CROSSBAR%
HKR,,FriendlyName,,%Cinergy.Crossbar%
[TvAudio]
AddReg=TvAudio.AddReg

[TvAudio.AddReg]
HKR,,CLSID,,%PROXY_TVAUDIO%
HKR,,FriendlyName,,%Cinergy.TvAudio%
;==============================================================================
; CAPTURE SERVICES 
;==============================================================================

[Cap7134.Device.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.ServiceInstall]
DisplayName   = %Cinergy.Capture%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\vm7133.sys

;---------------------------------------------------------------

;===============================================================
;                S t r i n g s
;===============================================================
[Strings]

;--------------------------------------------------------
; Non-Localizable
;--------------------------------------------------------

SERVICE_KERNEL_DRIVER=1
SERVICE_ERROR_NORMAL=1
SERVICE_AUTO_START=2
SERVICE_DEMAND_START=3

PROXY_CAPTURE      = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
PROXY_CROSSBAR     = "{71F96460-78F3-11D0-A18C-00A0C9118956}"
PROXY_TVAUDIO      = "{71F96462-78F3-11D0-A18C-00A0C9118956}"
PROXY_TVTUNER      = "{266EEE40-6C63-11CF-8A03-00AA006ECB65}"

KSCATEGORY_AUDIO   = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_VIDEO   = "{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_CAPTURE = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_CROSSBAR= "{a799a801-A46D-11D0-A18C-00a02401dcd4}"
KSCATEGORY_TVAUDIO = "{a799a802-A46D-11D0-A18C-00a02401dcd4}"
KSCATEGORY_TVTUNER = "{a799a800-A46D-11D0-A18C-00a02401dcd4}"
KSCATEGORY_VBICODEC= "{07dad660-22f1-11D1-a9f4-00c04fbbde8f}"

refGlobal="GLOBAL"
refWave="WAVE"

;--------------------------------------------------------
; Localizable
;--------------------------------------------------------
TerraTec            = "TerraTec "
DiskName            = "Cinergy Driver CD"

; Device Manager strings
CinergyCap.Desc     = "Cinergy 400 mobile Capture"

; DirectShow Strings
; FMB NOTE:The string "Cinergy.Capture" is used for both audio and video devices !
Cinergy.Capture     = "Cinergy 400 mobile Capture"
Cinergy.Tuner       = "Cinergy 400 mobile Tuner"
Cinergy.Crossbar    = "Cinergy 400 mobile Crossbar"
Cinergy.TvAudio     = "Cinergy 400 mobile TvAudio"
Cinergy.Audio       = "Cinergy 400 mobile Audio Capture"
