This folder contains BDA drivers for Windows XP in the main folder, Windowws XP64 in the AMD64 and Ia64 folders and Window 2000, in the Win2K folder.

There are three remote options you can choose from:

No remote - does not install any remote HID drivers
With remote - gives the option of installing the old remote, new remote (the one currently on our website) or to use the MCE remote via the TinyUSB inbuilt IR receiver.

To update the HID driver follow these steps:

Go to the device manager, under Human Interface Devices
Right Click on DNTV Live! Tiny USB 2.0 HID RC Device
Select Update Driver
No, not this time, Next
Install from a Specific Location, Next
Don't search, I will choose the driver to install, Next
Have Disk,
Browse to the folder you have put the driver downloaded
double click on the "UDTT2HID_Newremote" or "UDTT2HID_oldremote"
OK
Double clcik on the DNTV Live! Tiny USB 2.0 HID RC Device (New remote)
Continue Anyway
Finish
