;****************************************************************************************
;
;   DR71WU.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   D-Link RT73 series USB Wireless LAN Card.
;
;   Copyright (c)2005 , D-Link Corp., All Rights Reserved
;   All Rights Reserved.
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %D-Link%
Compatible      = 1
DriverVer       = 01/15/2008, 1.03.00.0000
CatalogFile     = Dr71WU.cat            ;for WHQL certified

[ControlFlags]
;***********D-Link 802.11g board  ***********
ExcludeFromSelect = VID_07D1&PID_3C03
ExcludeFromSelect = VID_07D1&PID_3C04
ExcludeFromSelect = VID_07D1&PID_3C07


[Manufacturer]
%D-Link%        = D-Link,NTX86, NTAMD64


[D-Link]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%D-Link.DeviceDesc%         = D-Link.ndi,           USB\VID_07D1&PID_3C03
%WUA1340.DeviceDesc%	    = WUA1340.ndi,          USB\VID_07D1&PID_3C04
%DWA110.DeviceDesc%	    = DWA110.ndi,          USB\VID_07D1&PID_3C07

[D-Link.NTX86]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%D-Link.DeviceDesc%         = D-Link.ndi,           USB\VID_07D1&PID_3C03
%WUA1340.DeviceDesc%	    = WUA1340.ndi,          USB\VID_07D1&PID_3C04
%DWA110.DeviceDesc%	    = DWA110.ndi,          USB\VID_07D1&PID_3C07

[D-Link.NTAMD64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%D-Link.DeviceDesc%         = D-Link.ndi,           USB\VID_07D1&PID_3C03
%WUA1340.DeviceDesc%	    = WUA1340.ndi,          USB\VID_07D1&PID_3C04
%DWA110.DeviceDesc%	    = DWA110.ndi,          USB\VID_07D1&PID_3C07

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[D-Link.ndi]
AddReg                  = DRT71W9x.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[WUA1340.ndi]
AddReg                  = WUA13409x.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[DWA110.ndi]
AddReg                  = DWA110.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[D-Link.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles


[WUA1340.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[DWA110.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

; NT services sections
[D-Link.ndi.NT.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[WUA1340.ndi.NT.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[DWA110.ndi.NT.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog


;*******************************************************************************************
; NTAMD64 specific entries
;*******************************************************************************************

[D-Link.ndi.NTAMD64]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NTAMD64.CopyFiles

[WUA1340.ndi.NTAMD64]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NTAMD64.CopyFiles

[DWA110.ndi.NTAMD64]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NTAMD64.CopyFiles

; NT services sections
[D-Link.ndi.NTAMD64.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[WUA1340.ndi.NTAMD64.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[DWA110.ndi.NTAMD64.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "1"   ; 0=disable(default), 1=enable

;
; Country Region G Band
;
;HKR, ,                                 CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region 11G"
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, "(Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    1,                  0, "(Channel 1 - 13)"
;HKR, NDI\params\CountryRegion\enum,    2,                  0, "(Channel 10 - 11)"
;HKR, NDI\params\CountryRegion\enum,    3,                  0, "(Channel 10 - 13)"
;HKR, NDI\params\CountryRegion\enum,    4,                  0, "(Channel 14)"
;HKR, NDI\params\CountryRegion\enum,    5,                  0, "(Channel 1 - 14)"
;HKR, NDI\params\CountryRegion\enum,    6,                  0, "(Channel 3 - 9)"

;
; Country Region A Band
;
;HKR, ,                                 CountryRegionABand, 0, "7"
;HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, "Country Region 11A"
;HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
;HKR, NDI\params\CountryRegionABand,    default,            0, "7"
;HKR, NDI\params\CountryRegionABand\enum,0,                 0, "Ch(36 - 64,149 - 165)"
;HKR, NDI\params\CountryRegionABand\enum,1,                 0, "Ch(36 - 140)"
;HKR, NDI\params\CountryRegionABand\enum,2,                 0, "Ch(36 - 64)"
;HKR, NDI\params\CountryRegionABand\enum,3,                 0, "Ch(52 - 64,149 - 161)"
;HKR, NDI\params\CountryRegionABand\enum,4,                 0, "Ch(149 - 165)"
;HKR, NDI\params\CountryRegionABand\enum,5,                 0, "Ch(149 - 161)"
;HKR, NDI\params\CountryRegionABand\enum,6,                 0, "Ch(36 - 48)"
;HKR, NDI\params\CountryRegionABand\enum,7,                 0, "Ch(36 - 165)"
;HKR, NDI\params\CountryRegionABand\enum,8,                 0, "Ch(52 - 64)"
;HKR, NDI\params\CountryRegionABand\enum,9,                 0, "Ch(34 - 46)"
;HKR, NDI\params\CountryRegionABand\enum,10,                0, "Ch(34 - 64)"

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "3"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "1"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "0"
HKR, ,                                  AdhocOfdm, 0, "0"
HKR, NDI\params\AdhocOfdm,              ParamDesc, 0, "Adhoc Wireless Mode"
HKR, NDI\params\AdhocOfdm,              type,      0, "enum"
HKR, NDI\params\AdhocOfdm,              default,   0, "1"
HKR, NDI\params\AdhocOfdm\enum,         0,         0, "802.11 B Only"
HKR, NDI\params\AdhocOfdm\enum,         1,         0, "802.11 B/G Mix"
HKR, NDI\params\AdhocOfdm\enum,         2,         0, "802.11 G Only"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"
HKR, NDI\params\BGProtection,           ParamDesc, 0, "B/G Protection"
HKR, NDI\params\BGProtection,           type,      0, "enum"
HKR, NDI\params\BGProtection,           default,   0, "0"
HKR, NDI\params\BGProtection\enum,      0,         0, "Auto"
HKR, NDI\params\BGProtection\enum,      1,         0, "On"
HKR, NDI\params\BGProtection\enum,      2,         0, "Off"

;
; FrameAggregation
;
HKR, ,                            FrameAggregation,0, "1"
HKR, NDI\params\FrameAggregation,       ParamDesc, 0, "Frame Aggregation"
HKR, NDI\params\FrameAggregation,       type,      0, "enum"
HKR, NDI\params\FrameAggregation,       default,   0, "1"
HKR, NDI\params\FrameAggregation\enum,  0,         0, "Disable"
HKR, NDI\params\FrameAggregation\enum,  1,         0, "Enable"

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
;HKR, NDI\params\IEEE80211H,       ParamDesc,       0, "IEEE802.11h"
;HKR, NDI\params\IEEE80211H,       type,            0, "enum"
;HKR, NDI\params\IEEE80211H,       default,         0, "0"
;HKR, NDI\params\IEEE80211H\enum,  0,               0, "Disable"
;HKR, NDI\params\IEEE80211H\enum,  1,               0, "Enable"

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"
;HKR, NDI\params\AutoChannelSelect,       ParamDesc,0, "Auto Channel Select"
;HKR, NDI\params\AutoChannelSelect,       type,     0, "enum"
;HKR, NDI\params\AutoChannelSelect,       default,  0, "0"
;HKR, NDI\params\AutoChannelSelect\enum,  0,        0, "Disable"
;HKR, NDI\params\AutoChannelSelect\enum,  1,        0, "Enable"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, "WMM Capable"
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "1"
HKR, NDI\params\WMMCapable\enum,        0,         0, "Disable"
HKR, NDI\params\WMMCapable\enum,        1,         0, "Enable"

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "1"
HKR, NDI\params\APSDCapable,            ParamDesc, 0, "APSD Capable"
HKR, NDI\params\APSDCapable,            type,      0, "enum"
HKR, NDI\params\APSDCapable,            default,   0, "1"
HKR, NDI\params\APSDCapable\enum,       0,         0, "Disable"
HKR, NDI\params\APSDCapable\enum,       1,         0, "Enable"

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "1"
HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, "AC_BE support APSD"
HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
HKR, NDI\params\APSDAC_BE,              default,   0, "1"
HKR, NDI\params\APSDAC_BE\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BE\enum,         1,         0, "Enable"

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "1"
HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, "AC_BK support APSD"
HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
HKR, NDI\params\APSDAC_BK,              default,   0, "1"
HKR, NDI\params\APSDAC_BK\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BK\enum,         1,         0, "Enable"

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "1"
HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, "AC_VI support APSD"
HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
HKR, NDI\params\APSDAC_VI,              default,   0, "1"
HKR, NDI\params\APSDAC_VI\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VI\enum,         1,         0, "Enable"

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "1"
HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, "AC_VO support APSD"
HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
HKR, NDI\params\APSDAC_VO,              default,   0, "1"
HKR, NDI\params\APSDAC_VO\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VO\enum,         1,         0, "Enable"

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
HKR, Default,                     MaxSPLength,     0, "0"
HKR, NDI\params\MaxSPLength,      ParamDesc,       0, "Max Service Period Length"
HKR, NDI\params\MaxSPLength,      type,            0, "int"
HKR, Ndi\params\MaxSPLength,      default,         0, "0"
HKR, NDI\params\MaxSPLength,      min,             0, "0"
HKR, NDI\params\MaxSPLength,      max,             0, "3"
HKR, NDI\params\MaxSPLength,      step,            0, "1"
HKR, NDI\params\MaxSPLength,      optional,        0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "1"
HKR, NDI\params\DLSCapable,             ParamDesc, 0, "DLS Capable"
HKR, NDI\params\DLSCapable,             type,      0, "enum"
HKR, NDI\params\DLSCapable,             default,   0, "1"
HKR, NDI\params\DLSCapable\enum,        0,         0, "Disable"
HKR, NDI\params\DLSCapable\enum,        1,         0, "Enable"

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "1"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "1"
HKR, NDI\params\PSPXlink\enum,    0,               0, "Disable"
HKR, NDI\params\PSPXlink\enum,    1,               0, "Enable"

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600
;
; Aggressive Roaming
;
;
; Aggressive Roaming
;
HKR, ,                                 CCX2Control,     0x00010001, 0x00fa4600
HKR, ,                                 FstRoam,     0, "0"
HKR, NDI\params\FstRoam,         ParamDesc,          0, "Aggressive Roaming Condition"
HKR, NDI\params\FstRoam,         type,               0, "enum"
HKR, NDI\params\FstRoam,         default,            0, "Disabled"
HKR, NDI\params\FstRoam\enum,     0,                  0, "Disabled"
HKR, NDI\params\FstRoam\enum,     1,                  0, "-60dbm"
HKR, NDI\params\FstRoam\enum,     2,                  0, "-70dbm"
HKR, NDI\params\FstRoam\enum,     3,                  0, "-80dbm"
HKR, NDI\params\FstRoam\enum,     4,                  0, "-90dbm"

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%


;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "32"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "32"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

;*******************************************************************************************
; DeviceID for Win9X 
;*******************************************************************************************
[DRT71W9x.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_07D1&PID_3C03"

[WUA13409x.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_07D1&PID_3C04"

[DWA110.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_07D1&PID_3C07"

[USB9X.ndi.reg]
HKR, ,                            NTMPDriver,       0, Dr71WU98.sys

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "Dr71WU98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "Dr71WU98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
win9x.CopyFiles         = 11    ; system32 subdirectory on win9x
NTAMD64.CopyFiles   = 12  ; system32\drivers

[NT.CopyFiles]
Dr71WU.sys                   ; NT Installation

[win9x.CopyFiles]
Dr71WU98.sys                     ;  Win9x Installation

[NTAMD64.CopyFiles]
Dr71WU.sys                   ; NT Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
Dr71WU.sys                = 1
Dr71WU98.sys             = 1

[SourceDisksFiles.X86]  
Dr71WU.sys                = 1
Dr71WU98.sys             = 1
 
[SourceDisksFiles.AMD64]
Dr71WU.sys           = 1
Dr71WU98.sys        = 1

 
;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt73"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[D-Link.Service]
DisplayName                 = %D-Link.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\Dr71WU.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\Dr71WU.sys"
HKR, , TypesSupported,   0x00010001, 7



;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "D-Link"
D-Link                      = "D-Link"
D-Link.DeviceDesc           = "D-Link AirPlus G DWL-G122 Wireless USB Adapter(rev.C)"
WUA1340.DeviceDesc          = "D-Link WUA-1340 USB Adapter"
DWA110.DeviceDesc           = "D-Link Wireless G DWA-110 USB Adapter"
INSTALL_DISK_STR            = "D-Link USB Wireless Card Installation Disk"
D-Link.Service.DispName     = "D-Link USB Wireless LAN Card Driver"
;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR                = "dlink"
VENDOR_DESC_DEF_STR         = "D-Link USB Wireless LAN Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "6"

