;***********************************************************************
;
; smc2802wnic.inf
;
;   This installation script supports Windows 98,Me,2000,XP for the
;   SMC 2802 Wireless LAN Adapters.
;
;   Copyright (c) 2003 SMC Networks, Inc.
;   All Rights Reserved.
;
;***********************************************************************

[Version]
 DriverVer = 06/16/2003, 1.0.17
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %DCB_DESC_STR%     = PRISM_DCB1,        PCI\VEN_1260&DEV_3890&SUBSYS_280210B8
 
;==========================================
[PRISM_DCB1]       ; Win9x
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_FWDCB.copy, PRISM_APPLET.copy, PRISM_NDI.copy, PRISM_DOM.copy

[PRISM_DCB1.ME]    ; WinMe
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_FWDCB.copy.ME, PRISM_APPLET.copy.ME, PRISM_DOM.copy, PRISM_NDI.copy.ME,

[PRISM_DCB1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PS_MODE.reg, COMMON_AMAC.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_FWDCB.copy.ME, PRISM_APPLET.copy.ME, PRISM_DOM.copy, PRISM_NDI.copy.ME

[PRISM_DCB1.NT]    ; Win2k
 DelReg         = COMMON_AMAC_DEL.reg
 AddReg         = PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_FWDCB.copy.NT, PRISM_APPLET.copy.NT, PRISM_DOM.copy
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[PRISM_DCB1.NT.Services]
 AddService     = "PRISM_ICB", 2, PRISM_DRIVER_DCB.Service, PRISM_DRIVER.EventLog

[PRISM_DCB1.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_DCB1.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_280210B8"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR%
 HKR,,FWFileName,0,"smc2802w.arm"

;###############################################################################

[PRISM_COINSTALL.reg.NT]
; HKR,           ,CoInstallers32         ,0x00010000     ,"Coexe.dll,CoTest"
[PRISM_DRIVER_DCB.Service]
 DisplayName    = %PRISM_SERVICE_DISPLAY_DCB%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\smc2802w.sys
 LoadOrderGroup = NDIS
 
[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################
[COMMON_ICB.reg]
 HKR,NDI                ,Service                ,0      ,"smc2802_ICB"
 ;HKR,NDI                ,CardType               ,0      ,"PCI"
 HKR,                   ,BusType                ,0      ,"5"
 HKR,                   ,DeviceVxDs             ,0      ,"smc2802w.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00
[COMMON_NDIS.reg]
 ;;HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"smc2802"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.ME]
 ;;HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"smc2802"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.NT]
 ;;HKR,                   ,EnumPropPages32        ,0      ,"PRISMCFG.cpl,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,WLANIOC         ,0      ,"XG-300"
 ;;HKR,                   ,PRISMIOC         ,0      ,"1"
 HKR,                   ,Band				    ,0      ,"1"
 ;;HKR,                   ,RegulatorDomain		,0      ,"16"
;Uncomment the line above to install without user interface prompts

 HKR,,SSID,0,"ANY"
 HKR,defaults,SSID,0,"ANY"
 HKR,NDI\params\SSID,ParamDesc,0,%ESSID_STR%
 HKR,NDI\params\SSID,default,0,"ANY"
 HKR,Ndi\params\SSID,type,0,"edit"
 HKR,NDI\params\SSID,limitText,0,"32"

 HKR,,NetworkType,0,1
 HKR,defaults,NetworkType,0,1
 HKR,NDI\params\NetworkType,ParamDesc,0,%Network_Type_STR%
 HKR,Ndi\params\NetworkType,default,0,"1"
 HKR,NDI\params\NetworkType,type,0,"enum"
 HKR,NDI\params\NetworkType\enum,0,0,"Ad Hoc"
 HKR,NDI\params\NetworkType\enum,1,0,"Infrastructure"

 HKR,,DSChannel,0,1
 HKR,defaults,DSChannel,0,1
 HKR,NDI\params\DSChannel,ParamDesc,0,%CHANNEL_STR%
 HKR,Ndi\params\DSChannel,default,0,"1"
 HKR,NDI\params\DSChannel,type,0,"enum"
 HKR,NDI\params\DSChannel\enum,1,0,"01"
 HKR,NDI\params\DSChannel\enum,2,0,"02"
 HKR,NDI\params\DSChannel\enum,3,0,"03"
 HKR,NDI\params\DSChannel\enum,4,0,"04"
 HKR,NDI\params\DSChannel\enum,5,0,"05"
 HKR,NDI\params\DSChannel\enum,6,0,"06"
 HKR,NDI\params\DSChannel\enum,7,0,"07"
 HKR,NDI\params\DSChannel\enum,8,0,"08"
 HKR,NDI\params\DSChannel\enum,9,0,"09"
 HKR,NDI\params\DSChannel\enum,10,0,"10"
 HKR,NDI\params\DSChannel\enum,11,0,"11"

 HKR,,TxRate,,15
 HKR,defaults,TxRate,,15
 HKR,NDI\params\TxRate,ParamDesc,0,%TX_RATE_STR%
 HKR,NDI\params\TxRate,default,0,"15"
 HKR,NDI\params\TxRate,type,0,"enum"
 HKR,NDI\params\TxRate\enum,1,0,"1 Mbps"
 HKR,NDI\params\TxRate\enum,2,0,"2 Mbps"
 HKR,NDI\params\TxRate\enum,3,0,"1 or 2 Mbps"
 HKR,NDI\params\TxRate\enum,4,0,"5.5 Mbps"
 HKR,NDI\params\TxRate\enum,8,0,"11 Mbps"
 HKR,NDI\params\TxRate\enum,15,0,"Fully Auto" 

 HKR,,WepReq,0,0
 HKR,defaults,WepReq,0,0
 HKR,NDI\params\WepReq,ParamDesc,0,%WEP_STR%
 HKR,Ndi\params\WepReq,default,0,"0"
 HKR,NDI\params\WepReq,type,0,"enum"
 HKR,NDI\params\WepReq\enum,0,0,"Disable"
 HKR,NDI\params\WepReq\enum,2,0,"64-bit"
 HKR,NDI\params\WepReq\enum,6,0,"128-bit"
 HKR,NDI\params\WepReq,optional,0,"0"

 HKR,NDI\params\RTSThresh,,0,2347
 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,step,0,1
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,NDI\params\FragThresh,,0,2346
 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2
 HKR,NDI\params\FragThresh,optional,0,1
  
 HKR,         ,LongPreamble,0,0
 HKR, defaults,LongPreamble,0,0   ;Infrasturcture
 HKR, NDI\params\LongPreamble,,0,0
 HKR, Ndi\params\LongPreamble,default,0,0 
 HKR, Ndi\params\LongPreamble,ParamDesc,0, %SHORT_PREAM_STR%
 HKR, Ndi\params\LongPreamble,type,0, "enum"
 HKR, Ndi\params\LongPreamble,default,0, "1"
 HKR, Ndi\params\LongPreamble\enum,1,0, "Long"
 HKR, Ndi\params\LongPreamble\enum,0,0, "Short"
 HKR, NDI\params\LongPreamble,optional,0,1  
 
;11d Mode.
 HKR,         ,11dMode,0,0
 HKR, defaults,11dMode,0,0   ;Disalbed
 HKR, NDI\params\11dMode,,0,0
 HKR, Ndi\params\11dMode,default,0,0 
 HKR, Ndi\params\11dMode,ParamDesc,0, %11D_MODE%
 HKR, Ndi\params\11dMode,type,0, "enum"
 HKR, Ndi\params\11dMode,default,0, "0"
 HKR, Ndi\params\11dMode\enum,0,0, "Disabled"
 HKR, Ndi\params\11dMode\enum,1,0, "Strict"
 HKR, Ndi\params\11dMode\enum,2,0, "Flexible"
 HKR, NDI\params\11dMode,optional,0,1
 
 ;Nitro Mode
 HKR,		,NitroMode,0,1
; HKR,defaults,NitroMode,0,1
; HKR,NDI\params\NitroMode,,0,1
; HKR,NDI\params\NitroMode,default,0,1
; HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
; HKR,NDI\params\NitroMode,type,0,int
; HKR,NDI\params\NitroMode,min,0,0
; HKR,NDI\params\NitroMode,max,0,1
; HKR,NDI\params\NitroMode,step,0,1
; HKR,NDI\params\NitroMode,optional,0,1
 
 ;NitroTime
 
 HKR,		,NitroTime,0,0
; HKR,defaults,NitroTime,0,0
; HKR,NDI\params\NitroTime,,0,0
; HKR,NDI\params\NitroTime,default,0,0
; HKR,NDI\params\NitroTime,ParamDesc,,"NitroTime"
; HKR,NDI\params\NitroTime,type,0,int
; HKR,NDI\params\NitroTime,min,0,0
; HKR,NDI\params\NitroTime,max,0,5000
; HKR,NDI\params\NitroTime,step,0,10
; HKR,NDI\params\NitroTime,optional,0,1

[COMMON_AMAC_DEL.reg]
 HKR,defaults,DataRates
 HKR,NDI\params\DataRates
 HKR,NDI\params\DataRate
 HKR,DSChannel
 HKR,defaults,DSChannel
 HKR,NDI\params\DSChannel

[COMMON_AMAC.reg]
 HKR,NDI\params\ShortRetryLimit,,0,7
 HKR,NDI\params\ShortRetryLimit,default,0,7
 HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
 HKR,NDI\params\ShortRetryLimit,type,,int
 HKR,NDI\params\ShortRetryLimit,min,0,1
 HKR,NDI\params\ShortRetryLimit,max,0,255
 HKR,NDI\params\ShortRetryLimit,step,0,1
 HKR,NDI\params\ShortRetryLimit,optional,0,1

 HKR,NDI\params\LongRetryLimit,,0,4
 HKR,NDI\params\LongRetryLimit,default,0,4
 HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
 HKR,NDI\params\LongRetryLimit,type,0,int
 HKR,NDI\params\LongRetryLimit,min,0,1
 HKR,NDI\params\LongRetryLimit,max,0,255
 HKR,NDI\params\LongRetryLimit,step,0,1
 HKR,NDI\params\LongRetryLimit,optional,0,1

[COMMON_PSMODE.reg]
 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1

[COMMON_PS_MODE_XP.reg]
 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode\enum,4,,%POWER_SAVE_AUTO_DYN_STR%
 HKR,NDI\params\PSMode\enum,5,,%POWER_SAVE_AUTO_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1
 
;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers
 PRISM_FWDCB.copy      	= 11 ; Win9x=%windir%\system
 PRISM_FWDCB.copy.ME   	= 11 ; Win9x=%windir%\system
 PRISM_FWDCB.copy.NT  	= 12 ; Win2k=%windir%\system32\drivers
 PRISM_DOM.copy		= 10 ; %windir% all OS

[PRISM_NDI.copy]

[PRISM_NDI.copy.ME]

[PRISM_COINSTALL.copy.NT]
;Coexe.dll
;ChangeDomain.exe
[PRISM_DRIVER.copy]
 smc2802w.sys
 ;;PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.ME]
 smc2802w.sys
 ;;PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.NT]
 smc2802w.sys

[PRISM_FWDCB.copy]
 smc2802w.arm

[PRISM_FWDCB.copy.ME]
 smc2802w.arm

[PRISM_FWDCB.copy.NT]
 smc2802w.arm

[PRISM_APPLET.copy]

[PRISM_APPLET.copy.ME]

[PRISM_APPLET.copy.NT]

[PRISM_DOM.copy]
 smc2802w.ini

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 ;;PRISMIOC.vxd           = 1,win9x
 smc2802w.sys           = 1
 smc2802w.arm           = 1
 smc2802w.ini           = 1
; Coexe.dll				= 1
; ChangeDomain.exe		= 1

[SourceDisksFiles.ME]   ; WinMe
 ;;PRISMIOC.vxd           = 1,win9x
 smc2802w.sys           = 1
 smc2802w.arm           = 1
 smc2802w.ini           = 1
; Coexe.dll				= 1
; ChangeDomain.exe		= 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 smc2802w.sys           = 1
 smc2802w.arm           = 1
 smc2802w.ini           = 1
; Coexe.dll				= 1
; ChangeDomain.exe		= 1

;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = "SMC"
 VER_VENDOR_NAME_STR    = "SMC Networks, Inc."

 PRISM_SERVICE_DISPLAY_DCB = "SMC2802W 2.4GHz 54Mbps Wireless PCI Card"
 
 INSTALL_DISK_STR       = "SMC Wireless LAN Install Disk"

 ESSID_STR               = "ESSID"
 NETWORK_TYPE_STR        = "Network Type"
 CHANNEL_STR		 = "Channel"
 TX_RATE_STR		 = "Transmit Rate"
 WEP_STR                 = "Use WEP"
 ADHOC_DEMO_STR          = "Adhoc Demo Mode"
 SHORT_PREAM_STR         = "Preamble Mode"
 RTSTHRESH_STR           = "RTS Threshold"
 FRAGTHRESH_STR          = "Fragmentation Threshold"
 AUTHENT_TYPE_STR        = "Authentication Algorithm"
 LISTENINTERVAL_STR      = "Listen Interval"
 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic"
 POWER_SAVE_MAX_STR      = "Maximum"
 POWER_SAVE_AUTO_DYN_STR = "Auto Dynamic"
 POWER_SAVE_AUTO_MAX_STR = "Auto Maximum"
 LOAD_FIRMWARE_STR       = "Firmware Download"
 SHORT_RETRY_STR         = "Short Retry Limit"
 LONG_RETRY_STR          = "Long Retry Limit"
 CHANNEL_STR             = "Channel"
 DATARATES_STR           = "Data Rate"
 DATARATES_AUTO          = "Fully Automatic"
 ALSR_STR                = "Auto Long Slot Reassociation"
 11D_MODE				 = "11D Mode"	
 NITRO_MODE              = "Nitro Mode" 

 DCB_DESC_STR            = "SMC2802W 2.4GHz 54Mbps Wireless PCI Card"

