;/*++
;
;Module Name:
;
;    netathuw.inf
;
;Abstract:
;    Installs athuw.sys (NDIS 5/5.1 driver) on NT platforms (2000, XP and greater)
;    Installs athuwx.sys (NDIS 5 driver) on 9x platforms
;
;--*/

[Version]
Signature   = "$CHICAGO$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
Compatible  = 1
DriverVer   = 01/04/2010,7.7.0.75
Catalogfile.nt = netathuw.cat

[Manufacturer]
%ATHEROS%     = Atheros, NTamd64.5.1, NTX86.6.0, NTamd64.6.0, NTX86.6.1

[ControlFlags]
ExcludeFromSelect = *

[Atheros]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
; Atheros
%ATHER.DeviceDesc.9271% = ATHER_DEV_9271.ndi,     USB\VID_0CF3&PID_9271
%ATHER.DeviceDesc.1006% = ATHER_DEV_1006.ndi,     USB\VID_0CF3&PID_1006
[Atheros.NTamd64.5.1]
;------------------------------------------------------------------------------------
[Atheros.NTX86.6.0]
;------------------------------------------------------------------------------------
[Atheros.NTamd64.6.0]
;------------------------------------------------------------------------------------
[Atheros.NTX86.6.1]
;------------------------------------------------------------------------------------

; Windows NT specific entries
[ATHER_DEV_9271.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_9271.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7010.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgnub.reg, uapsd.reg, 7010.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7010.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7015.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg, 7010.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7015.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1006.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, customer1.SCAN.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1006.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog
;===========================CUSTOM SECTION=====================================
; Windows NT specific entries
[NTGR_DEV_9030.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, NTGR.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[NTGR_DEV_9030.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog

[DLINK_DEV_3A10.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 15
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, DLINK.reg, htDisableWepTkip.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[DLINK_DEV_3A10.ndi.NT.Services]
AddService      = AR9271, 2, ATHER.Service, common.EventLog


;===========================CUSTOM SECTION=====================================
;
; 5416 Enumerated Types
;

[5416.bgub.reg]
HKR, ,                                  NetBand,                        0x00002,  "12"
HKR, ,                                  wModeSelect,                    0x00002,  "40972"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"

[5416.bgnub.reg]
HKR, ,                                  NetBand,                        0x00002,  "40972"
HKR, ,                                  wModeSelect,                    0x00002,  "40972"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "1024"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"

[5416.abgnub.reg]
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "61455"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
;HKR, Ndi\params\NetBand\enum,           "61455",                        0,  %WirelessModeAuto%
;HKR, Ndi\params\NetBand\enum,           "20481",                        0,  %WirelessMode5GHzOnly%
HKR, Ndi\params\NetBand\enum,           "40972",                        0,  %WirelessMode2GHzOnly%

[5416.antennacontrols.reg] 
HKR, ,                                  rxChainSelect,                 	0x00002,  "7"
;HKR, ,                                  txChainSelectLegacy,            0x00002,  "5"
HKR, ,                                  rxChainSelectLegacy,           	0x00002,  "7"
HKR, ,                                  forceBias,           	        0x00002,  "2"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

[pushbutton.reg]
HKR, ,                                  wpsButtonGpio,                  0x00002,  "9"

[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1823"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
;HKR, Ndi\params\NetBand\enum,           "1823",                         0,        %WirelessModeAuto%
;HKR, Ndi\params\NetBand\enum,           "1795",                         0,        %WirelessMode5GHzOnly%
HKR, Ndi\params\NetBand\enum,           "28",                           0,        %WirelessMode2GHzOnly%

[pcibusconfig.reg]
HKR, ,                                  BusConfig,                 	0x00002,  "0"

[d3hot.reg]
HKR, ,                                  pciePowerReset,                 0x00002,  "0"
HKR, ,                                  pcieRestore,                 	0x00002,  "1"

[expresscardaspmoff.reg]
HKR, ,                                  pciDetectEnable,                0x00002,  "2"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[gpioled.reg]
HKR,,                                   linkLEDFunc,                    0,        "49"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

; Allow non admin uses to switch profiles
;[5211.reg.security]
;"D:ARAI(A;;GA;;;BA)(A;;GA;;;SY)(A;CI;GA;;;IU)"

[uapsd.reg]
HKR, Ndi\params\uapsdEnabledBE,            ParamDesc,                      0,  %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBE,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBE,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBE\enum,       "1",                            0,  %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum,       "0",                            0,  %uapsdEnabledBEOff%

HKR, Ndi\params\uapsdEnabledBK,            ParamDesc,                      0,  %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBK,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBK,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBK\enum,       "1",                            0,  %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum,       "0",                            0,  %uapsdEnabledBKOff%

HKR, Ndi\params\uapsdEnabledVI,            ParamDesc,                      0,  %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVI,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVI,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVI\enum,       "1",                            0,  %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum,       "0",                            0,  %uapsdEnabledVIOff%

HKR, Ndi\params\uapsdEnabledVO,            ParamDesc,                      0,  %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVO,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVO,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVO\enum,       "1",                            0,  %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum,       "0",                            0,  %uapsdEnabledVOOff%

HKR, Ndi\params\psPollEnable,            ParamDesc,                      0,  %psPoll%
HKR, Ndi\params\psPollEnable,            Base,                           0,  "10"
HKR, Ndi\params\psPollEnable,            default,                        0,  "0"
HKR, Ndi\params\psPollEnable,            type,                           0,  "enum"
HKR, Ndi\params\psPollEnable\enum,       "1",                            0,  %psPollEnable%
HKR, Ndi\params\psPollEnable\enum,       "0",                            0,  %psPollDisable%

;-----------------------------------------------------------------------------
;
; 5416 common
;
[5416.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,pcieClockReq
HKR,,rmEnable
HKR,,overrideACstatus
HKR, Ndi\params\NetBand
HKR,,rxChainSelect
HKR,,txChainSelectLegacy
HKR,,rxChainSelectLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR,,pciePowerSaveEnable
HKR,,pcieAspm

[5416.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "0"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, Ndi\params\PSPXLinkMode,           ParamDesc,                      0,  %PSPXLinkMode%
HKR, Ndi\params\PSPXLinkMode,           Base,                           0,  "10"
HKR, Ndi\params\PSPXLinkMode,           default,                        0,  "0"
HKR, Ndi\params\PSPXLinkMode,           type,                           0,  "enum"
HKR, Ndi\params\PSPXLinkMode\enum,      "1",                            0,  %PSPXLinkModeEnable%
HKR, Ndi\params\PSPXLinkMode\enum,      "0",                            0,  %PSPXLinkModeDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

[7010.reg]
HKR, ,                                  forceNormalSlotMrvl,             0x00002,  "1"
HKR, ,                                  htAdhocEnable,                   0x00002,  "0"
HKR, ,                                  isMagpie,                        0x00002, "1"
HKR, ,                                  gpioLedCustom,                   0x00002, "1"
HKR, ,                                  gpioPinFunc0,                    0x00002, "12"
HKR, ,                                  gpioPinFunc1,                    0x00002, "10"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program,  USBVIDPID,  0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%"

[htDisableWepTkip.reg]
HKR, ,                                  htEnableWepTkip,                 0x00002, "0"

[NTGR.reg]
HKR, ,                                  ignore11dBeacon,                0, 1
HKR, ,                                  gpioLedCustom,                  0, 8
HKR, ,                                  gpioPinFunc0,                   0, 15
HKR, ,                                  swapDefaultLED,                 0, 1
HKR, ,                                  GreenTx,                        0, 15
HKR, ,                                  htEnableWepTkip,          0x00002, "3"
HKR, ,                                  htEnableWepTkipAgg,       0x00002, "0"

[DLINK.reg]
HKR, , gpioLedCustom,   0, 1
HKR, , gpioPinFunc0,    0, 15
HKR, , swapDefaultLED,  0, 1
;-----------------------------------------------------------------------------
;;Customized Section

[customer0.reg]
;PCIe Related
HKR, ,                                  pcieAspm,                 	0x00002,  "2"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  forceWake,                 	0x00002,  "0"
HKR, ,                                  antennaSwitchSwap,              0x00002,  "1"
;LED Related
HKR, ,                                  gpioPinFunc1,                  0x00002,  "1"
;General Customer0
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	%Mode11d%
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		%Mode11dEnable%
HKR,NDI\params\ignore11dBeacon\enum,1,,		%Mode11dDisable%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,           	step,                           0,  "1"
HKR, Ndi\params\roamRssiA,           	base,                           0,  "10"
HKR, Ndi\params\roamRssiA,           	type,                           0,  "int"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR,,                 isMagpie,                 0, 0
[customer0.LED.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"

[customer0.LED1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  pcieClockReq,                   0x00002,  "0"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "2"

[customer1.SCAN.reg]
HKR, ,                                  bkPeriodicScanEnable,           0x00002,  "0"
HKR, ,                                  scanPendingCriterion,           0x00002,  "65"

[customer11_11nwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "49719"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "32772",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "16387",                        0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "32796",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "49719",                        0,        %wModeSelect11abgn%

[customer11_legacywmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "2075"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "3",                            0,        %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum,       "28",                           0,        %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum,       "2075",                         0,        %wModeLegacy11abg%

[customer11Ant.reg]
HKR, Ndi\params\antennaSwitch,          ParamDesc,                      0,        %antennaSwitch%
HKR, Ndi\params\antennaSwitch,          Base,                           0,        "10"
HKR, Ndi\params\antennaSwitch,          default,                        0,        "0"
HKR, Ndi\params\antennaSwitch,          type,                           0,        "enum"
HKR, Ndi\params\antennaSwitch\enum,     "1",                            0,        %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum,     "2",                            0,        %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum,     "0",                            0,        %antennaSwitchAuto%

[rssiAdjust.reg]
HKR, ,                                  rssiAdjust,                     0x00002,  "7"

[cmdRegister.reg]
HKR, ,                                  cmdRegister,                    0x00002,  "838"

;-----------------------------------------------------------------------------
; ATHER NT specific
;

[ATHER.reg]
HKR, Ndi,             Service,      0, "AR9271"
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet"

[ATHER.Service]
DisplayName     = %ATHER.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\athuw.sys
LoadOrderGroup  = NDIS

;-----------------------------------------------------------------------------
; ATHER NT/XP common
;
[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, ,                  EventMessageFile,   0x00020000,   "%%SystemRoot%%\System32\netevent.dll"
HKR, ,                  TypesSupported,     0x00010001,   7

;----------------------------------------------------------------------------
; System TCPIP parameter changes
;
[sys.TcpParams.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000003
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000

[sys.TcpParamslan.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000001
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000

;----------------------------------------------------------------------------
;*********************************************************************
;   Atheros Client Installation Program
;*********************************************************************
[ATHR_9271.reg]
HKR, ,                                  forceNormalSlotMrvl,             0x00002,  "1"
HKR, ,                                  htAdhocEnable,                   0x00002,  "0"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program,  USBVIDPID,  0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%"

;----------------------------------------------------------------------------
; NT Files to Copy
[ATHER.CopyFiles.nt]
athuw.sys,,,2

[ATHER.DelIniFiles]
Athnic.ini,,,1

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %Atheros_Disk%,,,

;----------------------------------------------------------------------------
; Source Files
[SourceDisksFiles]
athuw.sys                   = 1,, ; on distribution disk 1


[DestinationDirs]
ATHER.CopyFiles.nt           = 12
;ATHER.win.CopyFiles          = 10,system32\drivers ; %SystemRoot%\system32\drivers
ATHER.DelIniFiles            = 10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir               = 11

[DEFAULTDESTDIRS]
;


[Strings]
Atheros                      = "TP-LINK"
MapRegisters                 = "Map Registers"
NetworkAddress               = "Network Address"
sleepMode                    = "Power Save Mode"
scanTimeValid                = "Scan Valid Interval"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
sleepModeOff                 = "Off"
sleepModeNormal              = "Normal"
sleepModeMax                 = "Maximum"
tpc                          = "Transmit Power"
tpcLowest                    = "Lowest"
tpc12                        = "12.5%"
tpc25                        = "25%"
tpc50                        = "50%"
tpc100                       = "100%"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
WirelessMode                 = "Wireless Mode Selection"
WirelessModeAuto             = "Auto"
WirelessMode5GHzOnly         = "5 GHz Only"
WirelessMode2GHzOnly         = "2.4 GHz Only"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
roamPolicy                   = "Roaming Policy"
roamPolicyVeryLow            = "Very Low"
roamPolicyLow                = "Low"
roamPolicyNormal             = "Normal"
roamPolicyHigh               = "High"
roamPolicyVeryHigh           = "Very High"
scanTimeValidcust            = "Roam Time (sec)"
scanTimeValidcust120         = "120"
scanTimeValidcust60          = "60"
scanTimeValidcust45          = "45"
scanTimeValidcust30          = "30"
scanTimeValidcust20          = "20"
scanTimeValidcust10          = "10"
scanTimeValidcust5           = "5"
sleepMode_DEFAULT            = "2"  
NetBand_DEF_STR_A            = "3"                       ; (A/T) 
NetBand_DEF_STR_AB           = "7"                       ; (A/T/B)   
NetBand_DEF_STR_G            = "12"                      ; (B/G)     
NetBand_DEF_STR_AG           = "15"                      ; (A/T/B/G)
AdhocBand_DEF_STR_A          = "1"                       ; (A)
AdhocBand_DEF_STR_AB         = "1"                       ; (A)
AdhocBand_DEF_STR_G          = "0"                       ; (B)
AdhocBand_DEF_STR_AG         = "0"                       ; (B)
shortPreamble_DEFAULT        = "1"
authTypeUseOnly              = "802.11 Authentication Type"
authAuto                     = "Auto"
authOpen                     = "Open"
authShared                   = "Shared"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOn               = "On"
bkScanEnableOff              = "Off"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRateA                    = "roamRateA"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRateBOnly11M             = "11Mbps"
roamRateB                    = "roamRateB"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateB11M                 = "11Mbps"
pcieAspm                     = "pcieAspm"
pcieAspmOff                  = "L0s Off, L1 Off"
pcieAspmL1On                 = "L0s Off, L1 On"
wModeSelect                  = "Wireless Mode"
wModeSelect11bonly           = "11b only"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11abgn            = "11abgn"
wModeLegacy11a               = "11a only"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11abg             = "11abg"
antennaSwitch                = "AntennaSwitch"
antennaSwitchAuto            = "Auto"
antennaSwitchA               = "Antenna A"
antennaSwitchB               = "Antenna B"
uapsdEnabledBE               = "Power Save Policy (Best Effort)"
uapsdEnabledBEOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBEOff            = "Legacy Power Save"
uapsdEnabledBK               = "Power Save Policy (Background)"
uapsdEnabledBKOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBKOff            = "Legacy Power Save"
uapsdEnabledVI               = "Power Save Policy (Voice)"
uapsdEnabledVIOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVIOff            = "Legacy Power Save"
uapsdEnabledVO               = "Power Save Policy (Video)"
uapsdEnabledVOOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVOOff            = "Legacy Power Save"
psPoll                       = "Power Save Legacy Algorithm"
psPollEnable                 = "PS Poll"
psPollDisable                = "PS non Poll"
ccx5FeatureEnable            = "MFP"
ccx5FeatureEnableMfpEnable   = "Enable"
ccx5FeatureEnableMfpDisable  = "Disable"
Mode11d                      = "11d Mode Switch"
Mode11dEnable                = "Enable"
Mode11dDisable               = "Disable"
RateCtrl                     = "Auto Transmit Rate"
RateCtrlEnable               = "Enable"
RateCtrlDisable              = "Disable"
TxRate11b                    = "11b Transmit Rates"
TxRate11b1M                  = "1 Mbps"
TxRate11b2M                  = "2 Mbps"
TxRate11b5M                  = "5.5 Mbps"
TxRate11b11M                 = "11 Mbps"
TxRate11g                    = "11g Transmit Rates"
TxRate11g1M                  = "1 Mbps"
TxRate11g2M                  = "2 Mbps"
TxRate11g5M                  = "5.5 Mbps"
TxRate11g11M                 = "11 Mbps"
TxRate11g6M                  = "6 Mbps"
TxRate11g9M                  = "9 Mbps"
TxRate11g12M                 = "12 Mbps"
TxRate11g18M                 = "18 Mbps"
TxRate11g24M                 = "24 Mbps"
TxRate11g36M                 = "36 Mbps"
TxRate11g48M                 = "48 Mbps"
TxRate11g54M                 = "54 Mbps"
TxRate11a                    = "11a Transmit Rates"
TxRate11a6M                  = "6 Mbps"
TxRate11a9M                  = "9 Mbps"
TxRate11a12M                 = "12 Mbps"
TxRate11a18M                 = "18 Mbps"
TxRate11a24M                 = "24 Mbps"
TxRate11a36M                 = "36 Mbps"
TxRate11a48M                 = "48 Mbps"
TxRate11a54M                 = "54 Mbps"
ATHR_VID_0CF3                = "VID_0CF3"
NTGR_VID_0846                = "VID_0846"
PSPXLinkMode                 = "PSP XLink mode"
PSPXLinkModeEnable           = "Enable"
PSPXLinkModeDisable          = "Disable"

Atheros_Disk                 = "Driver Disk 1"
ATHER.Service.DispName       = "Wireless Network Adapter Service"
ATHER.DeviceDesc.9271        = "TP-LINK 150Mbps Wireless Lite N Adapter"
ATHER.DeviceDesc.1006        = "Wireless G USB Adapter"
