;****************************************************************
; WHQL172.INF for Windows 98/ME/2000 and XP			*
;								*
; ASIX AX88172 USB2 to Fast Ethernet Adapter			*
;								*
; Copyright 2001-2003, ASIX Electronics Corporation		*
;
; Version: 2.0.0.5
;****************************************************************

[Version]
Signature  = "$Windows NT$"
CatalogFile = ax88172xp.cat
Class      = Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider   = %ASIX%
;LayoutFile = layout.inf
DriverVer = 05/22/2003, 2.0.0.5

[Manufacturer]
%ASIX%   = USB

[ControlFlags]
ExcludeFromSelect = USB\VID_0B95&PID_1720

[USB]
%AX88172.DeviceDesc% = AX88172.Ndi,USB\VID_0B95&PID_1720

;****************************************************************
; Win98 main sections						*
;****************************************************************
[AX88172.Ndi]
AddReg   = AX88172.Reg, AX88172.Con.Reg	;, AX88172.Params
DeviceID = USB\VID_0B95&PID_1720


;****************************************************************
; NT main sections						*
;****************************************************************
[AX88172.Ndi.NT]
AddReg          = AX88172.NT.Reg, AX88172.Con.Reg	;, AX88172.Params
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15	; USB
CopyFiles       = CopyFile.NT.Sys

[AX88172.Ndi.NT.Services]
AddService = AX88172, 2, AX88172.Service, Common.EventLog


;****************************************************************
; Windows 98 section						*
;****************************************************************
[AX88172.Reg]
HKR,Ndi,DeviceID,,USB\VID_0B95&PID_1720
HKR,Ndi,CardType,,"PNP"

HKR,,AdapterName,,AX88172

HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,ax88172.sys

; NDIS Info
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,AX88172

; Interfaces
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"

; Install sections
HKR,Ndi\Install,ndis3,,"AX88172.Install"

HKR,Ndi,HelpText,,"AX88172 USB2 to Fast Ethernet Adpater"


;****************************************************************
; Driver parameters						*
;****************************************************************
;[AX88172.Params]

[AX88172.Con.Reg]
HKR,Ndi\params\ConnectionType,ParamDesc,,"Connection Type"
HKR,Ndi\params\ConnectionType,default,,0
HKR,Ndi\params\ConnectionType,type,,enum
HKR,Ndi\params\ConnectionType\enum,0,,"AutoSense"
HKR,Ndi\params\ConnectionType\enum,2,,"10BaseT Half_Duplex"
HKR,Ndi\params\ConnectionType\enum,3,,"10BaseT Full_Duplex"
HKR,Ndi\params\ConnectionType\enum,8,,"100BaseTx Half_Duplex"
HKR,Ndi\params\ConnectionType\enum,9,,"100BaseTx Full_Duplex"
HKR,NDI\params\ConnectionType,flag,1,20,00,00,00

;****************************************************************
; Install section for OSR2 and Windows 98			*
;****************************************************************

[AX88172.Install]
;CopyFiles=CopyFile.Inf,CopyFile.Sys	;Signability
CopyFiles=CopyFile.Sys

;[CopyFile.Inf]		;Signability
;AX88172.inf		;Signability

[CopyFile.Sys]
ax88172.sys


;****************************************************************
; Install section for Windows NT 5				*
;****************************************************************

[AX88172.NT.Reg]
; Interfaces
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "AX88172"

[AX88172.Service]
DisplayName    = %AX88172.DeviceDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\ax88172.sys
LoadOrderGroup = NDIS
AddReg         = TextModeFlags.Reg

[Common.EventLog]
AddReg = Common.AddEventLog.Reg

[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

[TextModeFlags.Reg]
HKR, , TextModeFlags, 0x00010001, 0x0001

[CopyFile.NT.Sys]
ax88172.sys,,,2


;**********************************************************************
; Destination directories                                             *
;**********************************************************************

[DestinationDirs]
CopyFile.Sys    = 11
;CopyFile.Inf    = 17	;Signability
CopyFile.NT.Sys = 12

[SourceDisksNames]
; Cabinet file names and associated disks
; <cab#> = <disk#>,<cabinet filename>, ID (Unused, must be 0)
50=%AX88172.DiskName%,,

[SourceDisksFiles]
;<file> = <cabinet number>,<subdir>,<filename>,<size>
;Note: File is not in a cabinet if cab# is 0
ax88172.sys=50,.,ax88172.sys,10000
;AX88172.inf=50,.,AX88172.inf,10000	;Signability


;**********************************************************************
; Localizable strings                                                 *
;**********************************************************************

[Strings]
ASIX = "ASIX"
AX88172.DiskName = "AX88172 USB2 to Fast Ethernet Driver Diskette"
AX88172.DeviceDesc = "ASIX AX88172 USB2 to Fast Ethernet Adapter"


