;****************************************************************
; NETCOKK.INF for Windows 98/ME/2000 and XP			*
;								*
; corega FEther USB2-TX				                *
;								*
; Copyright 2000-2001    corega K.K.              		*
;****************************************************************

[Version]
Signature  = "$Windows NT$"
Class      = Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider   = %USB%
;LayoutFile = layout.inf
;CatalogFile = NETCOKK.cat     ;; for WHQL certified
DriverVer   = 09/28/2002, 1.0.0.2

[Manufacturer]
%USB%   = USB

[ControlFlags]
ExcludeFromSelect = USB\VID_07AA&PID_0017

[USB]
%COUSB2T5.DeviceDesc% = COUSB2T5.Ndi,USB\VID_07AA&PID_0017

;****************************************************************
; Win98 main sections						*
;****************************************************************
[COUSB2T5.Ndi]
AddReg   = COUSB2T5.Reg, COUSB2T5.Params, COUSB2T5.Con.Reg
DeviceID = USB\VID_07AA&PID_0017


;****************************************************************
; NT main sections						*
;****************************************************************
[COUSB2T5.Ndi.NT]
AddReg          = COUSB2T5.NT.Reg, COUSB2T5.Params, COUSB2T5.Con.Reg
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 0 ; USB
CopyFiles       = CopyFile.NT.Sys

[COUSB2T5.Ndi.NT.Services]
AddService = COUSB2T5, 2, COUSB2T5.Service, Common.EventLog


;****************************************************************
; Windows 98 section						*
;****************************************************************
[COUSB2T5.Reg]
HKR,Ndi,DeviceID,,USB\VID_07AA&PID_0017
HKR,Ndi,CardType,,"PNP"

HKR,,AdapterName,,COUSB2T5

HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,COUSB2T5.SYS

; NDIS Info
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,COUSB2T5

; Interfaces
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"

; Install sections
HKR,Ndi\Install,ndis3,,"COUSB2T5.Install"

HKR,Ndi,HelpText,,"corega FEther USB2-TX"


;****************************************************************
; Driver parameters						*
;****************************************************************

[COUSB2T5.Params]
HKR, ,TxPacketDesc,    0, "20"   ; 0x32
HKR, ,RxPacketDesc,    0, "20"   ; 0x78

[COUSB2T5.Con.Reg]
HKR,Ndi\params\ConnectionType,ParamDesc,,"Connection Type"
HKR,Ndi\params\ConnectionType,default,,0
HKR,Ndi\params\ConnectionType,type,,enum
HKR,Ndi\params\ConnectionType\enum,0,,"Auto-Negotiation"
HKR,Ndi\params\ConnectionType\enum,2,,"10BaseT Half_Duplex"
HKR,Ndi\params\ConnectionType\enum,3,,"10BaseT Full_Duplex"
HKR,Ndi\params\ConnectionType\enum,8,,"100BaseTx Half_Duplex"
HKR,Ndi\params\ConnectionType\enum,9,,"100BaseTx Full_Duplex"
;HKR,Ndi\params\ConnectionType\enum,102,,"1Mbps HomePNA"
HKR,NDI\params\ConnectionType,flag,1,20,00,00,00

;HKR,Ndi\params\RemoteWakeup,ParamDesc,,"Remote Wakeup"
;HKR,Ndi\params\RemoteWakeup,default,,2
;HKR,Ndi\params\RemoteWakeup,type,,enum
;HKR,Ndi\params\RemoteWakeup\enum,0,,"Disable"
;HKR,Ndi\params\RemoteWakeup\enum,2,,"Link up"
;HKR,Ndi\params\RemoteWakeup\enum,6,,"Magic Packet"
;HKR,NDI\params\RemoteWakeup,flag,1,20,00,00,00

;HKR,Ndi\params\FlowControl,ParamDesc,,"Flow Control"
;HKR,Ndi\params\FlowControl,default,,1
;HKR,Ndi\params\FlowControl,type,,enum
;HKR,Ndi\params\FlowControl\enum,0,,"Disable"
;HKR,Ndi\params\FlowControl\enum,1,,"Enable"
;HKR,NDI\params\FlowControl,flag,1,20,00,00,00

;HKR,Ndi\params\PhoneLine,ParamDesc,,"Phone Line"
;HKR,Ndi\params\PhoneLine,default,,4
;HKR,Ndi\params\PhoneLine,type,,enum
;HKR,Ndi\params\PhoneLine\enum,0,,"Low Speed, Low Power"
;HKR,Ndi\params\PhoneLine\enum,2,,"Low Speed, High Power"
;HKR,Ndi\params\PhoneLine\enum,4,,"High Speed, Low Power"
;HKR,Ndi\params\PhoneLine\enum,6,,"High Speed, High Power"
;HKR,NDI\params\PhoneLine,flag,1,20,00,00,00

;****************************************************************
; Install section for OSR2 and Windows 98			*
;****************************************************************

[COUSB2T5.Install]
CopyFiles=CopyFile.Inf,CopyFile.Sys

[CopyFile.Inf]
cousb2t5.inf

[CopyFile.Sys]
COUSB2T5.SYS


;****************************************************************
; Install section for Windows NT 5				*
;****************************************************************

[COUSB2T5.NT.Reg]
; Interfaces
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "COUSB2T5"

[COUSB2T5.Service]
DisplayName    = %COUSB2T5.DeviceDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\COUSB2T5.SYS
LoadOrderGroup = NDIS
AddReg         = TextModeFlags.Reg

[Common.EventLog]
AddReg = Common.AddEventLog.Reg

[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

[TextModeFlags.Reg]
HKR, , TextModeFlags, 0x00010001, 0x0001

[CopyFile.NT.Sys]
COUSB2T5.SYS,,,2


;**********************************************************************
; Destination directories                                             *
;**********************************************************************

[DestinationDirs]
CopyFile.Sys    = 11
CopyFile.Inf    = 17
CopyFile.NT.Sys = 12

[SourceDisksNames]
; Cabinet file names and associated disks
; <cab#> = <disk#>,<cabinet filename>, ID (Unused, must be 0)
50="corega FEther USB2-TX Driver Diskette",,

[SourceDisksFiles]
;<file> = <cabinet number>,<subdir>,<filename>,<size>
;Note: File is not in a cabinet if cab# is 0
COUSB2T5.SYS=50,.,COUSB2T5.SYS,10000
cousb2t5.inf=50,.,cousb2t5.inf,10000


;**********************************************************************
; Localizable strings                                                 *
;**********************************************************************

[Strings]
USB = "corega K.K."
COUSB2T5.DeviceDesc = "corega FEther USB2-TX"


