;
; VaultMicro Serial Port Setup File
; Copyright (c) 2009 Vault Micro
;

[Version]
signature  = "$WINDOWS NT$"
Class      = Ports
Provider   = %VAULTMICRO%
ClassGuid  = {4D36E978-E325-11CE-BFC1-08002BE10318}
DriverVer=02/16/2011,2.3.0.0216
Catalogfile= LGELTEprt.cat

[ControlFlags]
ExcludeFromSelect = *

;*****************************************
; Vaultprt  Install Section
;*****************************************

[Manufacturer]
%VAULTMICRO% = VaultSerialPort, NTamd64

;*****************************************
; Vaultprt  Driver Path
;*****************************************

[SourceDisksNames.x86]
1 = %VaultSrcDisk%,,,\i386

[SourceDisksNames.amd64]
1 = %VaultSrcDisk%,,,\amd64

[SourceDisksFiles]
  LGELTEprt.sys = 1

[VaultSerialPort]
%VAULT_MODELS00% = VMportInstall, USB\VID_1004&PID_616B&MI_VP02	; for LGE G13 LTE serial
%VAULT_MODELS01% = VMportInstall, USB\VID_1004&PID_616B&MI_VP03	; for LGE G13 CDMA
%VAULT_MODELS02% = VMportInstall, USB\VID_1004&PID_616B&MI_VP04	; for LGE G13 GPS
%VAULT_MODELS03% = VMportInstall, USB\VID_1004&PID_616B&MI_VP05	; for LGE G13 LBS

%VAULT_MODELS00% = VMportInstall, USB\VID_1004&PID_61AA&MI_VP02	; for LGE G13 LTE serial
%VAULT_MODELS01% = VMportInstall, USB\VID_1004&PID_61AA&MI_VP03	; for LGE G13 CDMA
%VAULT_MODELS02% = VMportInstall, USB\VID_1004&PID_61AA&MI_VP04	; for LGE G13 GPS
%VAULT_MODELS03% = VMportInstall, USB\VID_1004&PID_61AA&MI_VP05	; for LGE G13 LBS


[VaultSerialPort.NTamd64]
%VAULT_MODELS00% = VMportInstall, USB\VID_1004&PID_616B&MI_VP02	; for LGE LTE serial
%VAULT_MODELS01% = VMportInstall, USB\VID_1004&PID_616B&MI_VP03	; for LGE CDMA
%VAULT_MODELS02% = VMportInstall, USB\VID_1004&PID_616B&MI_VP04	; for LGE GPS
%VAULT_MODELS03% = VMportInstall, USB\VID_1004&PID_616B&MI_VP05	; for LGE G13 LBS

%VAULT_MODELS00% = VMportInstall, USB\VID_1004&PID_61AA&MI_VP02	; for LGE LTE serial
%VAULT_MODELS01% = VMportInstall, USB\VID_1004&PID_61AA&MI_VP03	; for LGE CDMA
%VAULT_MODELS02% = VMportInstall, USB\VID_1004&PID_61AA&MI_VP04	; for LGE GPS
%VAULT_MODELS03% = VMportInstall, USB\VID_1004&PID_61AA&MI_VP05	; for LGE G13 LBS



[VMportInstall.NT]
CopyFiles=VMUsbDriverFiles
AddReg = All00, AddReg

[VMUsbDriverFiles]
LGELTEprt.sys

[DestinationDirs]
DefaultDestDir = 12

[VMportInstall.NT.Services]
AddService=LGELTEprt,  0x00000002, VM_USBSerialService

[VM_USBSerialService]
DisplayName   = %VMUSBSER%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\LGELTEprt.sys

[All00]
HKR,,NTMPDriver,,LGELTEprt.sys

[AddReg]
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[Strings]
VMUSBSER = "LGE USB Device for Serial Communication"
VaultSrcDisk = "LGE Serial Driver Disk"
VAULTMICRO   = "LG Electronics"

; for vendor specific string
VAULT_MODELS00 = "LGE LTE RF Serial Port "
VAULT_MODELS01 = "LGE CDMA USB Serial Port "
VAULT_MODELS02 = "LGE CDMA USB GPS NMEA Port "
VAULT_MODELS03 = "LGE CDMA LBS Serial Port "



VAULT_MODELS10 = "LGE LTE RF Serial Port "
VAULT_MODELS11 = "LGE WCDMA USB Serial Port "
VAULT_MODELS12 = "LGE WCDMA DS Serial Port "
VAULT_MODELS13 = "LGE WCDMA GPS1 Serial Port"
VAULT_MODELS14 = "LGE WCDMA GPS2 Serial Port"
VAULT_MODELS15 = "LGE WCDMA Download Serial Port"
VAULT_MODELS16 = "LGE WCDMA Packet Tool Serial Port"
