; Windows Virtual Serial Port Setup File
; Copyright (c) 2002,2003 
; Manufacturer: MBB
;

[Version]
signature  = "$WINDOWS NT$"
Class      = Ports
Provider   = %FlashCard%
ClassGuid  = {4D36E978-E325-11CE-BFC1-08002BE10318}
DriverVer  = 01/30/2013,1.2.0.0
CatalogFile= FcSwitch.cat

[SourceDisksNames]
1000 = %FCSRCDISK%,"",,

[SourceDisksFiles]
FcSwitch.sys = 1000

[ControlFlags]
ExcludeFromSelect = *

[DestinationDirs]
DefaultDestDir = 12

[Manufacturer]
%FlashCard% = FcSerialPort

[FcSerialPort]
%FcDevice% = FcInstall00, USB\VID_12d1&PID_1440

%FcDevice% = FcInstall00, USB\VID_12d1&PID_1F01
%FcDevice% = FcInstall00, USB\VID_12d1&PID_1F02

%VDFDevice% = FcInstall00, USB\VID_12d1&PID_1F10
%VDFDevice% = FcInstall00, USB\VID_12d1&PID_1F11
%VDFDevice% = FcInstall00, USB\VID_12d1&PID_1F12
%VDFDevice% = FcInstall00, USB\VID_12d1&PID_1F13
%VDFDevice% = FcInstall00, USB\VID_12d1&PID_1F14

%FcDevice00% = FcInstall00, USB\VID_12d1&PID_15FF&MI_03

; ###### Installation Section ######
[FcInstall00.NT]
CopyFiles = CopyFileSection00
AddReg = All00, AddReg.NT

[FcInstall00.NT.Services]
AddService = FcSwitch,  0x00000002, Fc_Service_Inst00

[Fc_Service_Inst00]
DisplayName   = "Fc Switch Driver"
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\FcSwitch.sys

[CopyFileSection00]
FcSwitch.sys

[All00]
HKR,,NTMPDriver,,FcSwitch.sys

[AddReg.NT]
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[Strings]
FlashCard   = "Flash Card"
FCSRCDISK = "Flash Card USB Driver Disk"
FcDevice = "FC - USB Device"
VDFDevice = "QuickStart Update USB Device"
