;/*++
;
;Copyright (c) 2009 Vault Micro All rights Reserved
;
;Module Name:
;
;    VAULTMUX.INF
;
;Abstract:
;    INF file for installing toaster mux enumerator driver
;
;--*/
[Version]
Signature="$WINDOWS NT$"
Class=USB
ClassGuid={36FC9E60-C465-11CF-8056-444553540000}
Provider=%VMSFT%
DriverVer=02/16/2011,2.3.0.0216
CatalogFile=LGELTEMux.cat

[DestinationDirs]
DefaultDestDir = 12

;*****************************************
; VaultMux  Driver Path
;*****************************************

[SourceDisksNames.x86]
1 = %VaultSrcDisk%,,,\i386

[SourceDisksNames.amd64]
1 = %VaultSrcDisk%,,,\amd64


[SourceDisksFiles]
LGELTEMux.sys  = 1,,

;*****************************************
; VaultMux  Install Section
;*****************************************

[Manufacturer]
%VMSFT%=Standard, NTamd64

[Standard]
;
; These are the vault mux pnp ids
;

%VaultMux.DeviceDescG13%=VaultMux_Device, USB\VID_1004&PID_616B&MI_01 ; LGE G13
%VaultMux.DeviceDescG13%=VaultMux_Device, USB\VID_1004&PID_61AA&MI_01 ; LGE G13

[Standard.NTamd64]
%VaultMux.DeviceDescG13%=VaultMux_Device, USB\VID_1004&PID_616B&MI_01 ; LGE G13
%VaultMux.DeviceDescG13%=VaultMux_Device, USB\VID_1004&PID_61AA&MI_01 ; LGE G13


[VaultMux_Device.NT]
CopyFiles=Drivers_Dir

[VaultMux_Device.NT.HW]
AddReg=VaultMux_Device.NT.AddReg

[VaultMux_Device.NT.AddReg]                            
HKR,,DeviceCharacteristics,0x10001,0x0100         ; Use same security checks on relative opens
HKR,,Security,,"D:P(A;;GA;;;BA)(A;;GA;;;SY)"      ; Allow generic-all access to Built-in administrators and Local system 

[Drivers_Dir]
LGELTEMux.sys


;-------------- Service installation
[VaultMux_Device.NT.Services]
AddService = LGELTEMux,%SPSVCINST_ASSOCSERVICE%, LGELTEMux_Service_Inst

; -------------- LGELTEMux driver install sections
[LGELTEMux_Service_Inst]
DisplayName    = %LGELTEMux.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\LGELTEMux.sys
LoadOrderGroup = Extended Base


[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
VMSFT = "LG Electronics"
VaultSrcDisk = "LGE Mux Installation Disk #1"
VaultMux.DeviceDescG13 = "LGE LTE Mux Enumerator"
VaultMux.DeviceDescF1 = "LGE F1 Mux Enumerator "
LGELTEMux.SVCDESC = "LGE LTE Mux Enumerator "

