------------------------------------------------------------------------------
  Updating Creative Video Blaster WebCam Go ES Driver (Version 1.03)
  October 2001
------------------------------------------------------------------------------
  This document provides late-breaking of other information that supplements
  the WebCam Go ES documentation included with your camera.
--------
CONTENTS
--------

1.   UPDATING THE DRIVER

2.   WHAT'S NEW IN DRIVER VERSION 1.03


==============================================================================

1.   UPDATING THE DRIVER
     -------------------

     To install the new driver:

     1.  Disconnect Video Blaster WebCam Go ES from your computer.
     2.  Double-click CtDrvStp.exe in the installed folder. Follow the 
         instructions on the screen to uninstall the existing driver.
     3.  Connect Video Blaster WebCam Go ES to your computer.
         Windows will detect the camera and install the updated driver.

         NOTE: In Windows 2000 and Windows XP, the Digital Signature Not Found 
         dialog box may appear. Click the YES button to continue with the 
         installation.

2.   WHAT'S NEW IN DRIVER VERSION 1.03
     ---------------------------------

     1.  Fixed a page fault bug when images are downloaded from the camera.
     2.  The IYUV video format is replaced with the I420 video 
         format.
     3.  You can take a snapshot after disconnecting and reconnecting the 
         camera while running WebCam Go Control in Windows 2000.
     4.  Corrected an image processing step that can cause small amounts of 
         image corruption for downloaded images.

     
Copyright (c) October 2001 Creative Technology Ltd. All rights reserved.
--------------------------------------------------------------------------
  End of Readme File
--------------------------------------------------------------------------
