; Installation inf for the Multitouch USB Client Driver.

[Version]
Signature="$Windows NT$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
Provider=%Cypress%
DriverVer=01/11/2011,1.3.13
CatalogFile=MTUSB.cat

[SourceDisksNames]
1=%Disk_Description%,,,

[SourceDisksFiles]
mtusbclient.sys = 1

[Manufacturer]
%Cypress%=Cypress, NTx86, NTamd64

[Cypress.NTx86]
%MTClient.DeviceDesc%=MTUSB.Dev, USB\VID_04B4&PID_C001&MI_01

[Cypress.NTamd64]
%MTClient.DeviceDesc%=MTUSB.Dev, USB\VID_04B4&PID_C001&MI_01

[DestinationDirs]
MTUSB.Files.Ext = 10,System32\Drivers

[MTUSB.Dev.NT]
CopyFiles=MTUSB.Files.Ext

[MTUSB.Dev.NT.Services]
Addservice = MTUSB, 0x00000002, MTUSB.AddService

[MTUSB.AddService]
DisplayName    = %MTUSB.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\mtusbclient.sys
AddReg         = MTUSB.AddReg
LoadOrderGroup = Base

[MTUSB.AddReg]
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2
HKR,"Parameters","MTUSBEnable",0x10001,1

[MTUSB.Files.Ext]
mtusbclient.sys

;---------------------------------------------------------------;

[Strings]
Cypress="Cypress Semiconductor"
Disk_Description="MTUSB Installation Disk"
MTClient.DeviceDesc="Multitouch Client Driver"
MTUSB.SvcDesc="Multitouch Client Driver"
