;/*++
;
;Copyright (c) 2013 Intel Corporation
;
;Module Name:
;    iaLPSS_UART.inf
;
;Abstract:
;    INF file for installing the Intel(R) Serial IO UART Driver
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
DriverVer=02/08/2013,1.0.1.121
CatalogFile = iaLPSS.cat

[DestinationDirs]
DefaultDestDir = 12

; ================= Class section =====================

;[ClassInstall32]
;Addreg=SampleClassReg     

;[SampleClassReg]
;HKR,,,0,%ClassName%
;HKR,,Icon,,-5

[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles]
iaLPSS_UART.sys  = 1,,

;*****************************************
; iaLPSS_UART Install Section
;*****************************************

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%INTEL%=Intel,NTamd64

; For XP and later
[Intel.NTamd64]
; DisplayName               Section             DeviceId
; -----------               -------             --------
%iaLPSS_UART.DeviceDesc1%= iaLPSS_UART_Inst,   ACPI\INT33C4
%iaLPSS_UART.DeviceDesc2%= iaLPSS_UART_Inst,   ACPI\INT33C5

[iaLPSS_UART_Inst.NT]
CopyFiles=Drivers_Dir

[Drivers_Dir]
iaLPSS_UART.sys

;-------------- Service installation
[iaLPSS_UART_Inst.NT.Services]
AddService = iaLPSS_UART,%SPSVCINST_ASSOCSERVICE%, iaLPSS_UART_Service_Inst

; -------------- iaLPSS_UART driver install sections
[iaLPSS_UART_Service_Inst]
DisplayName    = %iaLPSS_UART.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\iaLPSS_UART.sys
LoadOrderGroup = Extended Base
Dependencies   = SerCx

[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
INTEL = "Intel Corporation"
DiskId1 = "Intel(R) Serial IO Installation Disk"
iaLPSS_UART.DeviceDesc1 = "Intel(R) Serial IO UART Host Controller - 9C63"
iaLPSS_UART.DeviceDesc2 = "Intel(R) Serial IO UART Host Controller - 9C64"
iaLPSS_UART.SVCDESC = "Intel(R) Serial IO UART Driver"


[PackageInfo]
Name=UART64
