;*****************************************************************************
;*
;*  E22w7x64.INF  -   Bigfoot llama e2200 Series PCI-E Ethernet Controller
;*  Copyright 2011 - Bigfoot Networks, Inc.
;*
;*  Created on 03/04/2011 by Yu Hao
;*  INF File for NDIS6.2 Miniport Driver for Windows7 x64 
;*  Modified on 08/09/2011 for Bigfoot Networks C. Musta 
;*    Bigfoot drivers only attache to DevID 1091
;*****************************************************************************
[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %BFTN%
CatalogFile = E22W7x64.cat
DriverVer=03/20/2013,8.0.2.42

[Manufacturer]
%BFTN% = Killer, NTamd64

[ControlFlags]

ExcludeFromSelect       = *


[Killer.NTamd64]
; DisplayName           Section                DeviceID
; -----------           -------                --------
%BFTN.L1F%  =           L1F.ndi,               PCI\VEN_1969&DEV_E091 				    ; e2201/e2205

;-----------------------------------------------------------------------------
; l1f supports new pm offload and rss, msi-x
;-----------------------------------------------------------------------------
[L1F.ndi]
Characteristics = 0x84
BusType         = 5             ;PCI
AddReg          = L1C.reg, L1C.params, Common.params, ShutOff.params, WOLDefault.params, PM.params, RSS.params, Intr.params, EEELPI.params, Ecma.params
CopyFiles       = L1C.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3

[L1F.ndi.HW]
Include = machine.inf
Needs = PciASPMOptOut
Addreg = MsiX.Addreg

[L1F.ndi.Services]
AddService = Ke2200, 2, L1C.Service, L1C.EventLog


;-----------------------------------------------------------------------------
; L1C  specific
;
[L1C.reg]
HKR, Ndi, HelpText,, %HelpText%
HKR, Ndi, Service,    0, "Ke2200"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[Msi.Addreg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[MsiX.Addreg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0

[L1C.Service]
DisplayName     = %L1C.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\e22w7x64.sys
LoadOrderGroup  = NDIS

[L1C.EventLog]
AddReg = L1C.AddEventLog.reg

[L1C.AddEventLog.reg]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\Drivers\e22w7x64.sys"
HKR,, TypesSupported,   0x00010001, 7

[Intr.params]
HKR,, MSIX,             0x00010001, 1

[L1C.params]
HKR, Ndi\Params\*JumboPacket,                   ParamDesc,      0,      %JumboFrame%
HKR, Ndi\Params\*JumboPacket,                   default,        0,      "1514"
HKR, Ndi\Params\*JumboPacket,                   type,           0,      "enum"
HKR, Ndi\Params\*JumboPacket\enum,              "1514",         0,      %Disabled%
HKR, Ndi\Params\*JumboPacket\enum,              "2048",         0,      %2KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,              "3072",         0,      %3KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,              "4096",         0,      %4KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,              "5120",         0,      %5KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,              "6144",         0,      %6KBMTU%
HKR, Ndi\Params\*JumboPacket\enum,              "7168",         0,      %7KBMTU%
HKR, Ndi\params\*JumboPacket\enum,              "8192",         0,      %8KBMTU%
HKR, Ndi\params\*JumboPacket\enum,              "9216",         0,      %9KBMTU%

[RSS.params]
HKR, Ndi\Params\RSS,                            ParamDesc,      0,      %RSS%
HKR, Ndi\Params\RSS,                            Type,           0,      "enum"
HKR, Ndi\Params\RSS\enum,                       1,              0,      %Enabled%
HKR, Ndi\Params\RSS\enum,                       0,              0,      %Disabled%
HKR, Ndi\Params\RSS,                            Default,        0,      "0"

HKR, Ndi\Params\*NumRssQueues,                  ParamDesc,      0,      %RssQs%
HKR, Ndi\Params\*NumRssQueues,                  Type,           0,      "enum"
HKR, Ndi\Params\*NumRssQueues\enum,             "8",            0,      "8 RSS Queues"
HKR, Ndi\Params\*NumRssQueues\enum,             "6",            0,      "6 RSS Queues"
HKR, Ndi\Params\*NumRssQueues\enum,             "4",            0,      "4 RSS Queues"
HKR, Ndi\Params\*NumRssQueues\enum,             "2",            0,      "2 RSS Queues"
HKR, Ndi\Params\*NumRssQueues\enum,             "1",            0,      "1 RSS Queues"
HKR, Ndi\Params\*NumRssQueues,                  Default,        0,      "4"

[L2CB.params]
HKR, Ndi\Params\APSmode,                        ParamDesc,      0,      %APSmode%
HKR, Ndi\Params\APSmode,                        Type,           0,      "enum"
HKR, Ndi\Params\APSmode\enum,                   "1",            0,      %Enabled%
HKR, Ndi\Params\APSmode\enum,                   "0",            0,      %Disabled%
HKR, Ndi\Params\APSmode,                        Default,        0,      "0"

[EEELPI.params]
HKR, Ndi\Params\*EEE,                           ParamDesc,      0,      %EEE%
HKR, Ndi\Params\*EEE,                           Type,           0,      "enum"
HKR, Ndi\Params\*EEE\enum,                      "1",            0,      %Enabled%
HKR, Ndi\Params\*EEE\enum,                      "0",            0,      %Disabled%
HKR, Ndi\Params\*EEE,                           Default,        0,      "0"

[EEELPIEn.params]
HKR, Ndi\Params\*EEE,                           ParamDesc,      0,      %EEE%
HKR, Ndi\Params\*EEE,                           Type,           0,      "enum"
HKR, Ndi\Params\*EEE\enum,                      "1",            0,      %Enabled%
HKR, Ndi\Params\*EEE\enum,                      "0",            0,      %Disabled%
HKR, Ndi\Params\*EEE,                           Default,        0,      "1"

[Ecma.params]
HKR, Ndi\Params\Ecma,                           ParamDesc,      0,      %ECMA%
HKR, Ndi\Params\Ecma,                           Type,           0,      "enum"
HKR, Ndi\Params\Ecma\enum,                      "1",            0,      %Enabled%
HKR, Ndi\Params\Ecma\enum,                      "0",            0,      %Disabled%
HKR, Ndi\Params\Ecma,                           Default,        0,      "0"

;-----------------------------------------------------------------------------

[Common.params]
HKR, Ndi\Params\MaxInterrupt,                   ParamDesc,      0,      %MaxIrq%
HKR, Ndi\Params\MaxInterrupt,                   Type,           0,      "int"
HKR, Ndi\Params\MaxInterrupt,                   Base,           0,      "10"
HKR, Ndi\Params\MaxInterrupt,                   Min,            0,      "1000"
HKR, Ndi\Params\MaxInterrupt,                   Max,            0,      "30000"
HKR, Ndi\Params\MaxInterrupt,                   Step,           0,      "500"
HKR, Ndi\Params\MaxInterrupt,                   Default,        0,      "10000"

HKR, Ndi\Params\*SpeedDuplex,                   ParamDesc,      0,      %SpeedDuplex%
HKR, Ndi\Params\*SpeedDuplex,                   Type,           0,      "enum"
HKR, Ndi\Params\*SpeedDuplex,                   Default,        0,      "0"
HKR, Ndi\Params\*SpeedDuplex\enum,              "0",            0,      %Auto%
HKR, Ndi\Params\*SpeedDuplex\enum,              "1",            0,      %10MHD%
HKR, Ndi\Params\*SpeedDuplex\enum,              "2",            0,      %10MFD%
HKR, Ndi\Params\*SpeedDuplex\enum,              "3",            0,      %100MHD%
HKR, Ndi\Params\*SpeedDuplex\enum,              "4",            0,      %100MFD%

HKR, Ndi\Params\*ReceiveBuffers,                ParamDesc,      0,      %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,                Type,           0,      "int"
HKR, Ndi\Params\*ReceiveBuffers,                Base,           0,      "10"
HKR, Ndi\Params\*ReceiveBuffers,                Min,            0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,                Max,            0,      "2048"
HKR, Ndi\Params\*ReceiveBuffers,                Step,           0,      "16"
HKR, Ndi\Params\*ReceiveBuffers,                Default,        0,      "512"

HKR, Ndi\Params\*TransmitBuffers,               ParamDesc,      0,      %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,               Type,           0,      "int"
HKR, Ndi\Params\*TransmitBuffers,               Base,           0,      "10"
HKR, Ndi\Params\*TransmitBuffers,               Min,            0,      "16"
HKR, Ndi\Params\*TransmitBuffers,               Max,            0,      "1024"
HKR, Ndi\Params\*TransmitBuffers,               Step,           0,      "16"
HKR, Ndi\Params\*TransmitBuffers,               Default,        0,      "512"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,        ParamDesc,      0,      %TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,        Type,           0,      "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,   "3",            0,      %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,   "2",            0,      %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,   "1",            0,      %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,   "0",            0,      %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,        Default,        0,      "3"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,         ParamDesc,      0,      %IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,         Type,           0,      "enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,    "3",            0,      %TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,    "2",            0,      %RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,    "1",            0,      %TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,    "0",            0,      %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,         Default,        0,      "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,        ParamDesc,      0,      %UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,        Type,           0,      "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,   "3",            0,      %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,   "2",            0,      %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,   "1",            0,      %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,   "0",            0,      %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,        Default,        0,      "3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,        ParamDesc,      0,      %TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,        Type,           0,      "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,   "3",            0,      %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,   "2",            0,      %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,   "1",            0,      %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,   "0",            0,      %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,        Default,        0,      "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,        ParamDesc,      0,      %UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,        Type,           0,      "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,   "3",            0,      %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,   "2",            0,      %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,   "1",            0,      %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,   "0",            0,      %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,        Default,        0,      "3"

HKR, Ndi\Params\*LsoV1IPv4,                     ParamDesc,      0,      %LSOv1IPv4%
HKR, Ndi\Params\*LsoV1IPv4,                     Type,           0,      "enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,                "1",            0,      %Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,                "0",            0,      %Disabled%
HKR, Ndi\Params\*LsoV1IPv4,                     Default,        0,      "1"

HKR, Ndi\Params\*LsoV2IPv4,                     ParamDesc,      0,      %LSOv2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,                     Type,           0,      "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,                "1",            0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,                "0",            0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv4,                     Default,        0,      "0"

HKR, Ndi\Params\*LsoV2IPv6,                     ParamDesc,      0,      %LSOv2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,                     Type,           0,      "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,                "1",            0,      %Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,                "0",            0,      %Disabled%
HKR, Ndi\Params\*LsoV2IPv6,                     Default,        0,      "0"

HKR, Ndi\Params\NetworkAddress,                 ParamDesc,      0,      %NetAddress%
HKR, Ndi\Params\NetworkAddress,                 Type,           0,      "edit"
HKR, Ndi\Params\NetworkAddress,                 LimitText,      0,      "12"
HKR, Ndi\Params\NetworkAddress,                 UpperCase,      0,      "1"
HKR, Ndi\Params\NetworkAddress,                 Default,        0,      ""
HKR, Ndi\Params\NetworkAddress,                 Optional,       0,      "1"

HKR, Ndi\Params\*InterruptModeration,           ParamDesc,      0,      %IntMod%
HKR, Ndi\Params\*InterruptModeration,           Type,           0,      "enum"
HKR, Ndi\Params\*InterruptModeration\enum,      "1",            0,      %Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,      "0",            0,      %Disabled%
HKR, Ndi\Params\*InterruptModeration,           Default,        0,      "0"

HKR, Ndi\Params\*FlowControl,                   ParamDesc,      0,      %FlowCtrl%
HKR, Ndi\Params\*FlowControl,                   Type,           0,      "enum"
HKR, Ndi\Params\*FlowControl\enum,              "3",            0,      %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,              "0",            0,      %Disabled%
HKR, Ndi\Params\*FlowControl,                   Default,        0,      "3"

HKR, Ndi\Params\VLanID,                         ParamDesc,      0,      %VLanID%
HKR, Ndi\Params\VLanID,                         Type,           0,      "long"
HKR, Ndi\Params\VLanID,                         Base,           0,      "10"
HKR, Ndi\Params\VLanID,                         Min,            0,      "0"
HKR, Ndi\Params\VLanID,                         Max,            0,      "4094"
HKR, Ndi\Params\VLanID,                         Step,           0,      "1"
HKR, Ndi\Params\VLanID,                         Default,        0,      "0"

[WOLDefault.params]
HKR, Ndi\Params\*WakeOnMagicPacket,             ParamDesc,      0,      %WakeOnMagic%
HKR, Ndi\Params\*WakeOnMagicPacket,             Type,           0,      "enum"
HKR, Ndi\Params\*WakeOnMagicPacket\enum,        "1",            0,      %Enabled%
HKR, Ndi\Params\*WakeOnMagicPacket\enum,        "0",            0,      %Disabled%
HKR, Ndi\Params\*WakeOnMagicPacket,             Default,        0,      "1"

HKR, Ndi\Params\*WakeOnPattern,                 ParamDesc,      0,      %WakeOnPattern%
HKR, Ndi\Params\*WakeOnPattern,                 Type,           0,      "enum"
HKR, Ndi\Params\*WakeOnPattern\enum,            "1",            0,      %Enabled%
HKR, Ndi\Params\*WakeOnPattern\enum,            "0",            0,      %Disabled%
HKR, Ndi\Params\*WakeOnPattern,                 Default,        0,      "1"

;HKR, Ndi\Params\*DeviceSleepOnDisconnect,      ParamDesc,      0,      %SleepOnDisconnect%
;HKR, Ndi\Params\*DeviceSleepOnDisconnect,      Type,           0,      "enum"
;HKR, Ndi\Params\*DeviceSleepOnDisconnect\enum, "1",            0,      %Enabled%
;HKR, Ndi\Params\*DeviceSleepOnDisconnect\enum, "0",            0,      %Disabled%
;HKR, Ndi\Params\*DeviceSleepOnDisconnect,      Default,        0,      "1"

[WOLMagic.params]
HKR, Ndi\Params\*WakeOnMagicPacket,             ParamDesc,      0,      %WakeOnMagic%
HKR, Ndi\Params\*WakeOnMagicPacket,             Type,           0,      "enum"
HKR, Ndi\Params\*WakeOnMagicPacket\enum,        "1",            0,      %Enabled%
HKR, Ndi\Params\*WakeOnMagicPacket\enum,        "0",            0,      %Disabled%
HKR, Ndi\Params\*WakeOnMagicPacket,             Default,        0,      "1"

HKR, Ndi\Params\*WakeOnPattern,                 ParamDesc,      0,      %WakeOnPattern%
HKR, Ndi\Params\*WakeOnPattern,                 Type,           0,      "enum"
HKR, Ndi\Params\*WakeOnPattern\enum,            "1",            0,      %Enabled%
HKR, Ndi\Params\*WakeOnPattern\enum,            "0",            0,      %Disabled%
HKR, Ndi\Params\*WakeOnPattern,                 Default,        0,      "0"

[WOLNone.params]
HKR, Ndi\Params\*WakeOnMagicPacket,             ParamDesc,      0,      %WakeOnMagic%
HKR, Ndi\Params\*WakeOnMagicPacket,             Type,           0,      "enum"
HKR, Ndi\Params\*WakeOnMagicPacket\enum,        "1",            0,      %Enabled%
HKR, Ndi\Params\*WakeOnMagicPacket\enum,        "0",            0,      %Disabled%
HKR, Ndi\Params\*WakeOnMagicPacket,             Default,        0,      "0"

HKR, Ndi\Params\*WakeOnPattern,                 ParamDesc,      0,      %WakeOnPattern%
HKR, Ndi\Params\*WakeOnPattern,                 Type,           0,      "enum"
HKR, Ndi\Params\*WakeOnPattern\enum,            "1",            0,      %Enabled%
HKR, Ndi\Params\*WakeOnPattern\enum,            "0",            0,      %Disabled%
HKR, Ndi\Params\*WakeOnPattern,                 Default,        0,      "0"

[PM.params]
HKR, Ndi\Params\*PMARPOffload,                  ParamDesc,      0,      %ARPOffload%
HKR, Ndi\Params\*PMARPOffload,                  Type,           0,      "enum"
HKR, Ndi\Params\*PMARPOffload\enum,             "1",            0,      %Enabled%
HKR, Ndi\Params\*PMARPOffload\enum,             "0",            0,      %Disabled%
HKR, Ndi\Params\*PMARPOffload,                  Default,        0,      "1"

HKR, Ndi\Params\*PMNSOffload,                   ParamDesc,      0,      %NSOffload%
HKR, Ndi\Params\*PMNSOffload,                   Type,           0,      "enum"
HKR, Ndi\Params\*PMNSOffload\enum,              "1",            0,      %Enabled%
HKR, Ndi\Params\*PMNSOffload\enum,              "0",            0,      %Disabled%
HKR, Ndi\Params\*PMNSOffload,                   Default,        0,      "1"

[ShutOn.params]
HKR, Ndi\Params\ShutdownWake,                   ParamDesc,      0,       %ShutDW%
HKR, Ndi\Params\ShutdownWake,                   Type,           0,       "enum"
HKR, Ndi\Params\ShutdownWake\enum,              1,              0,       %Enabled%
HKR, Ndi\Params\ShutdownWake\enum,              0,              0,       %Disabled%
HKR, Ndi\Params\ShutdownWake,                   Default,        0,       "1"

[ShutOff.params]
HKR, Ndi\Params\ShutdownWake,                   ParamDesc,      0,       %ShutDW%
HKR, Ndi\Params\ShutdownWake,                   Type,           0,       "enum"
HKR, Ndi\Params\ShutdownWake\enum,              1,              0,       %Enabled%
HKR, Ndi\Params\ShutdownWake\enum,              0,              0,       %Disabled%
HKR, Ndi\Params\ShutdownWake,                   Default,        0,       "0"

;-----------------------------------------------------------------------------
; DestinationDirs
;
[L1C.CopyFiles]
e22W7x64.sys,,,2

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %DriverDisk%,,,

[SourceDisksFiles]
;
; filename_on_source = diskID[, [subdir][, size]]
;
e22W7x64.sys = 1

[DestinationDirs]
L1C.CopyFiles           = 12
DefaultDestDir          = 11

[Strings]
BFTN                     = "Killer"
JumboFrame               = "Jumbo Frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
IntMod                   = "Interrupt Moderation"
L0sL1Threshold           = "L0sL1 Gateway"
MaxIrq                   = "Max IRQ per Second"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
SpeedDuplex              = "Speed & Duplex"
Auto                     = "Auto Negotiation"
1GFD                     = "1.0 Gbps Full Duplex"
10MHD                    = "10 Mbps Half Duplex"
10MFD                    = "10 Mbps Full Duplex"
100MHD                   = "100 Mbps Half Duplex"
100MFD                   = "100 Mbps Full Duplex"
FlowCtrl                 = "FlowControl"
ShutDW                   = "Shutdown Wake Up"
RSS                      = "Receive Side Scaling"
TXEna                    = "Tx Enabled"
RXEna                    = "Rx Enabled"
TXRXEna                  = "Tx & Rx Enabled"
ReceiveBuffers           = "Receive Buffers"
TransmitBuffers          = "Transmit Buffers"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
LSOv1IPv4                = "Large Send Offload (IPv4)"
LSOv2IPv4                = "Large Send Offload v2 (IPv4)"
LSOv2IPv6                = "Large Send Offload v2 (IPv6)"
NetAddress               = "Network Address"
APSmode                  = "APS mode"
EEE                      = "Energy Efficient Ethernet "
None                     = "None"
VLanID                   = "VLAN ID"
WakeOnPattern            = "Wake on pattern match"
WakeOnMagic              = "Wake on magic packet"
SleepOnDisconnect        = "Device sleep on disconnect"
ARPOffload               = "ARP offload"
NSOffload                = "NS offload"
ECMA                     = "ECMA"
RssQs                    = "RSS Queues"

BFTN.L1F                 = "Killer e2200 PCI-E Gigabit Ethernet Controller (NDIS 6.20)"
L1C.Service.DispName     = "NDIS Miniport Driver for the Killer e2200 PCI-E Ethernet Controller"
DriverDisk               = "Killer e2200 Series PCI-E Ethernet Controller Installation Disk"
HelpText                 = "This Killer e2200 Network Controller connects you to the network."

