
[version]
Signature  = "$Chicago$"
Class      = Net
Compatible = 1
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
provider   = %PC_CARD%
LayoutFile = layout.inf
DriverVer  = 01/17/2000

[Manufacturer]
%PC_CARD%  = PC_CARD

[PC_CARD]
%PC_CARD.DeviceDesc%  = le100cc.ndi, PCMCIA\Fast_Ethernet-16-bit_PC_Card-8B43
%PC_CARD.DeviceDesc%  = le100cc.ndi, PCMCIA\Fast_Ethernet-Adapter-8524
%PC_CARD.DeviceDesc%  = le100cc.ndi, PCMCIA\Fast_Ethernet-Adapter-A1C6
%PC_CARD.DeviceDesc%  = le100cc.ndi, PCMCIA\Dual_Speed-10/100_PC_Card-81FE
%PC_CARD.DeviceDesc%  = le100cc.ndi, PCMCIA\Fast_Ethernet-CF_Size_PC_Card-94CA

;----------------------------------------------------------------------------
; Win 2000 main sections
;
[le100cc.ndi.NT]
Characteristics = 0x84
BusType         = 8
AddReg          = le100.ndi.reg, common.reg
CopyFiles       = le100.ndis5.CopyFiles

[le100cc.ndi.NT.Services]
AddService = le100, 2, le100.Service, le100.AddEventLog

[Common.reg]
HKR,Ndi\params\ConnectionType,ParamDesc,0,"Connection Type"
HKR,Ndi\params\ConnectionType,default,0,5
HKR,Ndi\params\ConnectionType,type,0,enum
HKR,Ndi\params\ConnectionType\enum,5,0,"Auto Sense "
HKR,Ndi\params\ConnectionType\enum,6,0,"100Mbps Full Duplex"
HKR,Ndi\params\ConnectionType\enum,4,0,"100Mbps "
HKR,Ndi\params\ConnectionType\enum,2,0,"10Mbps Full Duplex "
HKR,Ndi\params\ConnectionType\enum,0,0,"10Mbps "
HKR, ,               ConnectionType,0,"5"

;----------------------------------------------------------------------------
;    Win 2000 Drivers
;
[le100.ndi.reg]
HKR, Ndi,               Service,    0, "le100"
HKR, Ndi\Interfaces,    LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces,    UpperRange, 0, "ndis5,ndis3"
HKR,               ,    Pcmcia    , 0, "2"

HKR,,InterruptNumber,1,04,00,00,00
HKR,,IOBaseAddress,1,02,00,00,00

[le100.ndis5.CopyFiles]
tx100nd5.sys,,,2

[le100.Service]
DisplayName     =   %Service.DispName%
ServiceType     =   1 ;%SERVICE_KERNEL_DRIVER%
StartType       =   3 ;%SERVICE_AUTO_START%
ErrorControl    =   1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   =   %12%\tx100nd5.sys
LoadOrderGroup  =   NDIS
AddReg          =   TextModeFlags.reg

[le100.AddEventLog]
AddReg = le100.AddEventLog.reg

[le100.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[TextModeFlags.reg]
HKR, , TextModeFlags, 0x00010001, 0x0001


;----------------------------------------------------------------------------
; Win 9x main sections
;
[le100cc.ndi]
AddReg=le100X.ndi.reg, ne2000.ndi.reg, Clone.params.reg, common.reg
LogConfig=le100cc.LogConfigOverride

[le100cc.LogConfigOverride]
IRQConfig=3,4,5,7,10,11,12,13,15
IOConfig=20@200-3FF%FFE0(3FF::)
ConfigPriority = HARDRECONFIG

[le100X.ndi.reg]
HKR,Ndi,DeviceID,,"PCMCIA-Fast_Ethernet-Adapter-8524"
HKR,Ndi,DeviceID,,"PCMCIA-Fast_Ethernet-Adapter-A1C6"
HKR,Ndi,DeviceID,,"PCMCIA-Dual_Speed-10/100_PC_Card-81FE"
HKR,Ndi,CardType,,"PCMCIA"


;****************************************************************************
; Win 9x Drivers
; Base section for ne2000 users
;
[ne2000.ndi.reg]
; key,subkey,valuname,type,value
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,tx100nds.sys
HKR,,Driver,,"tx100nds.sys"
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
; NDIS Info
HKR,NDIS,LogDriverName,,"le100"
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0A
; Interfaces
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
; Install sectioins
HKR,Ndi\Install,ndis3,,"le100X.ndis3"

;Install NDIS3
[le100X.ndis3]
CopyFiles = le100X.ndis3.CopyFiles

[le100X.ndis3.CopyFiles]
tx100nds.sys,,,2

;extra params for clones
[Clone.params.reg]
; Resources
HKR,,InterruptNumber,1,04,00,00,00
HKR,,IOBaseAddress,1,02,00,00,00
HKR,NDI\params\InterruptNumber,resc,1,04,00,00,00
HKR,Ndi\params\interruptNumber,ParamDesc,,"Interrupt Level"
HKR,NDI\params\InterruptNumber,flag,1,60,00,00,00
HKR,NDI\params\IOBaseAddress,resc,1,02,00,00,00
HKR,NDI\params\IOBaseAddress,ParamDesc,,"I/O Base Address"
HKR,NDI\params\IOBaseAddress,flag,1,20,00,00,00

;
;----------------------------------------------------------------------------
; Destination Directories
;
[DestinationDirs]
DefaultDestDir         = 11 ; LDID_SYS
le100X.ndis3.CopyFiles = 11
le100.ndis5.CopyFiles  = 12

[SourceDisksNames]
1 = "PCMCIA Fast Ethernet Card Driver Disk",,

[SourceDisksFiles]
;tx100nds.sys = 1
tx100nd5.sys = 1

[Strings]
Service.DispName =   "PCMCIA Fast Ethernet NT Driver"

PC_CARD   =   "PC Card Series Products"
PC_CARD.DeviceDesc  =   "PCMCIA Fast Ethernet Card"
