;; EP325.INF (NT 5.0 & Win98 combined inf for NDIS5 driver)

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %SURECOM%
LayoutFile  = layout.inf
DriverVer=07/01/2001,5.508.803.2000

[Manufacturer]
%SURECOM%   = SURECOM


[ControlFlags]
ExcludeFromSelect       = *

[SURECOM]

%RTL8029s.DeviceDesc%   = RTL8029.ndi, PCI\VEN_10EC&DEV_8029&SUBSYS_802910EC ; Realtek RTL8029(AS)-based PCI Ethernet Adapter


;-------------------------------------------------------------------------------
; Realtek Common
;
[RTL8029.ndi]
AddReg          = RTL8029.reg, RTL8029.ntpci.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8029.CopyFiles

[RTL8029.ndi.Services]
AddService      = rtl8029, 2, pcint.Service, RTL8029.EventLog

[RTL8029.CopyFiles]
RTL8029.sys,,,2

;-------------------------------------------------------------------------------
; RTL8029 Advanced UI
;
[RTL8029.ntpci.reg]
HKR, Ndi\params\MediaMode,       ParamDesc,  0, %MediaMode%
HKR, Ndi\params\MediaMode,       type,       0, "enum"
HKR, Ndi\params\MediaMode,       default,    0, "0"
HKR, Ndi\params\MediaMode\enum,  0,          0, %TPHD%
HKR, Ndi\params\MediaMode\enum,  1,          0, %TPFD%
HKR, Ndi\params\MediaMode\enum,  2,          0, %BNC%
HKR, Ndi\params\MediaMode\enum,  3,          0, %AUI%

;-------------------------------------------------------------------------------
; RTL8029 Service and Driver
;
[RTL8029.reg]
HKR, Ndi,                        Service,    0, "RTL8029"
HKR, Ndi\Interfaces,             UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,             LowerRange, 0, "ethernet"

[pcint.Service]
DisplayName     = %RTL8029.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\RTL8029.SYS
LoadOrderGroup  = NDIS

[RTL8029.EventLog]
Addreg = RTL8029.AddEventLog.reg

[RTL8029.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

[DestinationDirs]
DefaultDestDir     = 12
RTL8029.CopyFiles  = 12

[Strings]
;Msft                      = "Microsoft"

SURECOM                   = "SURECOM Technology Corp."

MediaMode                 = "Line Speed"
TPHD                      = "TP Half Duplex"
TPFD                      = "TP Full Duplex"
BNC                       = "BNC / 10Base2"
AUI                       = "AUI / 10Base5"



RTL8029s.DeviceDesc       = "SURECOM EP-325 PCI Ethernet Adapter"
RTL8029.Service.DispName  = "SURECOM EP-325 PCI Ethernet Adapter NT Driver"
