;/*++
;
;Copyright (c) Broadcom Corporation.  All rights reserved.
;
; x86 Vista Smart Card Reader Filter Install;
;
;--*/
[Version]
Signature="$Windows NT$"
Class=SmartCardReader
ClassGuid={50DD5230-BA8A-11D1-BF5D-0000F805F530}
Provider="Broadcom"
DriverVer=09/23/2008, 1.0.0.1
CatalogFile=ccidfltv.cat

[SourceDisksNames]
1=%Distribution%,,,

[SourceDisksFiles]
ccidflt.sys = 1

[Manufacturer]
Broadcom=Broadcom

[BROADCOM]
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5800&MI_01
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5800&MI_02
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5801&MI_01
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5801&MI_02
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5802&MI_01
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5802&MI_02
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5803&MI_01
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5803&MI_02
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5804&MI_01
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5804&MI_02
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5805&MI_01
%BRCMCCID.DeviceDesc% = BRCMCCID.Install,USB\VID_0A5C&PID_5805&MI_02

[BRCMCCID.Install.NT]
Include=usbccid.inf
Needs=USBCCID.Install.NT
CopyFiles=BRCMCCID.Install.CopyFiles

[BRCMCCID.Install.CopyFiles]
ccidflt.sys,,,2

[BRCMCCID.Install.NT.Services]
Include=usbccid.inf
Needs=USBCCID.Install.NT.Services
AddService = CCIDFILTER, , CCIDFILTER.AddService

[CCIDFILTER.AddService]
DisplayName = %CCIDFILTER.SvcDesc%
ServiceType = 1
StartType = 3
ErrorControl = 1
ServiceBinary = %12%\ccidflt.SYS
LoadOrderGroup = PnP Filter

[BRCMCCID.Install.NT.HW]
AddReg=CCIDFILTER_Filter_Reg

[CCIDFILTER_Filter_Reg]
HKR,,"UpperFilters",0x00010000,"CCIDFILTER"

[DestinationDirs]
BRCMCCID.Install.CopyFiles = 12

[Strings]
Broadcom = "Broadcom Corporation"
Distribution = "Broadcom Driver Disk"
BRCMCCID.DeviceDesc = "USB Smart Card Reader"
CCIDFILTER.SvcDesc = "Broadcom Smart Card Reader Filter Driver"
