;/*++
;Abstract:
;    INF file for installing the Nuvoton W836x7HG CIR Device Driver
;
;
;--*/
[Version]
Signature="$WINDOWS NT$"
Class=HIDClass
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
Provider=%PROVIDER_NAME%
DriverVer=05/05/2010,1.0.2010.0505
CatalogFile=nuviocir_xp_x64.cat

[DestinationDirs]
DefaultDestDir=12

[SourceDisksNames]
1=%DiskId1%,,,

[SourceDisksFiles]
nuviocir_xp_x64.sys=1,,

[Manufacturer]
%PROVIDER_NAME%=DeviceList, NTAMD64

[DeviceList.NTAMD64]
%DESCRIPTION%=DriverInstall, *NTN0530

[DriverInstall]
CopyFiles=DriverCopyFiles

[DriverInstall.HW]
AddReg=DriverInstall.AddReg

;=====below information is used by driver=====
[DriverInstall.AddReg]                            
HKR,,"VendorID",0x00010001,0x5CA3
HKR,,"ProductID",0x00010001,0x00A5
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\Media Center\Remote Controls","HID\VID_5CA3&PID_00A5",0x00000000,"" 
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\Media Center\Remote Controls","HID\*NTN0530&Col04",0x00000000,"" 
;=====above information is used by driver=====

[DriverCopyFiles]
nuviocir_xp_x64.sys,,,2

;==============================================================================

;-------------- Service installation
[DriverInstall.Services]
AddService=nuviocir,2,DriverService

; -------------- nuvcir driver install sections
[DriverService]
DisplayName=%SERVICE_DISPLAY_NAME%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\nuviocir_xp_x64.sys

[Strings]
PROVIDER_NAME="Nuvoton Technology Corp."
DESCRIPTION="Nuvoton W836x7HG CIR Device Driver"
DiskId1="Nuvoton W836x7HG CIR driver installation disk #1"
SERVICE_DISPLAY_NAME="Nuvoton W836x7HG CIR Device Driver"
