; Windows Modem Setup File
; Copyright 1994-1997 Microsoft Corp.
; serial wave driver INF for voice modems
; ---------------------------------------------------------------
; includes update for MS Windows98 and WindowsNT 5.0 Beta 2 voice
; ---------------------------------------------------------------

[Version]
; created on 11/18/1998 by Manfred Recla <support@zyxel.co.at>
; for ZyXEL Comet 3356 Modem(K.56)+Fax+Voice, v1.009-K56_DSL
; using the Rockwell chipset: 'RCVDL56ACF/SVD' (chip code: R6762-27)
; with enhanced voice support for Windows98 and WindowsNT 5.0 Beta 2
; based on MS-MDK v1.47 (MDK147.DOC & REG147.DOC, October 1998)

Signature="$CHICAGO$"
Class=MEDIA
provider=%Mfg%

[Manufacturer]
%Mfg%=ZyXEL

[Strings]
Mfg                  = "ZyXEL Communications Corp."
ZC56K.DeviceDesc     = "ZyXEL Comet 3356 Modem (K.56) Serial Wave Device"

[ZyXEL]
%ZC56K.DeviceDesc%=ZC56K, MODEMWAVE\ZyXEL_Comet_3356_Modem(K.56)+Fax+Voice
%ZC56K.DeviceDesc%=ZC56K, MODEMWAVE\ZyXEL_Comet_3356_Modem(K.56)+Fax+Voice,_Plug&Play

; --------------- begin Windows98 (Memphis) & NT 5.0 voice -------------------
; this section adds Memphis support...provides ID string link to
; modem INF key named WaveHardwareID elsewhere in the corresponding modem INF
; Also see additional Memphis entries elsewhere in this INF
%ZC56K.DeviceDesc%=ZC56K.Mem, MODEMWAVE\ZyXEL_Comet_3356_(K.56)_VoiceModemWave
; --------------- end Windows98 (Memphis) & NT 5.0 voice ---------------------

[ClassInstall]
Addreg=Class.AddReg

[Class.AddReg]
HKR,,,,%MediaClassName%
HKR,,Icon,,"-1"
HKR,,Installer,,mmci.dll

[PreCopySection]
HKR,,NoSetupUI,,1

[ZC56K]
AddReg=MSSERWAVE.AddReg, ZC56K.AddReg

[ZC56K.AddReg]
HKR,Drivers\wave\serwvdrv.drv,Description,,%ZC56K.DeviceDesc%
HKR,Config,XformModule,  , "umdmxfrm.dll"
HKR,Config,XformID,      1, 01,00,00,00
HKR,Config,Baudrate,     1, 00,c2,01,00
HKR,Config,WaveDevices,  1, 02,00

; --------------- begin Windows98 (Memphis) & NT 5.0 voice --------------------------------------------------------
[ZC56K.Mem]
AddReg=MSSERWAVE.AddReg, ZC56K.Mem.AddReg

[ZC56K.Mem.AddReg]
HKR,Drivers\wave\serwvdrv.drv,Description,,%ZC56K.DeviceDesc%
; --------------- end Windows98 (Memphis) & NT 5.0 voice --------------------------------------------------------


[MSSERWAVE.AddReg]	; this section should never change
HKR,,DevLoader,,mmdevldr.vxd
HKR,Drivers,MIGRATED,,0
HKR,Drivers\wave,,,
HKR,,Driver,,serwave.vxd
HKR,Drivers\wave\serwvdrv.drv,Driver,,serwvdrv.drv
HKR,Drivers,SubClasses,,"wave"

