; Copyright 2005, Philips Semiconductors GmbH

[Version]
signature="$CHICAGO$" ;all windows os
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%ASUSTeK%
DriverVer=02/14/2006,13.3.1.4
CatalogFile=34AVStrm.cat

[Manufacturer]
%ASUSTeK%=ASUSTeK

[ASUSTeK]
;%30Hybrid.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7130
;%34Hybrid.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7134
;******** the following Id is the same for 7133 and 7135
;%33Hybrid.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133
;******** Subvendors
%30Hybrid.DeviceDesc8%=3xHybrid,PCI\VEN_1131&DEV_7130&SUBSYS_48471043
%33Hybrid.DeviceDesc8%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48471043
%34Hybrid.DeviceDesc8%=3xHybrid,PCI\VEN_1131&DEV_7134&SUBSYS_48471043

%30Hybrid.DeviceDesc6%=3xHybrid,PCI\VEN_1131&DEV_7130&SUBSYS_484E1043
%33Hybrid.DeviceDesc6%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_484E1043
%34Hybrid.DeviceDesc6%=3xHybrid,PCI\VEN_1131&DEV_7134&SUBSYS_484E1043

%30Hybrid.DeviceDesc8%=3xHybrid,PCI\VEN_1131&DEV_7130&SUBSYS_484F1043
%33Hybrid.DeviceDesc8%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_484F1043
%34Hybrid.DeviceDesc8%=3xHybrid,PCI\VEN_1131&DEV_7134&SUBSYS_484F1043

%30Hybrid.DeviceDesc6%=3xHybrid,PCI\VEN_1131&DEV_7130&SUBSYS_48501043
%33Hybrid.DeviceDesc6%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48501043
%34Hybrid.DeviceDesc6%=3xHybrid,PCI\VEN_1131&DEV_7134&SUBSYS_48501043

%33Silicon.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48451043
%33Can.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48431043
%34Can.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7134&SUBSYS_48421043

%34HybridFM.DeviceDesc8%=3xHybrid,PCI\VEN_1131&DEV_7134&SUBSYS_48531043

%33SiliconTiger.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48571043
%33HybridXceive.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48581043

%33AsusMercur.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48591043

%33DVBTTiger.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48611043
%33AsusTiger.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48621043

%33NtscMercur.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48631043
%33PalMercur.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48641043

%34LeadFreeEuropa2.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7134&SUBSYS_48731043
%33LeadFreeMercur.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48741043

%HPTigerSATX.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48751043
%ASUSTigerS.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48761043
%NECTigerS.DeviceDesc%=3xHybrid,PCI\VEN_1131&DEV_7133&SUBSYS_48771043

[DestinationDirs]
3xHybrid.CopyCoInst=11
3xHybrid.CopyFiles=10,system32\drivers ; be aware not to use 12 as the drivers directory,
                                       ; as driver will not work anymore in W98

[SourceDisksNames]
1 = %AVSTRM_INSTALLATION_DISK%,,

[SourceDisksFiles]
34CoInstaller.dll=1
3xHybrid.sys=1
Macrovision.dll=1
TvRatings.dll=1
[3xHybrid.CopyCoInst]
34CoInstaller.dll
Macrovision.dll
TvRatings.dll
[3xHybrid.CopyFiles]
3xHybrid.sys

;
;*** initialization and registry entries
;

[3xHybrid.CoInstallers]
CopyFiles = 3xHybrid.CopyCoInst
AddReg = 3xHybrid.CoInstaller_AddReg

[3xHybrid.ntx86.CoInstallers]
CopyFiles = 3xHybrid.CopyCoInst
AddReg = 3xHybrid.CoInstaller_AddReg

[3xHybrid.CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000,"34CoInstaller.dll, CoInstallerEntry"

[3xHybrid]
AlsoInstall=KS.Registration(ks.inf), WDMAUDIO.Registration(wdmaudio.inf), KSCAPTUR.Registration(kscaptur.inf), BDA.Installation(bda.inf)
CopyFiles=3xHybrid.CopyFiles
AddReg=3xHybrid.AddReg

[3xHybrid.ntx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT	  ; joner_md KS.Registration.NT to KS.Registration

CopyFiles=3xHybrid.CopyFiles
AddReg=3xHybrid.AddReg
RegisterDlls= TvRatings.Register , Macrovision.Register   ;joner+  register TvRatings.dll and Macrovision.dll for bugfix HCT chkinf issue

[3xHybrid.Services]
AddService=3xHybrid, 0x00000002, 3xHybrid.ServiceInstall

[3xHybrid.ntx86.Services]
AddService=3xHybrid, 0x00000002, 3xHybrid.ServiceInstall

[3xHybrid.ServiceInstall]
DisplayName=%DISPLAY_NAME%
Description=%SERVICE_DESCRIPTION%
ServiceType=%SERVICE_KERNEL_DRIVER%
StartType=%SERVICE_DEMAND_START%
ErrorControl=%SERVICE_ERROR_IGNORE%
ServiceBinary=%12%\3xHybrid.sys
; [StartName=driver-object-name]
; [AddReg=add-registry-section[, add-registry-section] ...]
; [DelReg=del-registry-section[, del-registry-section] ...]
; [BitReg=bit-registry-section[,bit-registry-section] ...]
; [LoadOrderGroup=load-order-group-name]
; [Dependencies=depend-on-item-name[,depend-on-item-name]...]

[3xHybrid.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,3xHybrid.sys

; audio capture registry entries

HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,3xHybrid.SYS

HKR,Drivers,SubClasses,,"wave,mixer"

HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv

HKR,Drivers\wave\wdmaud.drv,Description,,"Europa audio capture device"
HKR,Drivers\mixer\wdmaud.drv,Description,,"Europa audio capture device"

; Setting FM radio of the Silicon tuner via SIF (GPIO 21 in use/ 5.5MHz)
HKR, "Audio", "FM Radio IF",0x00010001,0x729555

; under MCE, IgnoreBW=1, prevents the driver to use the DShow bandwidth property.
; -1 is used instead to let the driver decide wich bandwidth to use (EEPROM settings)
HKR, "Parameters", "IgnoreBW",0x00010001,0x00

; under MCE, IgnoreDVBParameter=1, prevents the driver to use the DShow DVB properties.
; -1 is used instead
HKR, "Parameters", "IgnoreDVBParameter",0x00010001,0x01

; under MCE, IgnoreDVBParameter=1, prevents the driver to use the DShow DVB properties.
; -1 is used instead
HKR, "Parameters", "AsusSwitchIgnoreDVBT",0x00010001,0x0

; joner+ for My Cinema P7131D displays frame distortion and audio glitch when channels are changed issue
HKR, "Parameters", "TDA8275A_BlankVideo",0x00010001,0x01

; under HomeTheater, bugfix Audio/Video out of sync. issue
HKR, "Audio", "Pll_Xtal32_ACNI_32KHz", 0x00010001, 0x187D96

; for HP closed-caption issue and MCE   flickering and jumping issue, 12/15/2005
HKR, "Parameters", "AsusSwitch", 0x00010001, 1


; Enable MCE
;HKR, "Parameters", "MCE",0x00010001,0x01

; under Europa2, SmallXBar=0, for setting the number of input to 10, just support  (Tuner, Composite1, S-Video1, composite2, S-Video2) input sources.
; SmallXBar=1 for setting the number of input to 6, support (Tuner, Composite1, S-Video1) input sources.  ; joner_add+
HKR, "Parameters", "SmallXBar",0x00010001,0x01

;;joner+ for disable Preview_Pin
HKR, "Parameters", "CapPreviewEnabled",0x00010001,0

; this key improves the "Neighbour Channel Suppression" on the FMD1216 tuner
HKR, "Parameters", "ImproveNCS",0x00010001,0x01

;;joner+ for switch Macrovision detected
HKR, "Parameters", "IfMacrovision",0x00010001,0

;;joner+ for Samsung Disable audio capture filter
HKR, "Parameters", "IfDisableAudioFilter",0x00010001,0

;HKR, "Parameters", "TDA8275A_LNA_LVL_TV",0x00010001,0x2b
;ASUS Value 58=0x3a;   48 = 0x30;
HKR, "Parameters", "TDA8275A_LNA_LVL_TV",0x00010001,0x3a

;joner+ ASUS added Value 82 = 0x52;
HKR, "Parameters", "TDA8275A_LNA_LVLLow_TV",0x00010001,0x52

;joner+ ASUS added Value 1000
HKR, "Parameters", "TDA8275A_LNA_Monitor_TO",0x00010001,1000

;joner+ ASUS added Value 56
HKR, "Parameters", "TDA8275A_LNA_LVLHi_TV",0x00010001,56

;joner+ ASUS added Value 1
HKR, "Parameters", "TDA8275A_LNA_Monitor_Enable",0x00010001,1

;joner+ for Analog Capture Properties Video Standard detection issue, 01/25/2006
HKR, "Parameters", "IfStandardDetectSwitch",0x00010001,1

; add audio input and output pinnames

HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_MPEG_AES_PIN%,"Name",,"MPEG Audio ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_MPEG_VES_PIN%,"Name",,"MPEG Video ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_MPEG_PS_PIN%,"Name",, "MPEG2 Program"

;
;*** strings, GUIDs and names
;

;joner+  register TvRatings.dll and Macrovision.dll for bugfix HCT chkinf issue

[TvRatings.Register]
11,,TvRatings.dll,1 ;FLG_REGSVR_DLLREGISTER

[Macrovision.Register]
11,,Macrovision.dll,1 ;FLG_REGSVR_DLLREGISTER

;joner-  register TvRatings.dll and Macrovision.dll for bugfix HCT chkinf issue

[Strings]

; Proxy GUIDs

KSProxy.CLSID   = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSXBar.CLSID    = "{71F96460-78F3-11d0-A18C-00A0C9118956}"
KSTVAudio.CLSID = "{71F96462-78F3-11d0-A18C-00A0C9118956}"
KSTvTune.CLSID  = "{266EEE40-6C63-11cf-8A03-00AA006ECB65}"

; Category GUIDs

KSCATEGORY_CAPTURE                = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO                  = "{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_AUDIO                  = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}"

; Our Pin Name GUIDs

VAMP_ANLG_AUDIO_IN_PIN   = "{7BB284B9-714D-493d-A101-B1B028E782BD}"
VAMP_ANLG_AUDIO_OUT_PIN  = "{5582E657-E596-42b5-9DB3-541B27A2355F}"
VAMP_ANLG_AUDIO_I2S_PIN  = "{C2E46358-F032-4d88-B802-06B59D162730}"
VAMP_ANLG_VIDEO_ITU_PIN  = "{82631A2E-403C-4581-A4B0-EC173D004410}"

VAMP_MPEG_AES_PIN        = "{9DEC84B9-BCEF-4aac-997E-43EDD0A2D6C7}"
VAMP_MPEG_VES_PIN        = "{181CF87E-7741-47ba-8629-22347E03C64C}"
VAMP_MPEG_PS_PIN         = "{DDA87B83-65DB-4aec-82D0-79FBE67D2BB6}"

; Our Filter GUIDs

VAMP_ANLG_AUDIO_FILTER   = "{F3B951E7-8619-4ff3-91CA-03910E4BB900}"
VAMP_ANLG_CAP_FILTER     = "{BBEFB6C7-2FC4-4139-BB8B-A58BBA724000}"

; system defines

SERVICE_BOOT_START     = 0x0
SERVICE_SYSTEM_START   = 0x1
SERVICE_AUTO_START     = 0x2
SERVICE_DEMAND_START   = 0x3
SERVICE_DISABLED       = 0x4

SERVICE_KERNEL_DRIVER  = 0x1
SERVICE_ERROR_IGNORE   = 0x0
SERVICE_ERROR_NORMAL   = 0x1
SERVICE_ERROR_SEVERE   = 0x2
SERVICE_ERROR_CRITICAL = 0x3

FLG_REGSVR_DLLREGISTER = 0x00000001

;Our strings

ASUSTeK="ASUSTeK"
30Hybrid.DeviceDesc8      = "ASUSTeK SAA7130, Hybrid Capture Device"
34Hybrid.DeviceDesc8      = "ASUSTeK SAA7134, Hybrid Capture Device"
33Hybrid.DeviceDesc8      = "ASUSTeK SAA7133/35, Hybrid Capture Device"
30Hybrid.DeviceDesc6      = "ASUSTeK SAA7130, Hybrid Capture Device DVBT 6MHz"
34Hybrid.DeviceDesc6      = "ASUSTeK SAA7134, Hybrid Capture Device DVBT 6MHz"
33Hybrid.DeviceDesc6      = "ASUSTeK SAA7133/35, Hybrid Capture Device DVBT 6MHz"
33Silicon.DeviceDesc	  = "ASUSTeK Silicon BDA Video Capture"
33Can.DeviceDesc	  = "ASUSTeK SAA7133, Can BDA Video Capture"
34Can.DeviceDesc	  = "ASUSTeK SAA7134, Can BDA Video Capture"
34HybridFM.DeviceDesc8    = "ASUSTeK SAA7134, Hybrid + FM Capture Device"
33SiliconTiger.DeviceDesc    = "ASUSTeK Tiger Capture Device"
33DVBTTiger.DeviceDesc    = "ASUSTeK Tiger DVBT Capture Device"
33AsusTiger.DeviceDesc    = "ASUSTeK Tiger Hybrid Capture Device"

33HybridXceive.DeviceDesc    = "ASUSTeK Xceive Capture Device"
33AsusMercur.DeviceDesc    = "ASUSTeK Mercur Capture Device"
33NtscMercur.DeviceDesc    = "ASUSTeK NTSC Mercur Capture Device"
33PalMercur.DeviceDesc    = "ASUSTeK PAL Mercur Capture Device"

34LeadFreeEuropa2.DeviceDesc    = "ASUSTeK LeadFree Europa2 Hybrid Capture Device"
33LeadFreeMercur.DeviceDesc    = "ASUSTeK LeadFree Mercur Capture Device"

HPTigerSATX.DeviceDesc    = "ASUSTeK Tiger-S (ATX) Hybrid Capture Device"
ASUSTigerS.DeviceDesc    = "ASUSTeK Tiger-S Hybrid Capture Device"

NECTigerS.DeviceDesc    = "NECTiger-S Hybrid Capture Device"

AVSTRM_INSTALLATION_DISK = "3xHybrid installation disk"
DISPLAY_NAME             = "3xHybrid service"
SERVICE_DESCRIPTION      = "The Europa capture driver"