
[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Leadtek"
DriverVer=09/19/2006,4.0.112.3223
CatalogFile.ntx86=wfcxtcap.cat

[Manufacturer]
"Leadtek"=Leadtek

[SourceDisksNames]
1="WinFast TV (CX2388x) Drivers",,,""

[SourceDisksFiles]
wfcxtcap.sys=1

[Leadtek]
%LR6652.DeviceDesc%    = LR6652,    PCI\VEN_14F1&DEV_8802&SUBSYS_6F2B107D
%LR6652.DeviceDesc%    = LR6652,    PCI\VEN_14F1&DEV_8802&SUBSYS_665E107D
%LR6650.DeviceDesc%    = LR6650,    PCI\VEN_14F1&DEV_8802&SUBSYS_665F107D
%LR6650OEM.DeviceDesc% = LR6650OEM, PCI\VEN_14F1&DEV_8802&SUBSYS_665A107D
%LR6650OEM.DeviceDesc% = LR6650OEM, PCI\VEN_14F1&DEV_8802&SUBSYS_018714F1

[LR6650OEM]
Include=    ks.inf, kscaptur.inf, bda.inf
Needs=      KS.Registration
AddReg=     WFCXTCAP.AddReg,ThomsonDVBT.AddReg
CopyFiles=  WFCXTCAP.CopyDrivers

[LR6650]
Include=    ks.inf, kscaptur.inf, bda.inf
Needs=      KS.Registration
AddReg=     WFCXTCAP.AddReg,ThomsonDVBT.AddReg
CopyFiles=  WFCXTCAP.CopyDrivers

[LR6652]
Include=    ks.inf, kscaptur.inf, bda.inf
Needs=      KS.Registration
AddReg=     WFCXTCAP.AddReg,PhilipsPALDVBT.AddReg
CopyFiles=  WFCXTCAP.CopyDrivers

[DestinationDirs]
WFCXTCAP.CopyDrivers=10,system32\drivers

[WFCXTCAP.CopyDrivers]
wfcxtcap.sys

[WFCXTCAP.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,wfcxtcap.sys
HKR,,OkToHibernate,3,01
; Disable driver page out
HKR,,PageOutWhenUnopened,3,0
;HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKLM,System\CurrentControlSet\Control\MediaCategories\%TSPinID%,Display,1, 00,00,00,00
HKLM,System\CurrentControlSet\Control\MediaCategories\%TSPinID%,Name,,%TSPinName%

[ThomsonDVBT.AddReg]
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

[PhilipsPALDVBT.AddReg]
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

[LR6650OEM.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%KsNameFilter%,LR6650OEM_Interface,

[LR6650.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%KsNameFilter%,LR6650_Interface,

[LR6652.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%KsNameFilter%,LR6652_Interface,

[LR6650OEM_Interface]
AddReg=LR6650OEM_Interface.AddReg

[LR6650OEM_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%LR6650OEM.FriendlyName%

[LR6650_Interface]
AddReg=LR6650_Interface.AddReg

[LR6650_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%LR6650.FriendlyName%

[LR6652_Interface]
AddReg=LR6652_Interface.AddReg

[LR6652_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%LR6652.FriendlyName%

[LR6650OEM.Services]
AddService = wfcxtcap,2,wfcxtcap.ServiceInstall

[LR6650.Services]
AddService = wfcxtcap,2,wfcxtcap.ServiceInstall

[LR6652.Services]
AddService = wfcxtcap,2,wfcxtcap.ServiceInstall

[wfcxtcap.ServiceInstall]
DisplayName   = %tscap.ServiceDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\wfcxtcap.sys

[Strings]
KsNameFilter        =   "{5ea9c066-1dfe-41c5-a2de-bf766e83c98e}"

Proxy.CLSID         =   "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"

TSPinID             =   "{5237C937-0A21-4f7e-B338-DE0D0793D03F}"
TSPinName           =   "TS Out"

;; Service Name
tscap.ServiceDesc      = "WinFast DTV BDA Transport Stream Capture Driver"

;; Device Name
LR6652.DeviceDesc      = "WinFast DTV2000 H BDA Transport Stream Capture"
LR6650.DeviceDesc      = "WinFast DTV1000 T BDA Transport Stream Capture"
LR6650OEM.DeviceDesc   = "LR6650 BDA Transport Stream Capture"

;; Friendly Name
LR6652.FriendlyName    = "WinFast DTV2000 H BDA Transport Stream Capture"
LR6650.FriendlyName    = "WinFast DTV1000 T BDA Transport Stream Capture"
LR6650OEM.FriendlyName = "WinFast LR6650 BDA Transport Stream Capture"

